[    0.000000] Linux version 4.11.0-rc3-W4+ (erhoof@erhoof_tabletpc) (gcc version 6.3.1 20170306 (GCC) ) #7 SMP PREEMPT Wed Mar 22 23:22:51 MSK 2017
[    0.000000] Command line: BOOT_IMAGE=/vmlinuz-linux-test root=/dev/mmcblk1p2 rw i915.fastboot=1 debug=0x14
[    0.000000] x86/fpu: x87 FPU will use FXSAVE
[    0.000000] e820: BIOS-provided physical RAM map:
[    0.000000] BIOS-e820: [mem 0x0000000000000000-0x000000000008efff] usable
[    0.000000] BIOS-e820: [mem 0x000000000008f000-0x000000000008ffff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000000090000-0x000000000009dfff] usable
[    0.000000] BIOS-e820: [mem 0x000000000009e000-0x000000000009ffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000100000-0x000000001fffffff] usable
[    0.000000] BIOS-e820: [mem 0x0000000020000000-0x00000000200fffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000020100000-0x00000000782bafff] usable
[    0.000000] BIOS-e820: [mem 0x00000000782bb000-0x00000000784bafff] type 20
[    0.000000] BIOS-e820: [mem 0x00000000784bb000-0x0000000078bbafff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000078bbb000-0x0000000078cbafff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000078cbb000-0x0000000078cfafff] ACPI data
[    0.000000] BIOS-e820: [mem 0x0000000078cfb000-0x000000007951bfff] usable
[    0.000000] BIOS-e820: [mem 0x000000007951c000-0x000000007951cfff] reserved
[    0.000000] BIOS-e820: [mem 0x000000007951d000-0x0000000079526fff] usable
[    0.000000] BIOS-e820: [mem 0x0000000079527000-0x0000000079e26fff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000079e27000-0x0000000079ffffff] usable
[    0.000000] BIOS-e820: [mem 0x00000000e00f8000-0x00000000e00f8fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed01000-0x00000000fed01fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000ffd00000-0x00000000ffffffff] reserved
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] efi: EFI v2.31 by INSYDE Corp.
[    0.000000] efi:  ACPI 2.0=0x78cfa014  ESRT=0x78559e10  SMBIOS=0x78bba000 
[    0.000000] SMBIOS 2.7 present.
[    0.000000] DMI: Acer TP-W4-820-Z3742G06AII/Cheetah3, BIOS V1.16 03/13/2014
[    0.000000] e820: update [mem 0x00000000-0x00000fff] usable ==> reserved
[    0.000000] e820: remove [mem 0x000a0000-0x000fffff] usable
[    0.000000] e820: last_pfn = 0x7a000 max_arch_pfn = 0x400000000
[    0.000000] MTRR default type: uncachable
[    0.000000] MTRR fixed ranges enabled:
[    0.000000]   00000-9FFFF write-back
[    0.000000]   A0000-FFFFF write-protect
[    0.000000] MTRR variable ranges enabled:
[    0.000000]   0 base 0FFD00000 mask FFFC00000 write-protect
[    0.000000]   1 base 000000000 mask FC0000000 write-back
[    0.000000]   2 base 040000000 mask FE0000000 write-back
[    0.000000]   3 base 060000000 mask FF0000000 write-back
[    0.000000]   4 base 070000000 mask FF8000000 write-back
[    0.000000]   5 base 078000000 mask FFC000000 write-back
[    0.000000]   6 base 07B000000 mask FFF000000 uncachable
[    0.000000]   7 base 07AE00000 mask FFFE00000 uncachable
[    0.000000] x86/PAT: Configuration [0-7]: WB  WC  UC- UC  WB  WC  UC- WT  
[    0.000000] esrt: Reserving ESRT space from 0x0000000078559e10 to 0x0000000078559e48.
[    0.000000] Scanning 1 areas for low memory corruption
[    0.000000] Base memory trampoline at [ffff880000097000] 97000 size 24576
[    0.000000] BRK [0x02d43000, 0x02d43fff] PGTABLE
[    0.000000] BRK [0x02d44000, 0x02d44fff] PGTABLE
[    0.000000] BRK [0x02d45000, 0x02d45fff] PGTABLE
[    0.000000] BRK [0x02d46000, 0x02d46fff] PGTABLE
[    0.000000] BRK [0x02d47000, 0x02d47fff] PGTABLE
[    0.000000] BRK [0x02d48000, 0x02d48fff] PGTABLE
[    0.000000] Secure boot could not be determined
[    0.000000] RAMDISK: [mem 0x372c1000-0x37957fff]
[    0.000000] ACPI: Early table checksum verification disabled
[    0.000000] ACPI: RSDP 0x0000000078CFA014 000024 (v02 ACRSYS)
[    0.000000] ACPI: XSDT 0x0000000078CD4188 0000DC (v01 ACRSYS ACRPRDCT 00000003      01000013)
[    0.000000] ACPI: FACP 0x0000000078CF0000 00010C (v05 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: DSDT 0x0000000078CE0000 00B10F (v02 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: UEFI 0x0000000078CF9000 000236 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: TCPA 0x0000000078CF8000 000032 (v02 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: MSDM 0x0000000078CF7000 000055 (v03 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: UEFI 0x0000000078CF6000 000042 (v01 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CF2000 00305D (v01 ACRSYS ACRPRDCT 00001000 1025 00040000)
[    0.000000] ACPI: DBG2 0x0000000078CF1000 000072 (v00 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: HPET 0x0000000078CEF000 000038 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: LPIT 0x0000000078CEE000 000104 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: APIC 0x0000000078CED000 00006C (v03 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: MCFG 0x0000000078CEC000 00003C (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDF000 0005F9 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDD000 001C9F (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDC000 000058 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDB000 0000FF (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDA000 00043A (v01 ACRSYS ACRPRDCT 00001000 1025 00040000)
[    0.000000] ACPI: TPM2 0x0000000078CD9000 000034 (v03 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD8000 000763 (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD7000 000290 (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD6000 00017A (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: FPDT 0x0000000078CD5000 000044 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: CSRT 0x0000000078CD3000 00014C (v00 ACRSYS ACRPRDCT 00000005 1025 00040000)
[    0.000000] ACPI: BGRT 0x0000000078CD2000 000038 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] No NUMA configuration found
[    0.000000] Faking a node at [mem 0x0000000000000000-0x0000000079ffffff]
[    0.000000] NODE_DATA(0) allocated [mem 0x77fe7000-0x77febfff]
[    0.000000] Zone ranges:
[    0.000000]   DMA      [mem 0x0000000000001000-0x0000000000ffffff]
[    0.000000]   DMA32    [mem 0x0000000001000000-0x0000000079ffffff]
[    0.000000]   Normal   empty
[    0.000000]   Device   empty
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000000001000-0x000000000008efff]
[    0.000000]   node   0: [mem 0x0000000000090000-0x000000000009dfff]
[    0.000000]   node   0: [mem 0x0000000000100000-0x000000001fffffff]
[    0.000000]   node   0: [mem 0x0000000020100000-0x00000000782bafff]
[    0.000000]   node   0: [mem 0x0000000078cfb000-0x000000007951bfff]
[    0.000000]   node   0: [mem 0x000000007951d000-0x0000000079526fff]
[    0.000000]   node   0: [mem 0x0000000079e27000-0x0000000079ffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000000001000-0x0000000079ffffff]
[    0.000000] On node 0 totalpages: 494427
[    0.000000]   DMA zone: 64 pages used for memmap
[    0.000000]   DMA zone: 23 pages reserved
[    0.000000]   DMA zone: 3996 pages, LIFO batch:0
[    0.000000]   DMA32 zone: 7744 pages used for memmap
[    0.000000]   DMA32 zone: 490431 pages, LIFO batch:31
[    0.000000] x86/hpet: Will disable the HPET for this platform because it's not reliable
[    0.000000] Reserving Intel graphics memory at 0x000000007af00000-0x000000007eefffff
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] IOAPIC[0]: apic_id 2, version 32, address 0xfec00000, GSI 0-86
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.000000] Using ACPI (MADT) for SMP configuration information
[    0.000000] ACPI: HPET id: 0x8086a201 base: 0xfed00000
[    0.000000] smpboot: Allowing 4 CPUs, 0 hotplug CPUs
[    0.000000] PM: Registered nosave memory: [mem 0x00000000-0x00000fff]
[    0.000000] PM: Registered nosave memory: [mem 0x0008f000-0x0008ffff]
[    0.000000] PM: Registered nosave memory: [mem 0x0009e000-0x0009ffff]
[    0.000000] PM: Registered nosave memory: [mem 0x000a0000-0x000fffff]
[    0.000000] PM: Registered nosave memory: [mem 0x20000000-0x200fffff]
[    0.000000] PM: Registered nosave memory: [mem 0x782bb000-0x784bafff]
[    0.000000] PM: Registered nosave memory: [mem 0x784bb000-0x78bbafff]
[    0.000000] PM: Registered nosave memory: [mem 0x78bbb000-0x78cbafff]
[    0.000000] PM: Registered nosave memory: [mem 0x78cbb000-0x78cfafff]
[    0.000000] PM: Registered nosave memory: [mem 0x7951c000-0x7951cfff]
[    0.000000] PM: Registered nosave memory: [mem 0x79527000-0x79e26fff]
[    0.000000] e820: [mem 0x7ef00000-0xe00f7fff] available for PCI devices
[    0.000000] Booting paravirtualized kernel on bare hardware
[    0.000000] clocksource: refined-jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 6370452778343963 ns
[    0.000000] setup_percpu: NR_CPUS:128 nr_cpumask_bits:128 nr_cpu_ids:4 nr_node_ids:1
[    0.000000] percpu: Embedded 37 pages/cpu @ffff880076a00000 s111448 r8192 d31912 u524288
[    0.000000] pcpu-alloc: s111448 r8192 d31912 u524288 alloc=1*2097152
[    0.000000] pcpu-alloc: [0] 0 1 2 3 
[    0.000000] Built 1 zonelists in Node order, mobility grouping on.  Total pages: 486596
[    0.000000] Policy zone: DMA32
[    0.000000] Kernel command line: BOOT_IMAGE=/vmlinuz-linux-test root=/dev/mmcblk1p2 rw i915.fastboot=1 debug=0x14
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Calgary: detecting Calgary via BIOS EBDA area
[    0.000000] Calgary: Unable to locate Rio Grande table in EBDA - bailing!
[    0.000000] Memory: 1894044K/1977708K available (6432K kernel code, 1089K rwdata, 2000K rodata, 1308K init, 904K bss, 83664K reserved, 0K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000] 	Build-time adjustment of leaf fanout to 64.
[    0.000000] 	RCU restricting CPUs from NR_CPUS=128 to nr_cpu_ids=4.
[    0.000000] RCU: Adjusting geometry for rcu_fanout_leaf=64, nr_cpu_ids=4
[    0.000000] NR_IRQS:8448 nr_irqs:1024 0
[    0.000000] Console: colour dummy device 80x25
[    0.000000] console [tty0] enabled
[    0.000000] tsc: Detected 1333.000 MHz processor
[    0.000021] Calibrating delay loop (skipped), value calculated using timer frequency.. 2667.08 BogoMIPS (lpj=4443333)
[    0.000048] pid_max: default: 32768 minimum: 301
[    0.000092] ACPI: Core revision 20170119
[    0.003333] ACPI: 10 ACPI AML tables successfully acquired and loaded
[    0.003333] Security Framework initialized
[    0.003333] Yama: becoming mindful.
[    0.003333] Dentry cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.003333] Inode-cache hash table entries: 131072 (order: 8, 1048576 bytes)
[    0.003333] Mount-cache hash table entries: 4096 (order: 3, 32768 bytes)
[    0.003333] Mountpoint-cache hash table entries: 4096 (order: 3, 32768 bytes)
[    0.003333] CPU: Physical Processor ID: 0
[    0.003333] CPU: Processor Core ID: 0
[    0.003333] ENERGY_PERF_BIAS: Set to 'normal', was 'performance'
[    0.003333] ENERGY_PERF_BIAS: View and update with x86_energy_perf_policy(8)
[    0.003333] mce: CPU supports 6 MCE banks
[    0.003333] CPU0: Thermal monitoring enabled (TM1)
[    0.003333] process: using mwait in idle threads
[    0.003333] Last level iTLB entries: 4KB 48, 2MB 0, 4MB 0
[    0.003333] Last level dTLB entries: 4KB 128, 2MB 16, 4MB 16, 1GB 0
[    0.003333] Freeing SMP alternatives memory: 24K
[    0.003333] ftrace: allocating 25362 entries in 100 pages
[    0.003333] smpboot: Max logical packages: 1
[    0.003333] TSC deadline timer enabled
[    0.003333] smpboot: CPU0: Intel(R) Atom(TM) CPU  Z3740  @ 1.33GHz (family: 0x6, model: 0x37, stepping: 0x3)
[    0.010013] Performance Events: PEBS fmt2+, 8-deep LBR, Silvermont events, 8-deep LBR, full-width counters, Intel PMU driver.
[    0.010061] ... version:                3
[    0.010073] ... bit width:              40
[    0.010084] ... generic registers:      2
[    0.010095] ... value mask:             000000ffffffffff
[    0.010107] ... max period:             0000007fffffffff
[    0.010119] ... fixed-purpose events:   3
[    0.010129] ... event mask:             0000000700000003
[    0.033631] NMI watchdog: enabled on all CPUs, permanently consumes one hw-PMU counter.
[    0.040011] smp: Bringing up secondary CPUs ...
[    0.066711] x86: Booting SMP configuration:
[    0.066727] .... node  #0, CPUs:      #1 #2 #3
[    0.370153] smp: Brought up 1 node, 4 CPUs
[    0.370153] smpboot: Total of 4 processors activated (10677.44 BogoMIPS)
[    0.370872] sched_clock: Marking stable (369999963, 0)->(436505177, -66505214)
[    0.371601] devtmpfs: initialized
[    0.371758] x86/mm: Memory block size: 128MB
[    0.381625] PM: Registering ACPI NVS region [mem 0x0008f000-0x0008ffff] (4096 bytes)
[    0.381647] PM: Registering ACPI NVS region [mem 0x78bbb000-0x78cbafff] (1048576 bytes)
[    0.381712] PM: Registering ACPI NVS region [mem 0x79527000-0x79e26fff] (9437184 bytes)
[    0.382256] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 6370867519511994 ns
[    0.382298] futex hash table entries: 1024 (order: 4, 65536 bytes)
[    0.382464] pinctrl core: initialized pinctrl subsystem
[    0.382552] RTC time: 17:42:30, date: 03/23/17
[    0.382848] NET: Registered protocol family 16
[    0.386494] cpuidle: using governor ladder
[    0.386616] cpuidle: using governor menu
[    0.386636] PCCT header not found.
[    0.386717] ACPI: bus type PCI registered
[    0.386732] acpiphp: ACPI Hot Plug PCI Controller Driver version: 0.5
[    0.386908] PCI: MMCONFIG for domain 0000 [bus 00-3f] at [mem 0xe0000000-0xe3ffffff] (base 0xe0000000)
[    0.386964] PCI: not using MMCONFIG
[    0.386982] PCI: Using configuration type 1 for base access
[    0.389388] HugeTLB registered 2 MB page size, pre-allocated 0 pages
[    0.390129] ACPI: Added _OSI(Module Device)
[    0.390146] ACPI: Added _OSI(Processor Device)
[    0.390158] ACPI: Added _OSI(3.0 _SCP Extensions)
[    0.390170] ACPI: Added _OSI(Processor Aggregator Device)
[    0.410872] ACPI: Dynamic OEM Table Load:
[    0.410909] ACPI: SSDT 0xFFFF880073F66400 000353 (v01 PmRef  Cpu0Ist  00003000 INTL 20121114)
[    0.411560] ACPI: Dynamic OEM Table Load:
[    0.411591] ACPI: SSDT 0xFFFF880073F23800 000433 (v01 PmRef  Cpu0Cst  00003001 INTL 20121114)
[    0.412919] ACPI: Dynamic OEM Table Load:
[    0.412949] ACPI: SSDT 0xFFFF880073F61400 00015F (v01 PmRef  ApIst    00003000 INTL 20121114)
[    0.413540] ACPI: Dynamic OEM Table Load:
[    0.413569] ACPI: SSDT 0xFFFF880073FC9A80 00008D (v01 PmRef  ApCst    00003000 INTL 20121114)
[    0.417091] ACPI: Interpreter enabled
[    0.417132] ACPI: (supports S0)
[    0.417145] ACPI: Using IOAPIC for interrupt routing
[    0.417243] PCI: MMCONFIG for domain 0000 [bus 00-3f] at [mem 0xe0000000-0xe3ffffff] (base 0xe0000000)
[    0.422892] [Firmware Info]: PCI: MMCONFIG at [mem 0xe0000000-0xe3ffffff] not reserved in ACPI motherboard resources
[    0.422916] PCI: not using MMCONFIG
[    0.422934] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    0.426933] ACPI: Power Resource [USBC] (on)
[    0.427826] ACPI: Power Resource [WWPR] (off)
[    0.435322] ACPI: Power Resource [PLPE] (on)
[    0.443703] ACPI: Power Resource [CLK0] (on)
[    0.443978] ACPI: Power Resource [P28X] (off)
[    0.444109] ACPI: Power Resource [P18X] (off)
[    0.444799] ACPI: Power Resource [CLK1] (on)
[    0.446945] ACPI: Power Resource [TCPR] (off)
[    0.455920] ACPI: PCI Root Bridge [PCI0] (domain 0000 [bus 00-ff])
[    0.455948] acpi PNP0A08:00: _OSC: OS supports [ASPM ClockPM Segments MSI]
[    0.456094] acpi PNP0A08:00: _OSC failed (AE_ERROR); disabling ASPM
[    0.456139] acpi PNP0A08:00: fail to add MMCONFIG information, can't access extended PCI configuration space under this bridge.
[    0.456914] PCI host bridge to bus 0000:00
[    0.456932] pci_bus 0000:00: root bus resource [io  0x0070-0x0077]
[    0.456948] pci_bus 0000:00: root bus resource [io  0x0000-0x006f window]
[    0.456964] pci_bus 0000:00: root bus resource [io  0x0078-0x0cf7 window]
[    0.456979] pci_bus 0000:00: root bus resource [io  0x0d00-0xffff window]
[    0.456995] pci_bus 0000:00: root bus resource [mem 0x000a0000-0x000bffff window]
[    0.457015] pci_bus 0000:00: root bus resource [mem 0x000c0000-0x000dffff window]
[    0.457035] pci_bus 0000:00: root bus resource [mem 0x000e0000-0x000fffff window]
[    0.457055] pci_bus 0000:00: root bus resource [mem 0x90c00000-0x90ffffff window]
[    0.457075] pci_bus 0000:00: root bus resource [mem 0x7af00001-0x7ef00000 window]
[    0.457095] pci_bus 0000:00: root bus resource [mem 0x80000000-0x908ffffe window]
[    0.457115] pci_bus 0000:00: root bus resource [mem 0xfed40000-0xfed40fff window]
[    0.457135] pci_bus 0000:00: root bus resource [bus 00-ff]
[    0.457163] pci 0000:00:00.0: [8086:0f00] type 00 class 0x060000
[    0.457389] pci 0000:00:02.0: [8086:0f31] type 00 class 0x030000
[    0.457421] pci 0000:00:02.0: reg 0x10: [mem 0x90000000-0x903fffff]
[    0.457450] pci 0000:00:02.0: reg 0x18: [mem 0x80000000-0x8fffffff pref]
[    0.457477] pci 0000:00:02.0: reg 0x20: [io  0x1000-0x1007]
[    0.457716] pci 0000:00:14.0: [8086:0f35] type 00 class 0x0c0330
[    0.457754] pci 0000:00:14.0: reg 0x10: [mem 0x90800000-0x9080ffff 64bit]
[    0.457852] pci 0000:00:14.0: PME# supported from D3hot D3cold
[    0.458042] pci 0000:00:1a.0: [8086:0f18] type 00 class 0x108000
[    0.458081] pci 0000:00:1a.0: reg 0x10: [mem 0x90700000-0x907fffff]
[    0.458107] pci 0000:00:1a.0: reg 0x14: [mem 0x90600000-0x906fffff]
[    0.458225] pci 0000:00:1a.0: PME# supported from D0 D3hot
[    0.458410] pci 0000:00:1f.0: [8086:0f1c] type 00 class 0x060100
[    0.459685] ACPI: PCI Interrupt Link [LNKA] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.459911] ACPI: PCI Interrupt Link [LNKB] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.460152] ACPI: PCI Interrupt Link [LNKC] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.460376] ACPI: PCI Interrupt Link [LNKD] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.460600] ACPI: PCI Interrupt Link [LNKE] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.460823] ACPI: PCI Interrupt Link [LNKF] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.461049] ACPI: PCI Interrupt Link [LNKG] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.461282] ACPI: PCI Interrupt Link [LNKH] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.511221] random: fast init done
[    0.527259] dw_dmac INTL9C60:00: DesignWare DMA Controller, 8 channels
[    0.560628] dw_dmac INTL9C60:01: DesignWare DMA Controller, 8 channels
[    0.561322] pci 0000:00:02.0: vgaarb: setting as boot VGA device
[    0.561341] pci 0000:00:02.0: vgaarb: VGA device added: decodes=io+mem,owns=io+mem,locks=none
[    0.561378] pci 0000:00:02.0: vgaarb: bridge control possible
[    0.561391] vgaarb: loaded
[    0.561602] Registered efivars operations
[    0.576121] PCI: Using ACPI for IRQ routing
[    0.576144] PCI: pci_cache_line_size set to 64 bytes
[    0.576184] Expanded resource reserved due to conflict with PCI Bus 0000:00
[    0.576216] e820: reserve RAM buffer [mem 0x0008f000-0x0008ffff]
[    0.576231] e820: reserve RAM buffer [mem 0x0009e000-0x0009ffff]
[    0.576245] e820: reserve RAM buffer [mem 0x782bb000-0x7bffffff]
[    0.576260] e820: reserve RAM buffer [mem 0x7951c000-0x7bffffff]
[    0.576274] e820: reserve RAM buffer [mem 0x79527000-0x7bffffff]
[    0.576288] e820: reserve RAM buffer [mem 0x7a000000-0x7bffffff]
[    0.576600] NetLabel: Initializing
[    0.576613] NetLabel:  domain hash size = 128
[    0.576625] NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
[    0.576688] NetLabel:  unlabeled traffic allowed by default
[    0.577669] clocksource: Switched to clocksource refined-jiffies
[    0.607314] VFS: Disk quotas dquot_6.6.0
[    0.607415] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.607667] pnp: PnP ACPI init
[    0.608109] pnp 00:00: Plug and Play ACPI device, IDs PNP0b00 (active)
[    0.609087] system 00:01: [io  0x0680-0x069f] has been reserved
[    0.609105] system 00:01: [io  0x0400-0x047f] has been reserved
[    0.609121] system 00:01: [io  0x0500-0x05fe] has been reserved
[    0.609136] system 00:01: [io  0x0600-0x061f] has been reserved
[    0.609165] system 00:01: [io  0x164e-0x164f] has been reserved
[    0.609216] system 00:01: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.622331] pnp: PnP ACPI: found 2 devices
[    0.628250] pci_bus 0000:00: resource 4 [io  0x0070-0x0077]
[    0.628271] pci_bus 0000:00: resource 5 [io  0x0000-0x006f window]
[    0.628286] pci_bus 0000:00: resource 6 [io  0x0078-0x0cf7 window]
[    0.628302] pci_bus 0000:00: resource 7 [io  0x0d00-0xffff window]
[    0.628317] pci_bus 0000:00: resource 8 [mem 0x000a0000-0x000bffff window]
[    0.628333] pci_bus 0000:00: resource 9 [mem 0x000c0000-0x000dffff window]
[    0.628361] pci_bus 0000:00: resource 10 [mem 0x000e0000-0x000fffff window]
[    0.628377] pci_bus 0000:00: resource 11 [mem 0x90c00000-0x90ffffff window]
[    0.628393] pci_bus 0000:00: resource 12 [mem 0x7af00001-0x7ef00000 window]
[    0.628409] pci_bus 0000:00: resource 13 [mem 0x80000000-0x908ffffe window]
[    0.628424] pci_bus 0000:00: resource 14 [mem 0xfed40000-0xfed40fff window]
[    0.630583] NET: Registered protocol family 2
[    0.631036] TCP established hash table entries: 16384 (order: 5, 131072 bytes)
[    0.631173] TCP bind hash table entries: 16384 (order: 6, 262144 bytes)
[    0.631317] TCP: Hash tables configured (established 16384 bind 16384)
[    0.631432] UDP hash table entries: 1024 (order: 3, 32768 bytes)
[    0.631492] UDP-Lite hash table entries: 1024 (order: 3, 32768 bytes)
[    0.631646] NET: Registered protocol family 1
[    0.631709] pci 0000:00:02.0: Video device with shadowed ROM at [mem 0x000c0000-0x000dffff]
[    0.632384] PCI: CLS 0 bytes, default 64
[    0.632568] Unpacking initramfs...
[    0.882884] Freeing initrd memory: 6748K
[    0.882988] clocksource: tsc: mask: 0xffffffffffffffff max_cycles: 0x1336e3dbd1a, max_idle_ns: 440795236868 ns
[    0.883070] clocksource: Switched to clocksource tsc
[    0.884108] Scanning for low memory corruption every 60 seconds
[    0.885693] Initialise system trusted keyrings
[    0.885950] workingset: timestamp_bits=40 max_order=19 bucket_order=0
[    0.889686] zbud: loaded
[    0.892680] Key type asymmetric registered
[    0.892734] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 249)
[    0.892844] io scheduler noop registered
[    0.892859] io scheduler deadline registered
[    0.892957] io scheduler cfq registered (default)
[    0.892971] io scheduler mq-deadline registered
[    0.893414] efifb: probing for efifb
[    0.893459] efifb: framebuffer at 0x80000000, using 4032k, total 4032k
[    0.893475] efifb: mode is 800x1280x32, linelength=3200, pages=1
[    0.893487] efifb: scrolling: redraw
[    0.893499] efifb: Truecolor: size=8:8:8:8, shift=24:16:8:0
[    0.903275] Console: switching to colour frame buffer device 100x80
[    0.912817] fb0: EFI VGA frame buffer device
[    0.912912] intel_idle: MWAIT substates: 0x33000020
[    0.912992] intel_idle: v0.4.1 model 0x37
[    0.913826] intel_idle: lapic_timer_reliable_states 0xffffffff
[    0.924382] GHES: HEST is not enabled!
[    0.924832] Serial: 8250/16550 driver, 4 ports, IRQ sharing enabled
[    0.927493] hpet: number irqs doesn't agree with number of timers
[    0.927661] Linux agpgart interface v0.103
[    0.929930] ACPI Warning: Could not enable fixed event - RealTimeClock (4) (20170119/evxface-654)
[    0.930768] rtc_cmos 00:00: rtc core: registered rtc_cmos as rtc0
[    0.930907] rtc_cmos 00:00: alarms up to one day, 242 bytes nvram
[    0.931027] intel_pstate: Intel P-state driver initializing
[    0.933659] ledtrig-cpu: registered to indicate activity on CPUs
[    0.935844] NET: Registered protocol family 10
[    0.957874] Segment Routing with IPv6
[    0.957972] NET: Registered protocol family 17
[    0.960736] microcode: sig=0x30673, pf=0x2, revision=0x322
[    0.961400] microcode: Microcode Update Driver: v2.2.
[    0.962989] registered taskstats version 1
[    0.963135] Loading compiled-in X.509 certificates
[    0.963233] zswap: loaded using pool lzo/zbud
[    0.964530]   Magic number: 9:198:745
[    0.964747] rtc_cmos 00:00: setting system clock to 2017-03-23 17:42:31 UTC (1490290951)
[    0.964937] PM: Hibernation image not present or could not be loaded.
[    0.967719] Freeing unused kernel memory: 1308K
[    0.967785] Write protecting the kernel read-only data: 10240k
[    0.969263] Freeing unused kernel memory: 1744K
[    0.969628] Freeing unused kernel memory: 48K
[    1.130277] sdhci: Secure Digital Host Controller Interface driver
[    1.130358] sdhci: Copyright(c) Pierre Ossman
[    1.143672] i8042: PNP: No PS/2 controller found.
[    1.154024] ACPI: bus type USB registered
[    1.154428] usbcore: registered new interface driver usbfs
[    1.154529] usbcore: registered new interface driver hub
[    1.154657] usbcore: registered new device driver usb
[    1.176740] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.176839] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 1
[    1.178708] xhci_hcd 0000:00:14.0: hcc params 0x200077c1 hci version 0x100 quirks 0x00009810
[    1.179224] xhci_hcd 0000:00:14.0: cache line size of 64 is not supported
[    1.180201] hub 1-0:1.0: USB hub found
[    1.180287] hub 1-0:1.0: 6 ports detected
[    1.340735] mmc0: SDHCI controller on ACPI [INT33BB:00] using ADMA
[    1.360010] mmc1: SDHCI controller on ACPI [80860F14:00] using ADMA
[    1.382440] mmc2: SDHCI controller on ACPI [80860F14:01] using ADMA
[    1.484955] mmc0: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.502144] mmc2: new high speed SDXC card at address 59b4
[    1.504730] mmc1: new HS200 MMC card at address 0001
[    1.507697] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.507794] mmcblk2: mmc2:59b4 SD    58.9 GiB (ro)
[    1.509920]  mmcblk2: p1
[    1.511290] mmcblk1: mmc1:0001 MCG8GC 58.2 GiB 
[    1.518170] mmcblk1boot0: mmc1:0001 MCG8GC partition 1 4.00 MiB
[    1.525698] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.530445] mmcblk1boot1: mmc1:0001 MCG8GC partition 2 4.00 MiB
[    1.539689] mmcblk1rpmb: mmc1:0001 MCG8GC partition 3 4.00 MiB
[    1.548833]  mmcblk1: p1 p2
[    1.598007] mmc0: new ultra high speed DDR50 SDIO card at address 0001
[    1.707580] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.719082] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 2
[    1.723350] hub 2-0:1.0: USB hub found
[    1.726664] hub 2-0:1.0: 1 port detected
[    1.899184] EXT4-fs (mmcblk1p2): mounted filesystem with ordered data mode. Opts: (null)
[    2.094243] ip_tables: (C) 2000-2006 Netfilter Core Team
[    2.112099] systemd[1]: systemd 232 running in system mode. (+PAM -AUDIT -SELINUX -IMA -APPARMOR +SMACK -SYSVINIT +UTMP +LIBCRYPTSETUP +GCRYPT +GNUTLS +ACL +XZ +LZ4 +SECCOMP +BLKID +ELFUTILS +KMOD +IDN)
[    2.122788] systemd[1]: Detected architecture x86-64.
[    2.140164] systemd[1]: Set hostname to <erhoof_tabletpc>.
[    2.282591] systemd[1]: Reached target Swap.
[    2.296316] systemd[1]: Listening on Process Core Dump Socket.
[    2.303777] systemd[1]: Set up automount Arbitrary Executable File Formats File System Automount Point.
[    2.314674] systemd[1]: Listening on Journal Socket (/dev/log).
[    2.322004] systemd[1]: Listening on /dev/initctl Compatibility Named Pipe.
[    2.330255] systemd[1]: Created slice User and Session Slice.
[    2.337677] systemd[1]: Listening on udev Control Socket.
[    2.458133] EXT4-fs (mmcblk1p2): re-mounted. Opts: data=ordered,discard
[    2.837290] 80860F0A:00: ttyS0 at MMIO 0x9094d000 (irq = 186, base_baud = 2764800) is a 16550A
[    2.837415] ACPI: AC Adapter [ADP1] (on-line)
[    2.917839] Bluetooth: Core ver 2.22
[    2.922863] NET: Registered protocol family 31
[    2.926570] Bluetooth: HCI device and connection manager initialized
[    2.930287] Bluetooth: HCI socket layer initialized
[    2.930873] input: Lid Switch as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0C0D:00/input/input0
[    2.930880] ACPI: Lid Switch [LID]
[    2.942075] Bluetooth: L2CAP socket layer initialized
[    2.945830] Bluetooth: SCO socket layer initialized
[    2.969167] Bluetooth: HCI UART driver ver 2.3
[    2.973515] Bluetooth: HCI UART protocol H4 registered
[    2.977329] Bluetooth: HCI UART protocol BCSP registered
[    2.981065] Bluetooth: HCI UART protocol LL registered
[    2.984619] Bluetooth: HCI UART protocol ATH3K registered
[    2.988084] Bluetooth: HCI UART protocol Three-wire (H5) registered
[    2.991617] Bluetooth: HCI UART protocol Intel registered
[    2.995439] FUJITSU Extended Socket Network Device Driver - version 1.2 - Copyright (c) 2015 FUJITSU LIMITED
[    2.997400] wmi: Mapper loaded
[    3.004895] intel_sst_acpi 80860F28:00: BYT-CR not detected
[    3.005131] intel_sst_acpi 80860F28:00: LPE base: 0x90a00000 size:0x200000
[    3.005134] intel_sst_acpi 80860F28:00: IRAM base: 0x90ac0000
[    3.005185] intel_sst_acpi 80860F28:00: DRAM base: 0x90b00000
[    3.005192] intel_sst_acpi 80860F28:00: SHIM base: 0x90b40000
[    3.005200] intel_sst_acpi 80860F28:00: Mailbox base: 0x90b44000
[    3.005206] intel_sst_acpi 80860F28:00: DDR base: 0x20000000
[    3.008779] intel_sst_acpi 80860F28:00: Got drv data max stream 25
[    3.011883] hci_bcm BCM2E3F:00: BCM irq: 187
[    3.011959] hci_bcm BCM2E3F:00: BCM2E3F:00 device registered.
[    3.012130] Bluetooth: HCI UART protocol Broadcom registered
[    3.012132] Bluetooth: HCI UART protocol QCA registered
[    3.012134] Bluetooth: HCI UART protocol AG6XX registered
[    3.012135] Bluetooth: HCI UART protocol Marvell registered
[    3.033648] i8042: PNP: No PS/2 controller found.
[    3.041826] [drm] Memory usable by graphics device = 2048M
[    3.041831] checking generic (80000000 3f0000) vs hw (80000000 10000000)
[    3.041832] fb: switching to inteldrmfb from EFI VGA
[    3.071350] Console: switching to colour dummy device 80x25
[    3.071655] [drm] Replacing VGA console driver
[    3.072585] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[    3.072603] [drm] Driver supports precise vblank timestamp query.
[    3.073379] i915 0000:00:02.0: vgaarb: changed VGA decodes: olddecodes=io+mem,decodes=io+mem:owns=io+mem
[    3.073989] [drm:pwm_setup_backlight [i915]] *ERROR* Failed to own the pwm chip
[    3.077979] i8042: PNP: No PS/2 controller found.
[    3.079176] [Firmware Bug]: No valid trip found
[    3.090531] [drm] Initialized i915 1.6.0 20170320 for 0000:00:02.0 on minor 0
[    3.094871] ACPI: Video Device [GFX0] (multi-head: yes  rom: no  post: no)
[    3.096078] acpi device:1a: registered as cooling_device4
[    3.096237] input: Video Bus as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/LNXVIDEO:00/input/input1
[    3.096353] [drm] HDaudio controller not detected, using LPE audio instead

[    3.096610] [drm] Initialized i915 1.6.0 20170320 for 0000:00:02.0 on minor 0
[    3.108780] hidraw: raw HID events driver (C) Jiri Kosina
[    3.138798] genirq: Flags mismatch irq 8. 00002008 (SMO91D0:00) vs. 00000080 (rtc0)
[    3.138852] i2c_hid i2c-SMO91D0:00: Could not register for SMO91D0:00 interrupt, irq = 8, ret = -16
[    3.156618] i2c_hid: probe of i2c-SMO91D0:00 failed with error -16
[    3.161270] input: PC Speaker as /devices/platform/pcspkr/input/input2
[    3.171832] i915 0000:00:02.0: HDMI-A-2: EDID is invalid:
[    3.171851] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[    3.171861] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[    3.171871] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[    3.171880] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[    3.171889] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[    3.171899] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[    3.171908] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[    3.171917] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[    3.180001] fbcon: inteldrmfb (fb0) is primary device
[    3.184733] ACPI: Battery Slot [BATC] (battery present)
[    3.205318] random: crng init done
[    3.231770] SSE version of gcm_enc/dec engaged.
[    3.263787] [drm:pipe_config_err [i915]] *ERROR* mismatch in dsi_pll.div (expected 0x00000157, found 0x000001ab)
[    3.263795] ------------[ cut here ]------------
[    3.263863] WARNING: CPU: 3 PID: 50 at drivers/gpu/drm/i915/intel_display.c:12057 intel_atomic_commit_tail+0x14bb/0x1ee0 [i915]
[    3.263864] pipe state doesn't match!
[    3.263865] Modules linked in: aesni_intel(+) brcmfmac aes_x86_64 crypto_simd glue_helper cryptd brcmutil cfg80211 intel_cstate pcspkr snd_soc_rt5670 snd_soc_rt5645 i2c_hid hid battery snd_soc_rt5640 snd_soc_rl6231 mei_txe mei lpc_ich thermal i915 fjes wmi snd_intel_sst_acpi hci_uart tpm_crb snd_intel_sst_core btbcm btqca dptf_power soc_button_array btintel snd_soc_sst_atom_hifi2_platform int3406_thermal snd_soc_sst_match video snd_soc_core button bluetooth drm_kms_helper snd_compress intel_gtt syscopyarea snd_pcm_dmaengine sysfillrect sysimgblt int3402_thermal int3403_thermal int3400_thermal processor_thermal_device snd_pcm fb_sys_fops rfkill acpi_thermal_rel int340x_thermal_zone intel_soc_dts_iosf acpi_pad i2c_algo_bit snd_timer i2c_designware_platform ac i2c_designware_core snd soundcore ac97_bus
[    3.263922]  tpm_tis 8250_dw tpm_tis_core tpm spi_pxa2xx_platform sch_fq_codel ip_tables x_tables ext4 crc16 jbd2 fscrypto mbcache mmc_block xhci_pci xhci_hcd usbcore usb_common serio sdhci_acpi sdhci led_class mmc_core drm
[    3.263946] CPU: 3 PID: 50 Comm: kworker/3:1 Not tainted 4.11.0-rc3-W4+ #7
[    3.263947] Hardware name: Acer TP-W4-820-Z3742G06AII/Cheetah3, BIOS V1.16 03/13/2014
[    3.263956] Workqueue: events output_poll_execute [drm_kms_helper]
[    3.263958] Call Trace:
[    3.263969]  dump_stack+0x63/0x83
[    3.263974]  __warn+0xcb/0xf0
[    3.263978]  warn_slowpath_fmt+0x5f/0x80
[    3.264050]  ? intel_compare_link_m_n+0x6d/0xa0 [i915]
[    3.264112]  intel_atomic_commit_tail+0x14bb/0x1ee0 [i915]
[    3.264169]  ? intel_runtime_pm_put+0x56/0xc0 [i915]
[    3.264173]  ? insert_work+0x4f/0xc0
[    3.264178]  ? wake_atomic_t_function+0x60/0x60
[    3.264241]  intel_atomic_commit+0x3b7/0x4b0 [i915]
[    3.264256]  drm_atomic_commit+0x4b/0x50 [drm]
[    3.264263]  restore_fbdev_mode+0x14e/0x2a0 [drm_kms_helper]
[    3.264269]  drm_fb_helper_restore_fbdev_mode_unlocked+0x34/0x80 [drm_kms_helper]
[    3.264274]  drm_fb_helper_set_par+0x2d/0x60 [drm_kms_helper]
[    3.264279]  drm_fb_helper_hotplug_event+0xe3/0xf0 [drm_kms_helper]
[    3.264340]  intel_fbdev_output_poll_changed+0x24/0x30 [i915]
[    3.264346]  drm_kms_helper_hotplug_event+0x27/0x30 [drm_kms_helper]
[    3.264351]  output_poll_execute+0xae/0x1e0 [drm_kms_helper]
[    3.264356]  ? __schedule+0x2db/0x8a0
[    3.264360]  process_one_work+0x1e5/0x470
[    3.264363]  worker_thread+0x48/0x4e0
[    3.264367]  kthread+0x101/0x140
[    3.264370]  ? process_one_work+0x470/0x470
[    3.264372]  ? kthread_create_on_node+0x60/0x60
[    3.264375]  ret_from_fork+0x2c/0x40
[    3.264379] ---[ end trace ae3fbd454a2cb338 ]---
[    3.277748] Console: switching to colour frame buffer device 100x80
[    3.288190] i8042: PNP: No PS/2 controller found.
[    3.293481] input: gpio-keys as /devices/platform/gpio-keys.0.auto/input/input3
[    3.295050] input: gpio-keys as /devices/platform/gpio-keys.1.auto/input/input4
[    3.299164] bytcr_rt5640 bytcr_rt5640: quirk DMIC1_MAP enabled
[    3.299167] bytcr_rt5640 bytcr_rt5640: quirk DMIC enabled
[    3.299169] bytcr_rt5640 bytcr_rt5640: quirk MCLK_EN enabled
[    3.311196] bytcr_rt5640 bytcr_rt5640: snd-soc-dummy-dai <-> media-cpu-dai mapping ok
[    3.311257] bytcr_rt5640 bytcr_rt5640: snd-soc-dummy-dai <-> deepbuffer-cpu-dai mapping ok
[    3.311294] compress asoc: snd-soc-dummy-dai <-> compress-cpu-dai mapping ok
[    3.312399] bytcr_rt5640 bytcr_rt5640: rt5640-aif1 <-> ssp2-port mapping ok
[    3.317344] iTCO_vendor_support: vendor-support=0
[    3.332753] iTCO_wdt: Intel TCO WatchDog Timer Driver v1.11
[    3.332896] iTCO_wdt: Found a Bay Trail SoC TCO device (Version=3, TCOBASE=0x0460)
[    3.333192] iTCO_wdt: initialized. heartbeat=30 sec (nowayout=0)
[    3.359109] (NULL device *): hwmon_device_register() is deprecated. Please convert the driver to use hwmon_device_register_with_info().
[    3.359211] (NULL device *): hwmon_device_register() is deprecated. Please convert the driver to use hwmon_device_register_with_info().
[    3.366273] intel_rapl: Found RAPL domain package
[    3.366275] intel_rapl: Found RAPL domain core
[    3.475449] input: SYNA7300:00 06CB:0106 as /devices/platform/80860F41:05/i2c-5/i2c-SYNA7300:00/0018:06CB:0106.0001/input/input5
[    3.475928] hid-multitouch 0018:06CB:0106.0001: input,hidraw0: I2C HID v1.00 Device [SYNA7300:00 06CB:0106] on i2c-SYNA7300:00
[    3.500762] i915 0000:00:02.0: fb0: inteldrmfb frame buffer device
[    3.532952] mousedev: PS/2 mouse device common for all mice
[    3.558401] mmc0: queuing unknown CIS tuple 0x80 (7 bytes)
[    3.578607] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    3.596409] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    3.627589] systemd-journald[184]: Received request to flush runtime journal from PID 1
[    3.668107] usbcore: registered new interface driver brcmfmac
[    3.799833] FAT-fs (mmcblk1p1): Volume was not properly unmounted. Some data may be corrupt. Please run fsck.
[    3.918934] brcmfmac: brcmf_c_preinit_dcmds: Firmware version = wl0: Jul 17 2013 07:36:07 version 6.10.197.71 (r412987) FWID 01-882d2634
[    3.923977] brcmfmac: brcmf_cfg80211_reg_notifier: not a ISO3166 code (0x30 0x30)
[    4.677992] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    4.710358] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    5.237814] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    5.433425] brcmfmac: brcmf_p2p_create_p2pdev: set p2p_disc error
[    5.433444] brcmfmac: brcmf_cfg80211_add_iface: add iface p2p-dev-wlan0 type 10 failed: err=-16
[    5.451270] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    6.911399] fuse init (API version 7.26)
[    9.342399] Bluetooth: BNEP (Ethernet Emulation) ver 1.3
[    9.342408] Bluetooth: BNEP filters: protocol multicast
[    9.342422] Bluetooth: BNEP socket layer initialized
[    9.677313] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[   17.232246] IPv6: ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready