[    0.000000] Linux version 4.11.0-rc3-W4+ (erhoof@erhoof_tabletpc) (gcc version 6.3.1 20170306 (GCC) ) #7 SMP PREEMPT Wed Mar 22 23:22:51 MSK 2017
[    0.000000] Command line: BOOT_IMAGE=/vmlinuz-linux-test root=/dev/mmcblk1p2 rw reboot=pci,force drm.debug=14
[    0.000000] x86/fpu: x87 FPU will use FXSAVE
[    0.000000] e820: BIOS-provided physical RAM map:
[    0.000000] BIOS-e820: [mem 0x0000000000000000-0x000000000008efff] usable
[    0.000000] BIOS-e820: [mem 0x000000000008f000-0x000000000008ffff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000000090000-0x000000000009dfff] usable
[    0.000000] BIOS-e820: [mem 0x000000000009e000-0x000000000009ffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000100000-0x000000001fffffff] usable
[    0.000000] BIOS-e820: [mem 0x0000000020000000-0x00000000200fffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000020100000-0x00000000782bafff] usable
[    0.000000] BIOS-e820: [mem 0x00000000782bb000-0x00000000784bafff] type 20
[    0.000000] BIOS-e820: [mem 0x00000000784bb000-0x0000000078bbafff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000078bbb000-0x0000000078cbafff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000078cbb000-0x0000000078cfafff] ACPI data
[    0.000000] BIOS-e820: [mem 0x0000000078cfb000-0x000000007951bfff] usable
[    0.000000] BIOS-e820: [mem 0x000000007951c000-0x000000007951cfff] reserved
[    0.000000] BIOS-e820: [mem 0x000000007951d000-0x0000000079526fff] usable
[    0.000000] BIOS-e820: [mem 0x0000000079527000-0x0000000079e26fff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000079e27000-0x0000000079ffffff] usable
[    0.000000] BIOS-e820: [mem 0x00000000e00f8000-0x00000000e00f8fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed01000-0x00000000fed01fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000ffd00000-0x00000000ffffffff] reserved
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] efi: EFI v2.31 by INSYDE Corp.
[    0.000000] efi:  ACPI 2.0=0x78cfa014  ESRT=0x78559e10  SMBIOS=0x78bba000 
[    0.000000] SMBIOS 2.7 present.
[    0.000000] DMI: Acer TP-W4-820-Z3742G06AII/Cheetah3, BIOS V1.16 03/13/2014
[    0.000000] e820: update [mem 0x00000000-0x00000fff] usable ==> reserved
[    0.000000] e820: remove [mem 0x000a0000-0x000fffff] usable
[    0.000000] e820: last_pfn = 0x7a000 max_arch_pfn = 0x400000000
[    0.000000] MTRR default type: uncachable
[    0.000000] MTRR fixed ranges enabled:
[    0.000000]   00000-9FFFF write-back
[    0.000000]   A0000-FFFFF write-protect
[    0.000000] MTRR variable ranges enabled:
[    0.000000]   0 base 0FFD00000 mask FFFC00000 write-protect
[    0.000000]   1 base 000000000 mask FC0000000 write-back
[    0.000000]   2 base 040000000 mask FE0000000 write-back
[    0.000000]   3 base 060000000 mask FF0000000 write-back
[    0.000000]   4 base 070000000 mask FF8000000 write-back
[    0.000000]   5 base 078000000 mask FFC000000 write-back
[    0.000000]   6 base 07B000000 mask FFF000000 uncachable
[    0.000000]   7 base 07AE00000 mask FFFE00000 uncachable
[    0.000000] x86/PAT: Configuration [0-7]: WB  WC  UC- UC  WB  WC  UC- WT  
[    0.000000] esrt: Reserving ESRT space from 0x0000000078559e10 to 0x0000000078559e48.
[    0.000000] Scanning 1 areas for low memory corruption
[    0.000000] Base memory trampoline at [ffff880000097000] 97000 size 24576
[    0.000000] BRK [0x02d43000, 0x02d43fff] PGTABLE
[    0.000000] BRK [0x02d44000, 0x02d44fff] PGTABLE
[    0.000000] BRK [0x02d45000, 0x02d45fff] PGTABLE
[    0.000000] BRK [0x02d46000, 0x02d46fff] PGTABLE
[    0.000000] BRK [0x02d47000, 0x02d47fff] PGTABLE
[    0.000000] BRK [0x02d48000, 0x02d48fff] PGTABLE
[    0.000000] Secure boot could not be determined
[    0.000000] RAMDISK: [mem 0x372c1000-0x37957fff]
[    0.000000] ACPI: Early table checksum verification disabled
[    0.000000] ACPI: RSDP 0x0000000078CFA014 000024 (v02 ACRSYS)
[    0.000000] ACPI: XSDT 0x0000000078CD4188 0000DC (v01 ACRSYS ACRPRDCT 00000003      01000013)
[    0.000000] ACPI: FACP 0x0000000078CF0000 00010C (v05 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: DSDT 0x0000000078CE0000 00B10F (v02 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: UEFI 0x0000000078CF9000 000236 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: TCPA 0x0000000078CF8000 000032 (v02 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: MSDM 0x0000000078CF7000 000055 (v03 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: UEFI 0x0000000078CF6000 000042 (v01 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CF2000 00305D (v01 ACRSYS ACRPRDCT 00001000 1025 00040000)
[    0.000000] ACPI: DBG2 0x0000000078CF1000 000072 (v00 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: HPET 0x0000000078CEF000 000038 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: LPIT 0x0000000078CEE000 000104 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: APIC 0x0000000078CED000 00006C (v03 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: MCFG 0x0000000078CEC000 00003C (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDF000 0005F9 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDD000 001C9F (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDC000 000058 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDB000 0000FF (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDA000 00043A (v01 ACRSYS ACRPRDCT 00001000 1025 00040000)
[    0.000000] ACPI: TPM2 0x0000000078CD9000 000034 (v03 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD8000 000763 (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD7000 000290 (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD6000 00017A (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: FPDT 0x0000000078CD5000 000044 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: CSRT 0x0000000078CD3000 00014C (v00 ACRSYS ACRPRDCT 00000005 1025 00040000)
[    0.000000] ACPI: BGRT 0x0000000078CD2000 000038 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] No NUMA configuration found
[    0.000000] Faking a node at [mem 0x0000000000000000-0x0000000079ffffff]
[    0.000000] NODE_DATA(0) allocated [mem 0x77fe7000-0x77febfff]
[    0.000000] Zone ranges:
[    0.000000]   DMA      [mem 0x0000000000001000-0x0000000000ffffff]
[    0.000000]   DMA32    [mem 0x0000000001000000-0x0000000079ffffff]
[    0.000000]   Normal   empty
[    0.000000]   Device   empty
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000000001000-0x000000000008efff]
[    0.000000]   node   0: [mem 0x0000000000090000-0x000000000009dfff]
[    0.000000]   node   0: [mem 0x0000000000100000-0x000000001fffffff]
[    0.000000]   node   0: [mem 0x0000000020100000-0x00000000782bafff]
[    0.000000]   node   0: [mem 0x0000000078cfb000-0x000000007951bfff]
[    0.000000]   node   0: [mem 0x000000007951d000-0x0000000079526fff]
[    0.000000]   node   0: [mem 0x0000000079e27000-0x0000000079ffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000000001000-0x0000000079ffffff]
[    0.000000] On node 0 totalpages: 494427
[    0.000000]   DMA zone: 64 pages used for memmap
[    0.000000]   DMA zone: 23 pages reserved
[    0.000000]   DMA zone: 3996 pages, LIFO batch:0
[    0.000000]   DMA32 zone: 7744 pages used for memmap
[    0.000000]   DMA32 zone: 490431 pages, LIFO batch:31
[    0.000000] x86/hpet: Will disable the HPET for this platform because it's not reliable
[    0.000000] Reserving Intel graphics memory at 0x000000007af00000-0x000000007eefffff
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] IOAPIC[0]: apic_id 2, version 32, address 0xfec00000, GSI 0-86
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.000000] Using ACPI (MADT) for SMP configuration information
[    0.000000] ACPI: HPET id: 0x8086a201 base: 0xfed00000
[    0.000000] smpboot: Allowing 4 CPUs, 0 hotplug CPUs
[    0.000000] PM: Registered nosave memory: [mem 0x00000000-0x00000fff]
[    0.000000] PM: Registered nosave memory: [mem 0x0008f000-0x0008ffff]
[    0.000000] PM: Registered nosave memory: [mem 0x0009e000-0x0009ffff]
[    0.000000] PM: Registered nosave memory: [mem 0x000a0000-0x000fffff]
[    0.000000] PM: Registered nosave memory: [mem 0x20000000-0x200fffff]
[    0.000000] PM: Registered nosave memory: [mem 0x782bb000-0x784bafff]
[    0.000000] PM: Registered nosave memory: [mem 0x784bb000-0x78bbafff]
[    0.000000] PM: Registered nosave memory: [mem 0x78bbb000-0x78cbafff]
[    0.000000] PM: Registered nosave memory: [mem 0x78cbb000-0x78cfafff]
[    0.000000] PM: Registered nosave memory: [mem 0x7951c000-0x7951cfff]
[    0.000000] PM: Registered nosave memory: [mem 0x79527000-0x79e26fff]
[    0.000000] e820: [mem 0x7ef00000-0xe00f7fff] available for PCI devices
[    0.000000] Booting paravirtualized kernel on bare hardware
[    0.000000] clocksource: refined-jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 6370452778343963 ns
[    0.000000] setup_percpu: NR_CPUS:128 nr_cpumask_bits:128 nr_cpu_ids:4 nr_node_ids:1
[    0.000000] percpu: Embedded 37 pages/cpu @ffff880076a00000 s111448 r8192 d31912 u524288
[    0.000000] pcpu-alloc: s111448 r8192 d31912 u524288 alloc=1*2097152
[    0.000000] pcpu-alloc: [0] 0 1 2 3 
[    0.000000] Built 1 zonelists in Node order, mobility grouping on.  Total pages: 486596
[    0.000000] Policy zone: DMA32
[    0.000000] Kernel command line: BOOT_IMAGE=/vmlinuz-linux-test root=/dev/mmcblk1p2 rw reboot=pci,force drm.debug=14
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Calgary: detecting Calgary via BIOS EBDA area
[    0.000000] Calgary: Unable to locate Rio Grande table in EBDA - bailing!
[    0.000000] Memory: 1893952K/1977708K available (6432K kernel code, 1089K rwdata, 2000K rodata, 1308K init, 904K bss, 83756K reserved, 0K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000] 	Build-time adjustment of leaf fanout to 64.
[    0.000000] 	RCU restricting CPUs from NR_CPUS=128 to nr_cpu_ids=4.
[    0.000000] RCU: Adjusting geometry for rcu_fanout_leaf=64, nr_cpu_ids=4
[    0.000000] NR_IRQS:8448 nr_irqs:1024 0
[    0.000000] Console: colour dummy device 80x25
[    0.000000] console [tty0] enabled
[    0.000000] tsc: Detected 1333.000 MHz processor
[    0.000021] Calibrating delay loop (skipped), value calculated using timer frequency.. 2667.08 BogoMIPS (lpj=4443333)
[    0.000029] pid_max: default: 32768 minimum: 301
[    0.000062] ACPI: Core revision 20170119
[    0.003333] ACPI: 10 ACPI AML tables successfully acquired and loaded
[    0.003333] Security Framework initialized
[    0.003333] Yama: becoming mindful.
[    0.003333] Dentry cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.003333] Inode-cache hash table entries: 131072 (order: 8, 1048576 bytes)
[    0.003333] Mount-cache hash table entries: 4096 (order: 3, 32768 bytes)
[    0.003333] Mountpoint-cache hash table entries: 4096 (order: 3, 32768 bytes)
[    0.003333] CPU: Physical Processor ID: 0
[    0.003333] CPU: Processor Core ID: 0
[    0.003333] ENERGY_PERF_BIAS: Set to 'normal', was 'performance'
[    0.003333] ENERGY_PERF_BIAS: View and update with x86_energy_perf_policy(8)
[    0.003333] mce: CPU supports 6 MCE banks
[    0.003333] CPU0: Thermal monitoring enabled (TM1)
[    0.003333] process: using mwait in idle threads
[    0.003333] Last level iTLB entries: 4KB 48, 2MB 0, 4MB 0
[    0.003333] Last level dTLB entries: 4KB 128, 2MB 16, 4MB 16, 1GB 0
[    0.003333] Freeing SMP alternatives memory: 24K
[    0.003333] ftrace: allocating 25362 entries in 100 pages
[    0.003333] smpboot: Max logical packages: 1
[    0.003333] TSC deadline timer enabled
[    0.003333] smpboot: CPU0: Intel(R) Atom(TM) CPU  Z3740  @ 1.33GHz (family: 0x6, model: 0x37, stepping: 0x3)
[    0.010014] Performance Events: PEBS fmt2+, 8-deep LBR, Silvermont events, 8-deep LBR, full-width counters, Intel PMU driver.
[    0.010041] ... version:                3
[    0.010043] ... bit width:              40
[    0.010045] ... generic registers:      2
[    0.010047] ... value mask:             000000ffffffffff
[    0.010049] ... max period:             0000007fffffffff
[    0.010050] ... fixed-purpose events:   3
[    0.010052] ... event mask:             0000000700000003
[    0.033630] NMI watchdog: enabled on all CPUs, permanently consumes one hw-PMU counter.
[    0.040011] smp: Bringing up secondary CPUs ...
[    0.066707] x86: Booting SMP configuration:
[    0.066711] .... node  #0, CPUs:      #1 #2 #3
[    0.370153] smp: Brought up 1 node, 4 CPUs
[    0.370153] smpboot: Total of 4 processors activated (10677.53 BogoMIPS)
[    0.370835] sched_clock: Marking stable (369999963, 0)->(436519834, -66519871)
[    0.371539] devtmpfs: initialized
[    0.371687] x86/mm: Memory block size: 128MB
[    0.381542] PM: Registering ACPI NVS region [mem 0x0008f000-0x0008ffff] (4096 bytes)
[    0.381546] PM: Registering ACPI NVS region [mem 0x78bbb000-0x78cbafff] (1048576 bytes)
[    0.381593] PM: Registering ACPI NVS region [mem 0x79527000-0x79e26fff] (9437184 bytes)
[    0.382105] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 6370867519511994 ns
[    0.382126] futex hash table entries: 1024 (order: 4, 65536 bytes)
[    0.382280] pinctrl core: initialized pinctrl subsystem
[    0.382354] RTC time: 15:47:01, date: 03/23/17
[    0.382642] NET: Registered protocol family 16
[    0.386491] cpuidle: using governor ladder
[    0.386595] cpuidle: using governor menu
[    0.386601] PCCT header not found.
[    0.386671] ACPI: bus type PCI registered
[    0.386675] acpiphp: ACPI Hot Plug PCI Controller Driver version: 0.5
[    0.386839] PCI: MMCONFIG for domain 0000 [bus 00-3f] at [mem 0xe0000000-0xe3ffffff] (base 0xe0000000)
[    0.386876] PCI: not using MMCONFIG
[    0.386880] PCI: Using configuration type 1 for base access
[    0.389271] HugeTLB registered 2 MB page size, pre-allocated 0 pages
[    0.389994] ACPI: Added _OSI(Module Device)
[    0.389997] ACPI: Added _OSI(Processor Device)
[    0.389999] ACPI: Added _OSI(3.0 _SCP Extensions)
[    0.390002] ACPI: Added _OSI(Processor Aggregator Device)
[    0.410679] ACPI: Dynamic OEM Table Load:
[    0.410702] ACPI: SSDT 0xFFFF880073F5A800 000353 (v01 PmRef  Cpu0Ist  00003000 INTL 20121114)
[    0.411334] ACPI: Dynamic OEM Table Load:
[    0.411353] ACPI: SSDT 0xFFFF880073F15000 000433 (v01 PmRef  Cpu0Cst  00003001 INTL 20121114)
[    0.412661] ACPI: Dynamic OEM Table Load:
[    0.412679] ACPI: SSDT 0xFFFF880073F44400 00015F (v01 PmRef  ApIst    00003000 INTL 20121114)
[    0.413256] ACPI: Dynamic OEM Table Load:
[    0.413273] ACPI: SSDT 0xFFFF880073FC9A80 00008D (v01 PmRef  ApCst    00003000 INTL 20121114)
[    0.416776] ACPI: Interpreter enabled
[    0.416808] ACPI: (supports S0)
[    0.416811] ACPI: Using IOAPIC for interrupt routing
[    0.416899] PCI: MMCONFIG for domain 0000 [bus 00-3f] at [mem 0xe0000000-0xe3ffffff] (base 0xe0000000)
[    0.422529] [Firmware Info]: PCI: MMCONFIG at [mem 0xe0000000-0xe3ffffff] not reserved in ACPI motherboard resources
[    0.422533] PCI: not using MMCONFIG
[    0.422542] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    0.426521] ACPI: Power Resource [USBC] (on)
[    0.427417] ACPI: Power Resource [WWPR] (off)
[    0.434890] ACPI: Power Resource [PLPE] (on)
[    0.443232] ACPI: Power Resource [CLK0] (on)
[    0.443507] ACPI: Power Resource [P28X] (off)
[    0.443626] ACPI: Power Resource [P18X] (off)
[    0.444306] ACPI: Power Resource [CLK1] (on)
[    0.446432] ACPI: Power Resource [TCPR] (off)
[    0.455411] ACPI: PCI Root Bridge [PCI0] (domain 0000 [bus 00-ff])
[    0.455424] acpi PNP0A08:00: _OSC: OS supports [ASPM ClockPM Segments MSI]
[    0.455557] acpi PNP0A08:00: _OSC failed (AE_ERROR); disabling ASPM
[    0.455589] acpi PNP0A08:00: fail to add MMCONFIG information, can't access extended PCI configuration space under this bridge.
[    0.456329] PCI host bridge to bus 0000:00
[    0.456336] pci_bus 0000:00: root bus resource [io  0x0070-0x0077]
[    0.456341] pci_bus 0000:00: root bus resource [io  0x0000-0x006f window]
[    0.456345] pci_bus 0000:00: root bus resource [io  0x0078-0x0cf7 window]
[    0.456349] pci_bus 0000:00: root bus resource [io  0x0d00-0xffff window]
[    0.456353] pci_bus 0000:00: root bus resource [mem 0x000a0000-0x000bffff window]
[    0.456357] pci_bus 0000:00: root bus resource [mem 0x000c0000-0x000dffff window]
[    0.456361] pci_bus 0000:00: root bus resource [mem 0x000e0000-0x000fffff window]
[    0.456365] pci_bus 0000:00: root bus resource [mem 0x90c00000-0x90ffffff window]
[    0.456369] pci_bus 0000:00: root bus resource [mem 0x7af00001-0x7ef00000 window]
[    0.456373] pci_bus 0000:00: root bus resource [mem 0x80000000-0x908ffffe window]
[    0.456377] pci_bus 0000:00: root bus resource [mem 0xfed40000-0xfed40fff window]
[    0.456381] pci_bus 0000:00: root bus resource [bus 00-ff]
[    0.456399] pci 0000:00:00.0: [8086:0f00] type 00 class 0x060000
[    0.456612] pci 0000:00:02.0: [8086:0f31] type 00 class 0x030000
[    0.456632] pci 0000:00:02.0: reg 0x10: [mem 0x90000000-0x903fffff]
[    0.456664] pci 0000:00:02.0: reg 0x18: [mem 0x80000000-0x8fffffff pref]
[    0.456681] pci 0000:00:02.0: reg 0x20: [io  0x1000-0x1007]
[    0.456910] pci 0000:00:14.0: [8086:0f35] type 00 class 0x0c0330
[    0.456937] pci 0000:00:14.0: reg 0x10: [mem 0x90800000-0x9080ffff 64bit]
[    0.457022] pci 0000:00:14.0: PME# supported from D3hot D3cold
[    0.457201] pci 0000:00:1a.0: [8086:0f18] type 00 class 0x108000
[    0.457227] pci 0000:00:1a.0: reg 0x10: [mem 0x90700000-0x907fffff]
[    0.457241] pci 0000:00:1a.0: reg 0x14: [mem 0x90600000-0x906fffff]
[    0.457347] pci 0000:00:1a.0: PME# supported from D0 D3hot
[    0.457520] pci 0000:00:1f.0: [8086:0f1c] type 00 class 0x060100
[    0.458785] ACPI: PCI Interrupt Link [LNKA] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.458992] ACPI: PCI Interrupt Link [LNKB] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.459197] ACPI: PCI Interrupt Link [LNKC] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.459401] ACPI: PCI Interrupt Link [LNKD] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.459605] ACPI: PCI Interrupt Link [LNKE] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.459810] ACPI: PCI Interrupt Link [LNKF] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.460032] ACPI: PCI Interrupt Link [LNKG] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.460247] ACPI: PCI Interrupt Link [LNKH] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.510486] dw_dmac INTL9C60:00: DesignWare DMA Controller, 8 channels
[    0.543851] dw_dmac INTL9C60:01: DesignWare DMA Controller, 8 channels
[    0.544251] pci 0000:00:02.0: vgaarb: setting as boot VGA device
[    0.544257] pci 0000:00:02.0: vgaarb: VGA device added: decodes=io+mem,owns=io+mem,locks=none
[    0.544263] pci 0000:00:02.0: vgaarb: bridge control possible
[    0.544265] vgaarb: loaded
[    0.544435] Registered efivars operations
[    0.556157] PCI: Using ACPI for IRQ routing
[    0.556164] PCI: pci_cache_line_size set to 64 bytes
[    0.556194] Expanded resource reserved due to conflict with PCI Bus 0000:00
[    0.556201] e820: reserve RAM buffer [mem 0x0008f000-0x0008ffff]
[    0.556204] e820: reserve RAM buffer [mem 0x0009e000-0x0009ffff]
[    0.556208] e820: reserve RAM buffer [mem 0x782bb000-0x7bffffff]
[    0.556211] e820: reserve RAM buffer [mem 0x7951c000-0x7bffffff]
[    0.556214] e820: reserve RAM buffer [mem 0x79527000-0x7bffffff]
[    0.556217] e820: reserve RAM buffer [mem 0x7a000000-0x7bffffff]
[    0.556484] NetLabel: Initializing
[    0.556487] NetLabel:  domain hash size = 128
[    0.556489] NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
[    0.556528] NetLabel:  unlabeled traffic allowed by default
[    0.557433] clocksource: Switched to clocksource refined-jiffies
[    0.583790] VFS: Disk quotas dquot_6.6.0
[    0.583842] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.584087] pnp: PnP ACPI init
[    0.584246] pnp 00:00: Plug and Play ACPI device, IDs PNP0b00 (active)
[    0.584426] system 00:01: [io  0x0680-0x069f] has been reserved
[    0.584432] system 00:01: [io  0x0400-0x047f] has been reserved
[    0.584437] system 00:01: [io  0x0500-0x05fe] has been reserved
[    0.584441] system 00:01: [io  0x0600-0x061f] has been reserved
[    0.584446] system 00:01: [io  0x164e-0x164f] has been reserved
[    0.584456] system 00:01: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.587667] pnp: PnP ACPI: found 2 devices
[    0.592875] pci_bus 0000:00: resource 4 [io  0x0070-0x0077]
[    0.592881] pci_bus 0000:00: resource 5 [io  0x0000-0x006f window]
[    0.592885] pci_bus 0000:00: resource 6 [io  0x0078-0x0cf7 window]
[    0.592890] pci_bus 0000:00: resource 7 [io  0x0d00-0xffff window]
[    0.592894] pci_bus 0000:00: resource 8 [mem 0x000a0000-0x000bffff window]
[    0.592898] pci_bus 0000:00: resource 9 [mem 0x000c0000-0x000dffff window]
[    0.592903] pci_bus 0000:00: resource 10 [mem 0x000e0000-0x000fffff window]
[    0.592907] pci_bus 0000:00: resource 11 [mem 0x90c00000-0x90ffffff window]
[    0.592911] pci_bus 0000:00: resource 12 [mem 0x7af00001-0x7ef00000 window]
[    0.592915] pci_bus 0000:00: resource 13 [mem 0x80000000-0x908ffffe window]
[    0.592919] pci_bus 0000:00: resource 14 [mem 0xfed40000-0xfed40fff window]
[    0.593116] NET: Registered protocol family 2
[    0.593488] TCP established hash table entries: 16384 (order: 5, 131072 bytes)
[    0.593594] TCP bind hash table entries: 16384 (order: 6, 262144 bytes)
[    0.593714] TCP: Hash tables configured (established 16384 bind 16384)
[    0.593803] UDP hash table entries: 1024 (order: 3, 32768 bytes)
[    0.593833] UDP-Lite hash table entries: 1024 (order: 3, 32768 bytes)
[    0.593959] NET: Registered protocol family 1
[    0.594026] pci 0000:00:02.0: Video device with shadowed ROM at [mem 0x000c0000-0x000dffff]
[    0.594462] PCI: CLS 0 bytes, default 64
[    0.594608] Unpacking initramfs...
[    0.819061] Freeing initrd memory: 6748K
[    0.819151] clocksource: tsc: mask: 0xffffffffffffffff max_cycles: 0x1336e3dbd1a, max_idle_ns: 440795236868 ns
[    0.819198] clocksource: Switched to clocksource tsc
[    0.819464] Scanning for low memory corruption every 60 seconds
[    0.821039] Initialise system trusted keyrings
[    0.821273] workingset: timestamp_bits=40 max_order=19 bucket_order=0
[    0.825060] zbud: loaded
[    0.826823] Key type asymmetric registered
[    0.826863] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 249)
[    0.826946] io scheduler noop registered
[    0.826949] io scheduler deadline registered
[    0.827043] io scheduler cfq registered (default)
[    0.827046] io scheduler mq-deadline registered
[    0.827390] efifb: probing for efifb
[    0.827422] efifb: framebuffer at 0x80000000, using 1920k, total 1920k
[    0.827426] efifb: mode is 800x600x32, linelength=3200, pages=1
[    0.827427] efifb: scrolling: redraw
[    0.827431] efifb: Truecolor: size=8:8:8:8, shift=24:16:8:0
[    0.832069] Console: switching to colour frame buffer device 100x37
[    0.836430] fb0: EFI VGA frame buffer device
[    0.836453] intel_idle: MWAIT substates: 0x33000020
[    0.836456] intel_idle: v0.4.1 model 0x37
[    0.836911] intel_idle: lapic_timer_reliable_states 0xffffffff
[    0.841260] GHES: HEST is not enabled!
[    0.841503] Serial: 8250/16550 driver, 4 ports, IRQ sharing enabled
[    0.844460] hpet: number irqs doesn't agree with number of timers
[    0.844548] Linux agpgart interface v0.103
[    0.846984] ACPI Warning: Could not enable fixed event - RealTimeClock (4) (20170119/evxface-654)
[    0.848327] rtc_cmos 00:00: rtc core: registered rtc_cmos as rtc0
[    0.848416] rtc_cmos 00:00: alarms up to one day, 242 bytes nvram
[    0.848464] intel_pstate: Intel P-state driver initializing
[    0.851239] ledtrig-cpu: registered to indicate activity on CPUs
[    0.853171] NET: Registered protocol family 10
[    0.880513] Segment Routing with IPv6
[    0.880599] NET: Registered protocol family 17
[    0.883798] microcode: sig=0x30673, pf=0x2, revision=0x322
[    0.885187] microcode: Microcode Update Driver: v2.2.
[    0.888542] registered taskstats version 1
[    0.888604] Loading compiled-in X.509 certificates
[    0.888714] zswap: loaded using pool lzo/zbud
[    0.892492]   Magic number: 9:536:791
[    0.893085] rtc_cmos 00:00: setting system clock to 2017-03-23 15:47:02 UTC (1490284022)
[    0.893396] PM: Hibernation image not present or could not be loaded.
[    0.900673] Freeing unused kernel memory: 1308K
[    0.900678] Write protecting the kernel read-only data: 10240k
[    0.903127] Freeing unused kernel memory: 1744K
[    0.904264] Freeing unused kernel memory: 48K
[    0.962351] random: systemd-tmpfile: uninitialized urandom read (16 bytes read)
[    0.969158] random: systemd-udevd: uninitialized urandom read (16 bytes read)
[    0.969649] random: systemd-udevd: uninitialized urandom read (16 bytes read)
[    0.974489] random: systemd-udevd: uninitialized urandom read (16 bytes read)
[    0.974566] random: systemd-udevd: uninitialized urandom read (16 bytes read)
[    0.974603] random: systemd-udevd: uninitialized urandom read (16 bytes read)
[    0.975329] random: systemd-udevd: uninitialized urandom read (16 bytes read)
[    0.975398] random: systemd-udevd: uninitialized urandom read (16 bytes read)
[    0.975434] random: systemd-udevd: uninitialized urandom read (16 bytes read)
[    0.980804] random: udevadm: uninitialized urandom read (16 bytes read)
[    1.068177] sdhci: Secure Digital Host Controller Interface driver
[    1.068179] sdhci: Copyright(c) Pierre Ossman
[    1.084747] i8042: PNP: No PS/2 controller found.
[    1.117134] ACPI: bus type USB registered
[    1.117216] usbcore: registered new interface driver usbfs
[    1.117253] usbcore: registered new interface driver hub
[    1.117345] usbcore: registered new device driver usb
[    1.120871] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.120891] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 1
[    1.122012] xhci_hcd 0000:00:14.0: hcc params 0x200077c1 hci version 0x100 quirks 0x00009810
[    1.122021] xhci_hcd 0000:00:14.0: cache line size of 64 is not supported
[    1.122626] hub 1-0:1.0: USB hub found
[    1.122654] hub 1-0:1.0: 6 ports detected
[    1.277663] mmc0: SDHCI controller on ACPI [INT33BB:00] using ADMA
[    1.297238] mmc1: SDHCI controller on ACPI [80860F14:00] using ADMA
[    1.320892] mmc2: SDHCI controller on ACPI [80860F14:01] using ADMA
[    1.436212] mmc0: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.458424] mmc1: new HS200 MMC card at address 0001
[    1.465957] mmcblk1: mmc1:0001 MCG8GC 58.2 GiB 
[    1.467645] mmcblk1boot0: mmc1:0001 MCG8GC partition 1 4.00 MiB
[    1.469474] mmcblk1boot1: mmc1:0001 MCG8GC partition 2 4.00 MiB
[    1.469913] mmcblk1rpmb: mmc1:0001 MCG8GC partition 3 4.00 MiB
[    1.470697] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.478029]  mmcblk1: p1 p2
[    1.489091] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.491425] random: fast init done
[    1.556400] mmc0: new ultra high speed DDR50 SDIO card at address 0001
[    1.653592] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.653623] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 2
[    1.655107] hub 2-0:1.0: USB hub found
[    1.655170] hub 2-0:1.0: 1 port detected
[    1.786788] EXT4-fs (mmcblk1p2): mounted filesystem with ordered data mode. Opts: (null)
[    1.979746] usb 1-2: new high-speed USB device number 2 using xhci_hcd
[    1.988365] ip_tables: (C) 2000-2006 Netfilter Core Team
[    1.998520] systemd[1]: systemd 232 running in system mode. (+PAM -AUDIT -SELINUX -IMA -APPARMOR +SMACK -SYSVINIT +UTMP +LIBCRYPTSETUP +GCRYPT +GNUTLS +ACL +XZ +LZ4 +SECCOMP +BLKID +ELFUTILS +KMOD +IDN)
[    1.998899] systemd[1]: Detected architecture x86-64.
[    2.001746] systemd[1]: Set hostname to <erhoof_tabletpc>.
[    2.110439] hub 1-2:1.0: USB hub found
[    2.110518] hub 1-2:1.0: 4 ports detected
[    2.130672] systemd[1]: Created slice System Slice.
[    2.138642] systemd[1]: Listening on LVM2 metadata daemon socket.
[    2.140208] systemd[1]: Mounting Debug File System...
[    2.140880] systemd[1]: Set up automount Arbitrary Executable File Formats File System Automount Point.
[    2.141149] systemd[1]: Reached target Remote File Systems.
[    2.141340] systemd[1]: Reached target Swap.
[    2.141605] systemd[1]: Listening on Journal Socket (/dev/log).
[    2.171186] EXT4-fs (mmcblk1p2): re-mounted. Opts: data=ordered,discard
[    2.389236] usb 1-2.3: new low-speed USB device number 3 using xhci_hcd
[    2.498122] systemd-journald[165]: Received request to flush runtime journal from PID 1
[    2.520742] ACPI: AC Adapter [ADP1] (off-line)
[    2.539489] 80860F0A:00: ttyS0 at MMIO 0x9094d000 (irq = 186, base_baud = 2764800) is a 16550A
[    2.629647] Bluetooth: Core ver 2.22
[    2.629685] NET: Registered protocol family 31
[    2.629687] Bluetooth: HCI device and connection manager initialized
[    2.629694] Bluetooth: HCI socket layer initialized
[    2.629698] Bluetooth: L2CAP socket layer initialized
[    2.629709] Bluetooth: SCO socket layer initialized
[    2.640851] Bluetooth: HCI UART driver ver 2.3
[    2.640856] Bluetooth: HCI UART protocol H4 registered
[    2.640857] Bluetooth: HCI UART protocol BCSP registered
[    2.640859] Bluetooth: HCI UART protocol LL registered
[    2.640860] Bluetooth: HCI UART protocol ATH3K registered
[    2.640862] Bluetooth: HCI UART protocol Three-wire (H5) registered
[    2.640948] Bluetooth: HCI UART protocol Intel registered
[    2.642603] FUJITSU Extended Socket Network Device Driver - version 1.2 - Copyright (c) 2015 FUJITSU LIMITED
[    2.643562] wmi: Mapper loaded
[    2.660498] hci_bcm BCM2E3F:00: BCM irq: 187
[    2.660575] hci_bcm BCM2E3F:00: BCM2E3F:00 device registered.
[    2.660757] Bluetooth: HCI UART protocol Broadcom registered
[    2.660759] Bluetooth: HCI UART protocol QCA registered
[    2.660761] Bluetooth: HCI UART protocol AG6XX registered
[    2.660762] Bluetooth: HCI UART protocol Marvell registered
[    2.662638] i8042: PNP: No PS/2 controller found.
[    2.674493] input: Lid Switch as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0C0D:00/input/input0
[    2.674502] ACPI: Lid Switch [LID]
[    2.686371] intel_sst_acpi 80860F28:00: BYT-CR not detected
[    2.686577] intel_sst_acpi 80860F28:00: LPE base: 0x90a00000 size:0x200000
[    2.686580] intel_sst_acpi 80860F28:00: IRAM base: 0x90ac0000
[    2.686632] intel_sst_acpi 80860F28:00: DRAM base: 0x90b00000
[    2.686641] intel_sst_acpi 80860F28:00: SHIM base: 0x90b40000
[    2.686651] intel_sst_acpi 80860F28:00: Mailbox base: 0x90b44000
[    2.686658] intel_sst_acpi 80860F28:00: DDR base: 0x20000000
[    2.686752] intel_sst_acpi 80860F28:00: Got drv data max stream 25
[    2.693297] [Firmware Bug]: No valid trip found
[    2.723892] [Firmware Bug]: No valid trip found
[    2.740355] hidraw: raw HID events driver (C) Jiri Kosina
[    2.764302] genirq: Flags mismatch irq 8. 00002008 (SMO91D0:00) vs. 00000080 (rtc0)
[    2.765945] i2c_hid i2c-SMO91D0:00: Could not register for SMO91D0:00 interrupt, irq = 8, ret = -16
[    2.776113] i2c_hid: probe of i2c-SMO91D0:00 failed with error -16
[    2.778196] input: PC Speaker as /devices/platform/pcspkr/input/input1
[    2.811503] SSE version of gcm_enc/dec engaged.
[    2.818950] FAT-fs (mmcblk1p1): Volume was not properly unmounted. Some data may be corrupt. Please run fsck.
[    2.891413] i8042: PNP: No PS/2 controller found.
[    2.895233] input: gpio-keys as /devices/platform/gpio-keys.0.auto/input/input2
[    2.895458] input: gpio-keys as /devices/platform/gpio-keys.1.auto/input/input3
[    2.927070] iTCO_vendor_support: vendor-support=0
[    2.928233] bytcr_rt5640 bytcr_rt5640: quirk DMIC1_MAP enabled
[    2.928238] bytcr_rt5640 bytcr_rt5640: quirk DMIC enabled
[    2.928240] bytcr_rt5640 bytcr_rt5640: quirk MCLK_EN enabled
[    2.929587] iTCO_wdt: Intel TCO WatchDog Timer Driver v1.11
[    2.929712] iTCO_wdt: Found a Bay Trail SoC TCO device (Version=3, TCOBASE=0x0460)
[    2.929934] iTCO_wdt: initialized. heartbeat=30 sec (nowayout=0)
[    2.935993] bytcr_rt5640 bytcr_rt5640: snd-soc-dummy-dai <-> media-cpu-dai mapping ok
[    2.936053] bytcr_rt5640 bytcr_rt5640: snd-soc-dummy-dai <-> deepbuffer-cpu-dai mapping ok
[    2.936090] compress asoc: snd-soc-dummy-dai <-> compress-cpu-dai mapping ok
[    2.937333] bytcr_rt5640 bytcr_rt5640: rt5640-aif1 <-> ssp2-port mapping ok
[    2.999791] (NULL device *): hwmon_device_register() is deprecated. Please convert the driver to use hwmon_device_register_with_info().
[    2.999898] (NULL device *): hwmon_device_register() is deprecated. Please convert the driver to use hwmon_device_register_with_info().
[    3.006687] intel_rapl: Found RAPL domain package
[    3.006691] intel_rapl: Found RAPL domain core
[    3.070858] input: SYNA7300:00 06CB:0106 as /devices/platform/80860F41:05/i2c-5/i2c-SYNA7300:00/0018:06CB:0106.0001/input/input4
[    3.071153] hid-multitouch 0018:06CB:0106.0001: input,hidraw0: I2C HID v1.00 Device [SYNA7300:00 06CB:0106] on i2c-SYNA7300:00
[    3.079230] mousedev: PS/2 mouse device common for all mice
[    3.084770] usbcore: registered new interface driver usbhid
[    3.084775] usbhid: USB HID core driver
[    3.091390] input: Gaming Keyboard as /devices/pci0000:00/0000:00:14.0/usb1/1-2/1-2.3/1-2.3:1.0/0003:1017:0001.0002/input/input9
[    3.133832] mmc0: queuing unknown CIS tuple 0x80 (7 bytes)
[    3.146206] hid-generic 0003:1017:0001.0002: input,hidraw1: USB HID v1.11 Keyboard [Gaming Keyboard] on usb-0000:00:14.0-2.3/input0
[    3.148822] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    3.148941] input: Gaming Keyboard as /devices/pci0000:00/0000:00:14.0/usb1/1-2/1-2.3/1-2.3:1.1/0003:1017:0001.0003/input/input10
[    3.163879] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    3.205612] hid-generic 0003:1017:0001.0003: input,hiddev0,hidraw2: USB HID v1.11 Keyboard [Gaming Keyboard] on usb-0000:00:14.0-2.3/input1
[    3.240395] usbcore: registered new interface driver brcmfmac
[    3.402094] brcmfmac: brcmf_c_preinit_dcmds: Firmware version = wl0: Jul 17 2013 07:36:07 version 6.10.197.71 (r412987) FWID 01-882d2634
[    3.407530] brcmfmac: brcmf_cfg80211_reg_notifier: not a ISO3166 code (0x30 0x30)
[    3.587038] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    3.618299] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    3.786373] i2c_designware 80860F41:00: controller timed out
[    3.813608] i2c_designware 80860F41:00: timeout in disabling adapter
[    3.814350] ACPI: Battery Slot [BATC] (battery present)
[    3.840056] i2c_designware 80860F41:00: timeout waiting for bus ready
[    4.145042] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    4.374066] brcmfmac: brcmf_p2p_create_p2pdev: set p2p_disc error
[    4.374339] brcmfmac: brcmf_cfg80211_add_iface: add iface p2p-dev-wlan0 type 10 failed: err=-16
[    4.402110] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    5.343194] random: crng init done
[    5.364284] i2c_designware 80860F41:00: timeout in disabling adapter
[    8.679672] brcmfmac: brcmf_cfg80211_escan_handler: scan not ready, bsscfgidx=0
[    8.679975] brcmfmac: brcmf_fweh_event_worker: event handler failed (69)
[    8.692851] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[   16.112763] IPv6: ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
[   37.327658] [drm:i915_driver_load [i915]] No PCH found.
[   37.327720] [drm:intel_power_domains_init [i915]] Allowed DC state mask 00
[   37.327935] [drm:intel_device_info_dump [i915]] i915 device info: platform=VALLEYVIEW gen=7 pciid=0x0f31 rev=0x09
[   37.327992] [drm:intel_device_info_dump [i915]] i915 device info: is_mobile: no
[   37.328049] [drm:intel_device_info_dump [i915]] i915 device info: is_lp: yes
[   37.328105] [drm:intel_device_info_dump [i915]] i915 device info: is_alpha_support: no
[   37.328161] [drm:intel_device_info_dump [i915]] i915 device info: has_64bit_reloc: no
[   37.328217] [drm:intel_device_info_dump [i915]] i915 device info: has_aliasing_ppgtt: yes
[   37.328273] [drm:intel_device_info_dump [i915]] i915 device info: has_csr: no
[   37.328328] [drm:intel_device_info_dump [i915]] i915 device info: has_ddi: no
[   37.328384] [drm:intel_device_info_dump [i915]] i915 device info: has_decoupled_mmio: no
[   37.328441] [drm:intel_device_info_dump [i915]] i915 device info: has_dp_mst: no
[   37.328496] [drm:intel_device_info_dump [i915]] i915 device info: has_fbc: no
[   37.328552] [drm:intel_device_info_dump [i915]] i915 device info: has_fpga_dbg: no
[   37.328608] [drm:intel_device_info_dump [i915]] i915 device info: has_full_ppgtt: yes
[   37.328664] [drm:intel_device_info_dump [i915]] i915 device info: has_full_48bit_ppgtt: no
[   37.328720] [drm:intel_device_info_dump [i915]] i915 device info: has_gmbus_irq: yes
[   37.328776] [drm:intel_device_info_dump [i915]] i915 device info: has_gmch_display: yes
[   37.328832] [drm:intel_device_info_dump [i915]] i915 device info: has_guc: no
[   37.328888] [drm:intel_device_info_dump [i915]] i915 device info: has_hotplug: yes
[   37.328944] [drm:intel_device_info_dump [i915]] i915 device info: has_hw_contexts: yes
[   37.329000] [drm:intel_device_info_dump [i915]] i915 device info: has_l3_dpf: no
[   37.329056] [drm:intel_device_info_dump [i915]] i915 device info: has_llc: no
[   37.329112] [drm:intel_device_info_dump [i915]] i915 device info: has_logical_ring_contexts: no
[   37.329168] [drm:intel_device_info_dump [i915]] i915 device info: has_overlay: no
[   37.329224] [drm:intel_device_info_dump [i915]] i915 device info: has_pipe_cxsr: no
[   37.329327] [drm:intel_device_info_dump [i915]] i915 device info: has_pooled_eu: no
[   37.329385] [drm:intel_device_info_dump [i915]] i915 device info: has_psr: yes
[   37.329445] [drm:intel_device_info_dump [i915]] i915 device info: has_rc6: yes
[   37.329502] [drm:intel_device_info_dump [i915]] i915 device info: has_rc6p: no
[   37.329558] [drm:intel_device_info_dump [i915]] i915 device info: has_resource_streamer: no
[   37.329615] [drm:intel_device_info_dump [i915]] i915 device info: has_runtime_pm: yes
[   37.329671] [drm:intel_device_info_dump [i915]] i915 device info: has_snoop: no
[   37.329727] [drm:intel_device_info_dump [i915]] i915 device info: cursor_needs_physical: no
[   37.329787] [drm:intel_device_info_dump [i915]] i915 device info: hws_needs_physical: no
[   37.329844] [drm:intel_device_info_dump [i915]] i915 device info: overlay_needs_physical: no
[   37.329900] [drm:intel_device_info_dump [i915]] i915 device info: supports_tv: no
[   37.330256] [drm:intel_device_info_runtime_init [i915]] slice mask: 0000
[   37.330313] [drm:intel_device_info_runtime_init [i915]] slice total: 0
[   37.330370] [drm:intel_device_info_runtime_init [i915]] subslice total: 0
[   37.330428] [drm:intel_device_info_runtime_init [i915]] subslice mask 0000
[   37.330484] [drm:intel_device_info_runtime_init [i915]] subslice per slice: 0
[   37.330541] [drm:intel_device_info_runtime_init [i915]] EU total: 0
[   37.330600] [drm:intel_device_info_runtime_init [i915]] EU per subslice: 0
[   37.330656] [drm:intel_device_info_runtime_init [i915]] has slice power gating: n
[   37.330713] [drm:intel_device_info_runtime_init [i915]] has subslice power gating: n
[   37.330772] [drm:intel_device_info_runtime_init [i915]] has EU power gating: n
[   37.330831] [drm:intel_sanitize_enable_ppgtt [i915]] disabling PPGTT on pre-B3 step VLV
[   37.330887] [drm:i915_driver_load [i915]] ppgtt mode: 0
[   37.330945] [drm:i915_driver_load [i915]] use GPU semaphores? yes
[   37.330967] [drm] Memory usable by graphics device = 2048M
[   37.331027] [drm:i915_ggtt_probe_hw [i915]] GMADR size = 256M
[   37.331086] [drm:i915_ggtt_probe_hw [i915]] GTT stolen size = 64M
[   37.331093] checking generic (80000000 1e0000) vs hw (80000000 10000000)
[   37.331094] fb: switching to inteldrmfb from EFI VGA
[   37.331178] Console: switching to colour dummy device 80x25
[   37.331486] [drm] Replacing VGA console driver
[   37.331613] [drm:i915_gem_init_stolen [i915]] Memory reserved for graphics device: 65536K, usable: 65536K
[   37.331688] [drm:intel_opregion_setup [i915]] graphic opregion physical addr: 0x78c63010
[   37.331781] [drm:intel_opregion_setup [i915]] Public ACPI methods supported
[   37.331845] [drm:intel_opregion_setup [i915]] ASLE supported
[   37.331908] [drm:intel_opregion_setup [i915]] Found valid VBT in ACPI OpRegion (Mailbox #4)
[   37.332052] [drm:intel_gvt_init [i915]] GVT-g is disabled by kernel params
[   37.332056] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[   37.332057] [drm] Driver supports precise vblank timestamp query.
[   37.332120] [drm:intel_bios_init [i915]] Set default to SSC at 100000 kHz
[   37.332185] [drm:intel_bios_init [i915]] VBT signature "$VBT VALLEYVIEW    ", BDB version 178
[   37.332248] [drm:intel_bios_init [i915]] BDB_GENERAL_FEATURES int_tv_support 0 int_crt_support 0 lvds_use_ssc 0 lvds_ssc_freq 120000 display_clock_mode 0 fdi_rx_polarity_inverted 0
[   37.332317] [drm:intel_bios_init [i915]] crt_ddc_bus_pin: 2
[   37.332383] [drm:intel_opregion_get_panel_type [i915]] Failed to get panel details from OpRegion (-19)
[   37.332444] [drm:intel_bios_init [i915]] Panel type: 3 (VBT)
[   37.332506] [drm:intel_bios_init [i915]] DRRS supported mode is seamless
[   37.332573] [drm:intel_bios_init [i915]] Found panel mode in BIOS VBT tables:
[   37.332633] [drm:drm_mode_debug_printmodeline [drm]] Modeline 0:"800x1280" 0 81250 800 840 844 884 1280 1290 1294 1306 0x8 0xa
[   37.332698] [drm:intel_bios_init [i915]] VBT initial LVDS value 0
[   37.332763] [drm:intel_bios_init [i915]] VBT backlight PWM modulation frequency 10000 Hz, active high, min brightness 15, level 255, controller 0
[   37.332826] [drm:intel_bios_init [i915]] No SDVO device info is found in VBT
[   37.332889] [drm:intel_bios_init [i915]] DRRS State Enabled:1
[   37.332955] [drm:intel_bios_init [i915]] Found MIPI Config block, panel index = 3
[   37.333019] [drm:intel_bios_init [i915]] Found MIPI sequence block v1
[   37.333083] [drm:intel_bios_init [i915]] MIPI related VBT parsing complete
[   37.333171] [drm:intel_dsm_detect [i915]] no _DSM method for intel device
[   37.333246] [drm:intel_update_rawclk [i915]] rawclk rate: 200000 kHz
[   37.333317] [drm:intel_power_well_enable [i915]] enabling always-on
[   37.333375] [drm:intel_power_well_enable [i915]] enabling display
[   37.333440] [drm:intel_power_well_enable [i915]] enabling dpio-tx-b-01
[   37.333500] [drm:intel_power_well_enable [i915]] enabling dpio-tx-b-23
[   37.333560] [drm:intel_power_well_enable [i915]] enabling dpio-tx-c-01
[   37.333622] [drm:intel_power_well_enable [i915]] enabling dpio-tx-c-23
[   37.333682] [drm:intel_power_well_enable [i915]] enabling dpio-common
[   37.334357] [drm:intel_fbc_init [i915]] Sanitized enable_fbc value: 0
[   37.334424] [drm:intel_modeset_init [i915]] 2 display pipes available.
[   37.334537] [drm:intel_modeset_init [i915]] CZ clock rate: 266667 kHz
[   37.334606] [drm:intel_update_cdclk [i915]] Current CD clock rate: 320000 kHz, VCO: 1600000 kHz, ref: 0 kHz
[   37.334683] [drm:intel_update_max_cdclk [i915]] Max CD clock rate: 400000 kHz
[   37.334746] [drm:intel_update_max_cdclk [i915]] Max dotclock rate: 360000 kHz
[   37.334756] i915 0000:00:02.0: vgaarb: changed VGA decodes: olddecodes=io+mem,decodes=io+mem:owns=io+mem
[   37.335148] [drm:intel_dp_init_connector [i915]] Adding DP connector on port B
[   37.335219] [drm:intel_dp_init_connector [i915]] using AUX B for port B (platform default)
[   37.335295] [drm:intel_hdmi_init_connector [i915]] Adding HDMI connector on port B
[   37.335360] [drm:intel_hdmi_init_connector [i915]] Using DDC pin 0x5 for port B (platform default)
[   37.335429] [drm:intel_dp_init_connector [i915]] Adding DP connector on port C
[   37.335493] [drm:intel_dp_init_connector [i915]] using AUX C for port C (platform default)
[   37.335559] [drm:intel_hdmi_init_connector [i915]] Adding HDMI connector on port C
[   37.335623] [drm:intel_hdmi_init_connector [i915]] Using DDC pin 0x4 for port C (platform default)
[   37.335684] [drm:intel_dsi_init [i915]] 
[   37.335749] [drm:intel_dsi_vbt_init [i915]] 
[   37.335811] [drm:intel_dsi_vbt_init [i915]] Pclk 81250
[   37.335871] [drm:intel_dsi_vbt_init [i915]] Pixel overlap 0
[   37.335961] [drm:intel_dsi_vbt_init [i915]] Lane count 4
[   37.336024] [drm:intel_dsi_vbt_init [i915]] DPHY param reg 0x3d12400d
[   37.336085] [drm:intel_dsi_vbt_init [i915]] Video mode format non-burst with sync events
[   37.336148] [drm:intel_dsi_vbt_init [i915]] Burst mode ratio 100
[   37.336211] [drm:intel_dsi_vbt_init [i915]] Reset timer 255
[   37.336274] [drm:intel_dsi_vbt_init [i915]] Eot enabled
[   37.336335] [drm:intel_dsi_vbt_init [i915]] Clockstop enabled
[   37.336396] [drm:intel_dsi_vbt_init [i915]] Mode video
[   37.336457] [drm:intel_dsi_vbt_init [i915]] Dual link: NONE
[   37.336519] [drm:intel_dsi_vbt_init [i915]] Pixel Format 0
[   37.336581] [drm:intel_dsi_vbt_init [i915]] TLPX 0
[   37.336642] [drm:intel_dsi_vbt_init [i915]] LP RX Timeout 0xffff
[   37.336703] [drm:intel_dsi_vbt_init [i915]] Turnaround Timeout 0x14
[   37.336764] [drm:intel_dsi_vbt_init [i915]] Init Count 0x7d0
[   37.336826] [drm:intel_dsi_vbt_init [i915]] HS to LP Count 0x24
[   37.336887] [drm:intel_dsi_vbt_init [i915]] LP Byte Clock 4
[   37.336947] [drm:intel_dsi_vbt_init [i915]] DBI BW Timer 0x0
[   37.337008] [drm:intel_dsi_vbt_init [i915]] LP to HS Clock Count 0x23
[   37.337069] [drm:intel_dsi_vbt_init [i915]] HS to LP Clock Count 0xf
[   37.337130] [drm:intel_dsi_vbt_init [i915]] BTA enabled
[   37.354335] [drm:pwm_setup_backlight [i915]] *ERROR* Failed to own the pwm chip
[   37.354445] [drm:intel_panel_setup_backlight [i915]] failed to setup backlight for connector DSI-1
[   37.354561] [drm:intel_set_plane_visible [i915]] pipe A active planes 0x1
[   37.354649] [drm:intel_modeset_setup_hw_state [i915]] [CRTC:34:pipe A] hw state readout: enabled
[   37.354739] [drm:intel_set_plane_visible [i915]] pipe B active planes 0x0
[   37.354826] [drm:intel_modeset_setup_hw_state [i915]] [CRTC:43:pipe B] hw state readout: disabled
[   37.354915] [drm:intel_modeset_setup_hw_state [i915]] [ENCODER:44:DP B] hw state readout: disabled, pipe A
[   37.355004] [drm:intel_modeset_setup_hw_state [i915]] [ENCODER:48:HDMI B] hw state readout: disabled, pipe A
[   37.355093] [drm:intel_modeset_setup_hw_state [i915]] [ENCODER:51:DP C] hw state readout: disabled, pipe A
[   37.355181] [drm:intel_modeset_setup_hw_state [i915]] [ENCODER:53:HDMI C] hw state readout: disabled, pipe A
[   37.355265] [drm:intel_dsi_get_hw_state [i915]] 
[   37.355352] [drm:intel_dsi_get_config [i915]] 
[   37.355436] [drm:intel_dsi_get_pclk [i915]] 
[   37.355532] [drm:intel_modeset_setup_hw_state [i915]] [ENCODER:55:DSI A] hw state readout: enabled, pipe A
[   37.355617] [drm:intel_dsi_get_hw_state [i915]] 
[   37.355706] [drm:intel_modeset_setup_hw_state [i915]] [CONNECTOR:56:DSI-1] hw state readout: enabled
[   37.355795] [drm:intel_modeset_setup_hw_state [i915]] [CONNECTOR:45:DP-1] hw state readout: disabled
[   37.355884] [drm:intel_modeset_setup_hw_state [i915]] [CONNECTOR:49:HDMI-A-1] hw state readout: disabled
[   37.356000] [drm:intel_modeset_setup_hw_state [i915]] [CONNECTOR:52:DP-2] hw state readout: disabled
[   37.356090] [drm:intel_modeset_setup_hw_state [i915]] [CONNECTOR:54:HDMI-A-2] hw state readout: disabled
[   37.356202] [drm:intel_dump_pipe_config [i915]] [CRTC:34:pipe A][setup_hw_state]
[   37.356294] [drm:intel_dump_pipe_config [i915]] cpu_transcoder: A, pipe bpp: 24, dithering: 0
[   37.356382] [drm:intel_dump_pipe_config [i915]] audio: 0, infoframes: 0
[   37.356469] [drm:intel_dump_pipe_config [i915]] requested mode:
[   37.356493] [drm:drm_mode_debug_printmodeline [drm]] Modeline 0:"800x1280" 71 82292 800 840 844 884 1280 1290 1294 1306 0x40 0x0
[   37.356584] [drm:intel_dump_pipe_config [i915]] adjusted mode:
[   37.356603] [drm:drm_mode_debug_printmodeline [drm]] Modeline 0:"800x1280" 71 82292 800 840 844 884 1280 1290 1294 1306 0x40 0x0
[   37.356693] [drm:intel_dump_pipe_config [i915]] crtc timings: 82292 800 840 844 884 1280 1290 1294 1306, type: 0x40 flags: 0x0
[   37.356780] [drm:intel_dump_pipe_config [i915]] port clock: 82292, pipe src size: 800x600, pixel rate 82292
[   37.356872] [drm:intel_dump_pipe_config [i915]] gmch pfit: control: 0x80000000, ratios: 0x07801000, lvds border: 0x00000000
[   37.356958] [drm:intel_dump_pipe_config [i915]] ips: 0, double wide: 0
[   37.357046] [drm:intel_dpll_dump_hw_state [i915]] dpll_hw_state: dpll: 0x30002000, dpll_md: 0x3, fp0: 0x0, fp1: 0x0
[   37.357136] [drm:intel_dump_pipe_config [i915]] planes on this crtc
[   37.357212] [drm:intel_dump_pipe_config [i915]] [PLANE:26:primary A] disabled, scaler_id = 0
[   37.357275] [drm:intel_dump_pipe_config [i915]] [PLANE:28:sprite A] disabled, scaler_id = 0
[   37.357340] [drm:intel_dump_pipe_config [i915]] [PLANE:30:sprite B] disabled, scaler_id = 0
[   37.357402] [drm:intel_dump_pipe_config [i915]] [PLANE:32:cursor A] disabled, scaler_id = 0
[   37.357466] [drm:intel_dump_pipe_config [i915]] [CRTC:43:pipe B][setup_hw_state]
[   37.357531] [drm:intel_dump_pipe_config [i915]] cpu_transcoder: B, pipe bpp: 0, dithering: 0
[   37.357592] [drm:intel_dump_pipe_config [i915]] audio: 0, infoframes: 0
[   37.357654] [drm:intel_dump_pipe_config [i915]] requested mode:
[   37.357671] [drm:drm_mode_debug_printmodeline [drm]] Modeline 0:"" 0 0 0 0 0 0 0 0 0 0 0x0 0x0
[   37.357733] [drm:intel_dump_pipe_config [i915]] adjusted mode:
[   37.357746] [drm:drm_mode_debug_printmodeline [drm]] Modeline 0:"" 0 0 0 0 0 0 0 0 0 0 0x0 0x0
[   37.357809] [drm:intel_dump_pipe_config [i915]] crtc timings: 0 0 0 0 0 0 0 0 0, type: 0x0 flags: 0x0
[   37.357874] [drm:intel_dump_pipe_config [i915]] port clock: 0, pipe src size: 0x0, pixel rate 0
[   37.357936] [drm:intel_dump_pipe_config [i915]] gmch pfit: control: 0x00000000, ratios: 0x00000000, lvds border: 0x00000000
[   37.357998] [drm:intel_dump_pipe_config [i915]] ips: 0, double wide: 0
[   37.358063] [drm:intel_dpll_dump_hw_state [i915]] dpll_hw_state: dpll: 0x0, dpll_md: 0x0, fp0: 0x0, fp1: 0x0
[   37.358124] [drm:intel_dump_pipe_config [i915]] planes on this crtc
[   37.358187] [drm:intel_dump_pipe_config [i915]] [PLANE:35:primary B] disabled, scaler_id = 0
[   37.358252] [drm:intel_dump_pipe_config [i915]] [PLANE:37:sprite C] disabled, scaler_id = 0
[   37.358314] [drm:intel_dump_pipe_config [i915]] [PLANE:39:sprite D] disabled, scaler_id = 0
[   37.358376] [drm:intel_dump_pipe_config [i915]] [PLANE:41:cursor B] disabled, scaler_id = 0
[   37.358444] [drm:vlv_wm_get_hw_state [i915]] Pipe A FIFO size: 256/128/127/63
[   37.358502] [drm:vlv_wm_get_hw_state [i915]] Initial watermarks: pipe A, plane=15, cursor=15, sprite0=15, sprite1=15
[   37.358560] [drm:vlv_wm_get_hw_state [i915]] Pipe B FIFO size: 256/128/127/63
[   37.358620] [drm:vlv_wm_get_hw_state [i915]] Initial watermarks: pipe B, plane=15, cursor=15, sprite0=15, sprite1=15
[   37.358677] [drm:vlv_wm_get_hw_state [i915]] Initial watermarks: SR plane=127, SR cursor=0 level=0 cxsr=0
[   37.358742] [drm:intel_power_well_disable [i915]] disabling dpio-common
[   37.360873] [drm:intel_power_well_disable [i915]] disabling dpio-tx-c-23
[   37.362651] [drm:intel_power_well_disable [i915]] disabling dpio-tx-c-01
[   37.364923] [drm:intel_power_well_disable [i915]] disabling dpio-tx-b-23
[   37.366309] [drm:intel_power_well_disable [i915]] disabling dpio-tx-b-01
[   37.368957] [drm:i9xx_get_initial_plane_config [i915]] pipe/plane A/0 with fb: size=800x600@32, offset=0, pitch 3200, size 0x1d4c00
[   37.369067] [drm:i915_gem_object_create_stolen_for_preallocated [i915]] creating preallocated stolen object: stolen_offset=0, gtt_offset=0, size=1d5000
[   37.369214] [drm:intel_alloc_initial_plane_obj.isra.73 [i915]] initial plane fb obj ffff880071d65e00
[   37.369373] [drm:intel_set_plane_visible [i915]] pipe A active planes 0x1
[   37.369486] [drm:i915_gem_init_ggtt [i915]] clearing unused GTT space: [1d7000, 80000000]
[   37.373961] [drm:i915_gem_init_ggtt [i915]] clearing unused GTT space: [1d5000, 1d6000]
[   37.374102] [drm:i915_gem_context_init [i915]] HW context support initialized
[   37.375682] [drm:intel_init_ring_buffer [i915]] render ring hws offset: 0x001d8000
[   37.375826] [drm:intel_engine_create_scratch [i915]] render ring pipe control offset: 0x7fffc000
[   37.376350] [drm:intel_init_ring_buffer [i915]] blitter ring hws offset: 0x001fb000
[   37.377233] [drm:intel_init_ring_buffer [i915]] bsd ring hws offset: 0x0021e000
[   37.377368] [drm:init_workarounds_ring [i915]] render ring: Number of context specific w/a: 0
[   37.377531] [drm:i915_gem_object_create_stolen_for_preallocated [i915]] creating preallocated stolen object: stolen_offset=3efa000, gtt_offset=ffffffff, size=6000
[   37.377653] [drm:intel_init_gt_powersave [i915]] PCBR: 0x7edfa001
[   37.377771] [drm:vlv_init_gpll_ref_freq [i915]] GPLL reference freq: 22222 kHz
[   37.377888] [drm:intel_init_gt_powersave [i915]] DDR speed: 1066 MHz
[   37.378006] [drm:intel_init_gt_powersave [i915]] max GPU freq: 667 MHz (213)
[   37.378126] [drm:intel_init_gt_powersave [i915]] RPe GPU freq: 400 MHz (201)
[   37.378244] [drm:intel_init_gt_powersave [i915]] RP1(Guar Freq) GPU freq: 311 MHz (197)
[   37.378361] [drm:intel_init_gt_powersave [i915]] min GPU freq: 200 MHz (192)
[   37.378492] [drm:intel_fbdev_init [i915]] found possible fb from plane A
[   37.378615] [drm:intel_fbdev_init [i915]] pipe B not active or no fb, skipping
[   37.378737] [drm:intel_fbdev_init [i915]] checking plane A for BIOS fb
[   37.378861] [drm:intel_fbdev_init [i915]] pipe A area: 800x1280, bpp: 32, size: 4096000
[   37.378983] [drm:intel_fbdev_init [i915]] fb not big enough for plane A (4096000 vs 1921024)
[   37.379104] [drm:intel_fbdev_init [i915]] BIOS fb not suitable for all pipes, not using
[   37.381673] [drm:intel_dp_connector_register [i915]] registering DPDDC-B bus for card0-DP-1
[   37.382981] [drm:intel_dp_connector_register [i915]] registering DPDDC-C bus for card0-DP-2
[   37.383283] [drm] Initialized i915 1.6.0 20170320 for 0000:00:02.0 on minor 0
[   37.383549] [drm:intel_opregion_register [i915]] 5 outputs detected
[   37.385791] ACPI: Video Device [GFX0] (multi-head: yes  rom: no  post: no)
[   37.387150] acpi device:1a: registered as cooling_device5
[   37.387317] input: Video Bus as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/LNXVIDEO:00/input/input11
[   37.387795] [drm] HDaudio controller not detected, using LPE audio instead

[   37.387946] [drm:drm_setup_crtcs [drm_kms_helper]] 
[   37.387956] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:56:DSI-1]
[   37.387965] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:56:DSI-1] status updated from unknown to connected
[   37.388067] [drm:intel_dsi_get_modes [i915]] 
[   37.388149] [drm:intel_dsi_mode_valid [i915]] 
[   37.388159] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:56:DSI-1] probed modes :
[   37.388181] [drm:drm_mode_debug_printmodeline [drm]] Modeline 57:"800x1280" 70 81250 800 840 844 884 1280 1290 1294 1306 0x8 0xa
[   37.388191] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:45:DP-1]
[   37.388269] [drm:intel_dp_detect [i915]] [CONNECTOR:45:DP-1]
[   37.388341] [drm:intel_power_well_enable [i915]] enabling dpio-tx-b-01
[   37.388420] [drm] Initialized i915 1.6.0 20170320 for 0000:00:02.0 on minor 0
[   37.390475] [drm:intel_power_well_enable [i915]] enabling dpio-tx-b-23
[   37.392648] [drm:intel_power_well_enable [i915]] enabling dpio-tx-c-01
[   37.394766] [drm:intel_power_well_enable [i915]] enabling dpio-tx-c-23
[   37.395993] [drm:intel_power_well_enable [i915]] enabling dpio-common
[   37.398480] [drm:intel_power_well_disable [i915]] disabling dpio-common
[   37.400603] [drm:intel_power_well_disable [i915]] disabling dpio-tx-c-23
[   37.402662] [drm:intel_power_well_disable [i915]] disabling dpio-tx-c-01
[   37.404778] [drm:intel_power_well_disable [i915]] disabling dpio-tx-b-23
[   37.406020] [drm:intel_power_well_disable [i915]] disabling dpio-tx-b-01
[   37.409361] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:45:DP-1] status updated from unknown to disconnected
[   37.409371] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:45:DP-1] disconnected
[   37.409381] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:49:HDMI-A-1]
[   37.409472] [drm:intel_hdmi_detect [i915]] [CONNECTOR:49:HDMI-A-1]
[   37.411614] [drm:gmbus_xfer [i915]] GMBUS [i915 gmbus dpb] NAK for addr: 0050 w(1)
[   37.411700] [drm:gmbus_xfer [i915]] GMBUS [i915 gmbus dpb] NAK on first message, retry
[   37.414000] [drm:gmbus_xfer [i915]] GMBUS [i915 gmbus dpb] NAK for addr: 0050 w(1)
[   37.414023] [drm:drm_do_probe_ddc_edid [drm]] drm: skipping non-existent adapter i915 gmbus dpb
[   37.416411] [drm:gmbus_xfer [i915]] GMBUS [i915 gmbus dpb] NAK for addr: 0040 w(1)
[   37.416499] [drm:gmbus_xfer [i915]] GMBUS [i915 gmbus dpb] NAK on first message, retry
[   37.418987] [drm:gmbus_xfer [i915]] GMBUS [i915 gmbus dpb] NAK for addr: 0040 w(1)
[   37.419002] [drm:drm_dp_dual_mode_detect [drm_kms_helper]] DP dual mode HDMI ID:  (err -6)
[   37.419012] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:49:HDMI-A-1] status updated from unknown to disconnected
[   37.419019] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:49:HDMI-A-1] disconnected
[   37.419029] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:52:DP-2]
[   37.419095] [drm:intel_dp_detect [i915]] [CONNECTOR:52:DP-2]
[   37.419158] [drm:intel_power_well_enable [i915]] enabling dpio-tx-b-01
[   37.421727] [drm:intel_power_well_enable [i915]] enabling dpio-tx-b-23
[   37.423068] [drm:intel_power_well_enable [i915]] enabling dpio-tx-c-01
[   37.425636] [drm:intel_power_well_enable [i915]] enabling dpio-tx-c-23
[   37.427969] [drm:intel_power_well_enable [i915]] enabling dpio-common
[   37.430066] [drm:intel_power_well_disable [i915]] disabling dpio-common
[   37.432693] [drm:intel_power_well_disable [i915]] disabling dpio-tx-c-23
[   37.435316] [drm:intel_power_well_disable [i915]] disabling dpio-tx-c-01
[   37.437925] [drm:intel_power_well_disable [i915]] disabling dpio-tx-b-23
[   37.440279] [drm:intel_power_well_disable [i915]] disabling dpio-tx-b-01
[   37.443079] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:52:DP-2] status updated from unknown to disconnected
[   37.443097] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:52:DP-2] disconnected
[   37.443116] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:54:HDMI-A-2]
[   37.443278] [drm:intel_hdmi_detect [i915]] [CONNECTOR:54:HDMI-A-2]
[   37.485029] i915 0000:00:02.0: HDMI-A-2: EDID is invalid:
[   37.485045] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   37.485051] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   37.485056] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   37.485061] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   37.485066] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   37.485071] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   37.485076] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   37.485081] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   37.491244] [drm:drm_dp_dual_mode_detect [drm_kms_helper]] DP dual mode HDMI ID: \0\0\0\0\0\0\0\0\0\0\0\0\0\0\0\0 (err 0)
[   37.494873] [drm:drm_dp_dual_mode_detect [drm_kms_helper]] DP dual mode adaptor ID: 00 (err 0)
[   37.495115] [drm:intel_hdmi_set_edid [i915]] DP dual mode adaptor (type 1 DVI) detected (max TMDS clock: 165000 kHz)
[   37.495145] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:54:HDMI-A-2] status updated from unknown to disconnected
[   37.495167] [drm:drm_helper_probe_single_connector_modes [drm_kms_helper]] [CONNECTOR:54:HDMI-A-2] disconnected
[   37.495195] [drm:drm_setup_crtcs [drm_kms_helper]] connector 56 enabled? yes
[   37.495213] [drm:drm_setup_crtcs [drm_kms_helper]] connector 45 enabled? no
[   37.495231] [drm:drm_setup_crtcs [drm_kms_helper]] connector 49 enabled? no
[   37.495249] [drm:drm_setup_crtcs [drm_kms_helper]] connector 52 enabled? no
[   37.495267] [drm:drm_setup_crtcs [drm_kms_helper]] connector 54 enabled? no
[   37.495484] [drm:intel_fb_initial_config [i915]] Not using firmware configuration
[   37.495508] [drm:drm_setup_crtcs [drm_kms_helper]] looking for cmdline mode on connector 56
[   37.495527] [drm:drm_setup_crtcs [drm_kms_helper]] looking for preferred mode on connector 56 0
[   37.495545] [drm:drm_setup_crtcs [drm_kms_helper]] found mode 800x1280
[   37.495564] [drm:drm_setup_crtcs [drm_kms_helper]] picking CRTCs for 8192x8192 config
[   37.495593] [drm:drm_setup_crtcs [drm_kms_helper]] desired mode 800x1280 set on crtc 34 (0,0)
[   37.495818] [drm:intelfb_create [i915]] no BIOS fb, allocating a new one
[   37.498209] [drm:intelfb_create [i915]] allocated 800x1280 fb: 0x00240000
[   37.498900] fbcon: inteldrmfb (fb0) is primary device
[   37.499664] [drm:intel_atomic_check [i915]] [CONNECTOR:56:DSI-1] checking for sink bpp constrains
[   37.499886] [drm:intel_atomic_check [i915]] clamping display bpp (was 30) to default limit of 24
[   37.500111] [drm:intel_dsi_compute_config [i915]] 
[   37.500345] [drm:intel_compute_dsi_pll [i915]] dsi pll div 00000157, ctrl 80080100
[   37.500576] [drm:intel_atomic_check [i915]] hw max bpp: 30, pipe bpp: 24, dithering: 0
[   37.500803] [drm:intel_dump_pipe_config [i915]] [CRTC:34:pipe A][modeset]
[   37.501031] [drm:intel_dump_pipe_config [i915]] cpu_transcoder: A, pipe bpp: 24, dithering: 0
[   37.501253] [drm:intel_dump_pipe_config [i915]] audio: 0, infoframes: 0
[   37.501476] [drm:intel_dump_pipe_config [i915]] requested mode:
[   37.501530] [drm:drm_mode_debug_printmodeline [drm]] Modeline 0:"800x1280" 70 81250 800 840 844 884 1280 1290 1294 1306 0x8 0xa
[   37.501752] [drm:intel_dump_pipe_config [i915]] adjusted mode:
[   37.501800] [drm:drm_mode_debug_printmodeline [drm]] Modeline 0:"800x1280" 0 81250 800 840 844 884 1280 1290 1294 1306 0x8 0x0
[   37.502028] [drm:intel_dump_pipe_config [i915]] crtc timings: 81250 800 840 844 884 1280 1290 1294 1306, type: 0x8 flags: 0x0
[   37.502250] [drm:intel_dump_pipe_config [i915]] port clock: 81250, pipe src size: 800x1280, pixel rate 81250
[   37.502475] [drm:intel_dump_pipe_config [i915]] gmch pfit: control: 0x00000000, ratios: 0x00000000, lvds border: 0x00000000
[   37.502696] [drm:intel_dump_pipe_config [i915]] ips: 0, double wide: 0
[   37.502957] [drm:intel_dpll_dump_hw_state [i915]] dpll_hw_state: dpll: 0x30002000, dpll_md: 0x3, fp0: 0x0, fp1: 0x0
[   37.503173] [drm:intel_dump_pipe_config [i915]] planes on this crtc
[   37.503402] [drm:intel_dump_pipe_config [i915]] [PLANE:26:primary A] FB:61, fb = 800x600 format = XR24 little-endian (0x34325258)
[   37.503625] [drm:intel_dump_pipe_config [i915]] [PLANE:28:sprite A] disabled, scaler_id = 0
[   37.503850] [drm:intel_dump_pipe_config [i915]] [PLANE:30:sprite B] disabled, scaler_id = 0
[   37.504075] [drm:intel_dump_pipe_config [i915]] [PLANE:32:cursor A] disabled, scaler_id = 0
[   37.504316] [drm:intel_atomic_check [i915]] New cdclk calculated to be logical 266667 kHz, actual 266667 kHz
[   37.504543] [drm:vlv_compute_pipe_wm [i915]] primary A wms: [0]=50,[1]=0,[2]=0
[   37.504739] [drm:_intel_set_memory_cxsr [i915]] memory self-refresh is disabled (was disabled)
[   37.504809] [drm:intel_dsi_disable [i915]] 
[   37.533471] [drm:intel_disable_pipe [i915]] disabling pipe A
[   37.546354] [drm:i9xx_crtc_disable [i915]] disabling pfit, current: 0x80000000
[   37.546570] [drm:intel_dsi_post_disable [i915]] 
[   37.552231] [drm:intel_dsi_vbt_exec_sequence [i915]] Starting MIPI sequence 4 - MIPI_SEQ_DISPLAY_OFF
[   37.552442] [drm:mipi_exec_send_packet [i915]] 
[   37.552664] [drm:mipi_exec_delay [i915]] 
[   37.593438] [drm:mipi_exec_send_packet [i915]] 
[   37.593663] [drm:intel_dsi_post_disable [i915]] 
[   37.607650] [drm:intel_disable_dsi_pll [i915]] 
[   37.607883] [drm:intel_dsi_vbt_exec_sequence [i915]] Starting MIPI sequence 5 - MIPI_SEQ_ASSERT_RESET
[   37.608093] [drm:mipi_exec_delay [i915]] 
[   37.708788] [drm:mipi_exec_gpio [i915]] 
[   38.292957] [drm:intel_set_cdclk [i915]] Changing CDCLK to 266667 kHz, VCO 1600000 kHz, ref 0 kHz
[   38.295359] [drm:intel_update_cdclk [i915]] Current CD clock rate: 266667 kHz, VCO: 1600000 kHz, ref: 0 kHz
[   38.295538] [drm:intel_atomic_commit_tail [i915]] [ENCODER:44:DP B]
[   38.295711] [drm:intel_atomic_commit_tail [i915]] [ENCODER:48:HDMI B]
[   38.295884] [drm:intel_atomic_commit_tail [i915]] [ENCODER:51:DP C]
[   38.296088] [drm:intel_atomic_commit_tail [i915]] [ENCODER:53:HDMI C]
[   38.296261] [drm:intel_atomic_commit_tail [i915]] [ENCODER:55:DSI A]
[   38.296451] [drm:intel_dsi_pre_enable [i915]] 
[   38.296619] [drm:intel_disable_dsi_pll [i915]] 
[   38.296794] [drm:intel_enable_dsi_pll [i915]] 
[   38.299240] [drm:intel_enable_dsi_pll [i915]] DSI PLL locked
[   38.299451] [drm:intel_dsi_pre_enable [i915]] pipe A
[   38.356573] [drm:intel_dsi_pre_enable [i915]] 
[   38.369310] [drm:intel_dsi_vbt_exec_sequence [i915]] Starting MIPI sequence 2 - MIPI_SEQ_INIT_OTP
[   38.369598] [drm:mipi_exec_delay [i915]] 
[   38.410282] [drm:mipi_exec_gpio [i915]] 
[   38.410506] [drm:mipi_exec_delay [i915]] 
[   38.416172] [drm:mipi_exec_gpio [i915]] 
[   38.416396] [drm:mipi_exec_delay [i915]] 
[   38.422093] [drm:mipi_exec_gpio [i915]] 
[   38.422316] [drm:mipi_exec_delay [i915]] 
[   38.443013] [drm:mipi_exec_send_packet [i915]] 
[   38.445724] [drm:mipi_exec_send_packet [i915]] 
[   38.448399] [drm:mipi_exec_send_packet [i915]] 
[   38.451106] [drm:mipi_exec_send_packet [i915]] 
[   38.451330] [drm:mipi_exec_send_packet [i915]] 
[   38.451543] [drm:mipi_exec_send_packet [i915]] 
[   38.451756] [drm:mipi_exec_send_packet [i915]] 
[   38.451969] [drm:mipi_exec_send_packet [i915]] 
[   38.452182] [drm:mipi_exec_send_packet [i915]] 
[   38.452395] [drm:mipi_exec_send_packet [i915]] 
[   38.452608] [drm:mipi_exec_send_packet [i915]] 
[   38.452904] [drm:mipi_exec_send_packet [i915]] 
[   38.455566] [drm:mipi_exec_send_packet [i915]] 
[   38.455790] [drm:mipi_exec_send_packet [i915]] 
[   38.458487] [drm:mipi_exec_send_packet [i915]] 
[   38.458711] [drm:mipi_exec_send_packet [i915]] 
[   38.458925] [drm:mipi_exec_send_packet [i915]] 
[   38.459138] [drm:mipi_exec_send_packet [i915]] 
[   38.461895] [drm:mipi_exec_send_packet [i915]] 
[   38.464600] [drm:mipi_exec_send_packet [i915]] 
[   38.467306] [drm:mipi_exec_send_packet [i915]] 
[   38.470012] [drm:mipi_exec_send_packet [i915]] 
[   38.472723] [drm:mipi_exec_send_packet [i915]] 
[   38.475459] [drm:mipi_exec_send_packet [i915]] 
[   38.478165] [drm:mipi_exec_send_packet [i915]] 
[   38.480898] [drm:mipi_exec_send_packet [i915]] 
[   38.481123] [drm:mipi_exec_send_packet [i915]] 
[   38.481336] [drm:mipi_exec_send_packet [i915]] 
[   38.481549] [drm:mipi_exec_send_packet [i915]] 
[   38.484245] [drm:mipi_exec_send_packet [i915]] 
[   38.486945] [drm:mipi_exec_send_packet [i915]] 
[   38.489642] [drm:mipi_exec_send_packet [i915]] 
[   38.492334] [drm:mipi_exec_send_packet [i915]] 
[   38.495038] [drm:mipi_exec_send_packet [i915]] 
[   38.495262] [drm:mipi_exec_send_packet [i915]] 
[   38.497956] [drm:mipi_exec_send_packet [i915]] 
[   38.500656] [drm:mipi_exec_send_packet [i915]] 
[   38.500880] [drm:mipi_exec_send_packet [i915]] 
[   38.503551] [drm:mipi_exec_send_packet [i915]] 
[   38.503776] [drm:mipi_exec_send_packet [i915]] 
[   38.506475] [drm:mipi_exec_send_packet [i915]] 
[   38.509168] [drm:mipi_exec_send_packet [i915]] 
[   38.509394] [drm:mipi_exec_send_packet [i915]] 
[   38.512130] [drm:mipi_exec_send_packet [i915]] 
[   38.512354] [drm:mipi_exec_send_packet [i915]] 
[   38.515038] [drm:mipi_exec_send_packet [i915]] 
[   38.517740] [drm:mipi_exec_send_packet [i915]] 
[   38.517965] [drm:mipi_exec_send_packet [i915]] 
[   38.520636] [drm:mipi_exec_send_packet [i915]] 
[   38.520860] [drm:mipi_exec_send_packet [i915]] 
[   38.523555] [drm:mipi_exec_send_packet [i915]] 
[   38.526256] [drm:mipi_exec_send_packet [i915]] 
[   38.528946] [drm:mipi_exec_send_packet [i915]] 
[   38.531650] [drm:mipi_exec_send_packet [i915]] 
[   38.534354] [drm:mipi_exec_send_packet [i915]] 
[   38.537058] [drm:mipi_exec_send_packet [i915]] 
[   38.539736] [drm:mipi_exec_send_packet [i915]] 
[   38.542401] [drm:mipi_exec_send_packet [i915]] 
[   38.545106] [drm:mipi_exec_send_packet [i915]] 
[   38.547829] [drm:mipi_exec_send_packet [i915]] 
[   38.550533] [drm:mipi_exec_send_packet [i915]] 
[   38.553238] [drm:mipi_exec_send_packet [i915]] 
[   38.555932] [drm:mipi_exec_send_packet [i915]] 
[   38.558703] [drm:mipi_exec_send_packet [i915]] 
[   38.561379] [drm:mipi_exec_send_packet [i915]] 
[   38.564082] [drm:mipi_exec_send_packet [i915]] 
[   38.566798] [drm:mipi_exec_send_packet [i915]] 
[   38.569495] [drm:mipi_exec_send_packet [i915]] 
[   38.572190] [drm:mipi_exec_send_packet [i915]] 
[   38.574913] [drm:mipi_exec_send_packet [i915]] 
[   38.577620] [drm:mipi_exec_send_packet [i915]] 
[   38.580324] [drm:mipi_exec_send_packet [i915]] 
[   38.583024] [drm:mipi_exec_send_packet [i915]] 
[   38.585718] [drm:mipi_exec_send_packet [i915]] 
[   38.588397] [drm:mipi_exec_send_packet [i915]] 
[   38.591098] [drm:mipi_exec_send_packet [i915]] 
[   38.593791] [drm:mipi_exec_send_packet [i915]] 
[   38.596498] [drm:mipi_exec_send_packet [i915]] 
[   38.599196] [drm:mipi_exec_send_packet [i915]] 
[   38.601961] [drm:mipi_exec_send_packet [i915]] 
[   38.604665] [drm:mipi_exec_send_packet [i915]] 
[   38.607365] [drm:mipi_exec_send_packet [i915]] 
[   38.610071] [drm:mipi_exec_send_packet [i915]] 
[   38.612744] [drm:mipi_exec_send_packet [i915]] 
[   38.615484] [drm:mipi_exec_send_packet [i915]] 
[   38.618188] [drm:mipi_exec_send_packet [i915]] 
[   38.620924] [drm:mipi_exec_send_packet [i915]] 
[   38.623650] [drm:mipi_exec_send_packet [i915]] 
[   38.626349] [drm:mipi_exec_send_packet [i915]] 
[   38.629044] [drm:mipi_exec_send_packet [i915]] 
[   38.631764] [drm:mipi_exec_send_packet [i915]] 
[   38.634439] [drm:mipi_exec_send_packet [i915]] 
[   38.637145] [drm:mipi_exec_send_packet [i915]] 
[   38.639821] [drm:mipi_exec_send_packet [i915]] 
[   38.642489] [drm:mipi_exec_send_packet [i915]] 
[   38.645182] [drm:mipi_exec_send_packet [i915]] 
[   38.647927] [drm:mipi_exec_send_packet [i915]] 
[   38.648152] [drm:mipi_exec_send_packet [i915]] 
[   38.650910] [drm:mipi_exec_send_packet [i915]] 
[   38.653619] [drm:mipi_exec_send_packet [i915]] 
[   38.656288] [drm:mipi_exec_send_packet [i915]] 
[   38.658979] [drm:mipi_exec_send_packet [i915]] 
[   38.661676] [drm:mipi_exec_send_packet [i915]] 
[   38.664354] [drm:mipi_exec_send_packet [i915]] 
[   38.667060] [drm:mipi_exec_send_packet [i915]] 
[   38.669754] [drm:mipi_exec_send_packet [i915]] 
[   38.672419] [drm:mipi_exec_send_packet [i915]] 
[   38.675125] [drm:mipi_exec_send_packet [i915]] 
[   38.675349] [drm:mipi_exec_send_packet [i915]] 
[   38.675563] [drm:mipi_exec_send_packet [i915]] 
[   38.678257] [drm:mipi_exec_send_packet [i915]] 
[   38.680961] [drm:mipi_exec_send_packet [i915]] 
[   38.683666] [drm:mipi_exec_send_packet [i915]] 
[   38.686369] [drm:mipi_exec_send_packet [i915]] 
[   38.689060] [drm:mipi_exec_send_packet [i915]] 
[   38.691760] [drm:mipi_exec_send_packet [i915]] 
[   38.694436] [drm:mipi_exec_send_packet [i915]] 
[   38.697148] [drm:mipi_exec_send_packet [i915]] 
[   38.697372] [drm:mipi_exec_send_packet [i915]] 
[   38.697585] [drm:mipi_exec_send_packet [i915]] 
[   38.697798] [drm:mipi_exec_send_packet [i915]] 
[   38.698011] [drm:mipi_exec_send_packet [i915]] 
[   38.698224] [drm:mipi_exec_send_packet [i915]] 
[   38.698437] [drm:mipi_exec_send_packet [i915]] 
[   38.698649] [drm:mipi_exec_send_packet [i915]] 
[   38.698862] [drm:mipi_exec_send_packet [i915]] 
[   38.701556] [drm:mipi_exec_send_packet [i915]] 
[   38.704232] [drm:mipi_exec_send_packet [i915]] 
[   38.706938] [drm:mipi_exec_send_packet [i915]] 
[   38.709640] [drm:mipi_exec_send_packet [i915]] 
[   38.712335] [drm:mipi_exec_send_packet [i915]] 
[   38.715040] [drm:mipi_exec_send_packet [i915]] 
[   38.715265] [drm:mipi_exec_send_packet [i915]] 
[   38.715478] [drm:mipi_exec_send_packet [i915]] 
[   38.715691] [drm:mipi_exec_send_packet [i915]] 
[   38.715904] [drm:mipi_exec_send_packet [i915]] 
[   38.716236] [drm:mipi_exec_send_packet [i915]] 
[   38.716450] [drm:mipi_exec_send_packet [i915]] 
[   38.716663] [drm:mipi_exec_send_packet [i915]] 
[   38.716876] [drm:mipi_exec_send_packet [i915]] 
[   38.717088] [drm:mipi_exec_send_packet [i915]] 
[   38.717302] [drm:mipi_exec_send_packet [i915]] 
[   38.717515] [drm:mipi_exec_delay [i915]] 
[   38.838216] [drm:mipi_exec_send_packet [i915]] 
[   38.838441] [drm:mipi_exec_delay [i915]] 
[   38.980041] [drm:intel_enable_pipe [i915]] enabling pipe A
[   38.980282] [drm:intel_dsi_enable_nop [i915]] 
[   38.994914] [drm:_intel_set_memory_cxsr [i915]] memory self-refresh is enabled (was disabled)
[   38.995146] [drm:verify_connector_state.isra.46 [i915]] [CONNECTOR:56:DSI-1]
[   38.995357] [drm:intel_dsi_get_hw_state [i915]] 
[   38.995594] [drm:intel_atomic_commit_tail [i915]] [CRTC:34:pipe A]
[   38.995818] [drm:intel_dsi_get_hw_state [i915]] 
[   38.996031] [drm:intel_dsi_get_config [i915]] 
[   38.996325] [drm:intel_dsi_get_pclk [i915]] 
[   38.996663] Console: switching to colour frame buffer device 100x80
[   39.022652] i915 0000:00:02.0: fb0: inteldrmfb frame buffer device
[   39.519917] [drm:intel_print_rc6_info [i915]] Enabling RC6 states: RC6 on
[   39.520036] [drm:intel_enable_gt_powersave [i915]] GPLL enabled? yes
[   39.520139] [drm:intel_enable_gt_powersave [i915]] GPU status: 0x0000c590