[    0.000000] Linux version 4.12.0-W4+ (erhoof@erhoof_tablet) (gcc version 7.1.1 20170630 (GCC) ) #1 SMP PREEMPT Wed Jul 12 15:00:51 MSK 2017
[    0.000000] Command line: BOOT_IMAGE=/vmlinuz-next root=/dev/mmcblk1p2 rw intel_idle.max_cstate=1 fbcon=rotate:1 i915.modeset=1 i915.fastboot=1 enable_fbc=1 enable_psr=0 tsc=reliable clocksource=tsc force_tsc_stable=1 add_efi_memmap quiet
[    0.000000] x86/fpu: x87 FPU will use FXSAVE
[    0.000000] e820: BIOS-provided physical RAM map:
[    0.000000] BIOS-e820: [mem 0x0000000000000000-0x000000000008efff] usable
[    0.000000] BIOS-e820: [mem 0x000000000008f000-0x000000000008ffff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000000090000-0x000000000009dfff] usable
[    0.000000] BIOS-e820: [mem 0x000000000009e000-0x000000000009ffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000100000-0x000000001fffffff] usable
[    0.000000] BIOS-e820: [mem 0x0000000020000000-0x00000000200fffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000020100000-0x00000000782bafff] usable
[    0.000000] BIOS-e820: [mem 0x00000000782bb000-0x00000000784bafff] type 20
[    0.000000] BIOS-e820: [mem 0x00000000784bb000-0x0000000078bbafff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000078bbb000-0x0000000078cbafff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000078cbb000-0x0000000078cfafff] ACPI data
[    0.000000] BIOS-e820: [mem 0x0000000078cfb000-0x000000007951bfff] usable
[    0.000000] BIOS-e820: [mem 0x000000007951c000-0x000000007951cfff] reserved
[    0.000000] BIOS-e820: [mem 0x000000007951d000-0x0000000079526fff] usable
[    0.000000] BIOS-e820: [mem 0x0000000079527000-0x0000000079e26fff] ACPI NVS
[    0.000000] BIOS-e820: [mem 0x0000000079e27000-0x0000000079ffffff] usable
[    0.000000] BIOS-e820: [mem 0x00000000e00f8000-0x00000000e00f8fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed01000-0x00000000fed01fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000ffd00000-0x00000000ffffffff] reserved
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] efi: EFI v2.31 by INSYDE Corp.
[    0.000000] efi:  ACPI 2.0=0x78cfa014  ESRT=0x78559e10  SMBIOS=0x78bba000 
[    0.000000] SMBIOS 2.7 present.
[    0.000000] DMI: Acer TP-W4-820-Z3742G06AII/Cheetah3, BIOS V1.16 03/13/2014
[    0.000000] e820: update [mem 0x00000000-0x00000fff] usable ==> reserved
[    0.000000] e820: remove [mem 0x000a0000-0x000fffff] usable
[    0.000000] e820: last_pfn = 0x7a000 max_arch_pfn = 0x400000000
[    0.000000] MTRR default type: uncachable
[    0.000000] MTRR fixed ranges enabled:
[    0.000000]   00000-9FFFF write-back
[    0.000000]   A0000-FFFFF write-protect
[    0.000000] MTRR variable ranges enabled:
[    0.000000]   0 base 0FFD00000 mask FFFC00000 write-protect
[    0.000000]   1 base 000000000 mask FC0000000 write-back
[    0.000000]   2 base 040000000 mask FE0000000 write-back
[    0.000000]   3 base 060000000 mask FF0000000 write-back
[    0.000000]   4 base 070000000 mask FF8000000 write-back
[    0.000000]   5 base 078000000 mask FFC000000 write-back
[    0.000000]   6 base 07B000000 mask FFF000000 uncachable
[    0.000000]   7 base 07AE00000 mask FFFE00000 uncachable
[    0.000000] x86/PAT: Configuration [0-7]: WB  WC  UC- UC  WB  WC  UC- WT  
[    0.000000] esrt: Reserving ESRT space from 0x0000000078559e10 to 0x0000000078559e48.
[    0.000000] Scanning 1 areas for low memory corruption
[    0.000000] Base memory trampoline at [ffff880000098000] 98000 size 24576
[    0.000000] BRK [0x02f69000, 0x02f69fff] PGTABLE
[    0.000000] BRK [0x02f6a000, 0x02f6afff] PGTABLE
[    0.000000] BRK [0x02f6b000, 0x02f6bfff] PGTABLE
[    0.000000] BRK [0x02f6c000, 0x02f6cfff] PGTABLE
[    0.000000] BRK [0x02f6d000, 0x02f6dfff] PGTABLE
[    0.000000] BRK [0x02f6e000, 0x02f6efff] PGTABLE
[    0.000000] Secure boot could not be determined
[    0.000000] RAMDISK: [mem 0x37535000-0x37a91fff]
[    0.000000] ACPI: Early table checksum verification disabled
[    0.000000] ACPI: RSDP 0x0000000078CFA014 000024 (v02 ACRSYS)
[    0.000000] ACPI: XSDT 0x0000000078CD4188 0000DC (v01 ACRSYS ACRPRDCT 00000003      01000013)
[    0.000000] ACPI: FACP 0x0000000078CF0000 00010C (v05 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: DSDT 0x0000000078CE0000 00B10F (v02 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: UEFI 0x0000000078CF9000 000236 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: TCPA 0x0000000078CF8000 000032 (v02 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: MSDM 0x0000000078CF7000 000055 (v03 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: UEFI 0x0000000078CF6000 000042 (v01 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CF2000 00305D (v01 ACRSYS ACRPRDCT 00001000 1025 00040000)
[    0.000000] ACPI: DBG2 0x0000000078CF1000 000072 (v00 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: HPET 0x0000000078CEF000 000038 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: LPIT 0x0000000078CEE000 000104 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: APIC 0x0000000078CED000 00006C (v03 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: MCFG 0x0000000078CEC000 00003C (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDF000 0005F9 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDD000 001C9F (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDC000 000058 (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDB000 0000FF (v01 ACRSYS ACRPRDCT 00000003 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CDA000 00043A (v01 ACRSYS ACRPRDCT 00001000 1025 00040000)
[    0.000000] ACPI: TPM2 0x0000000078CD9000 000034 (v03 ACRSYS ACRPRDCT 00000000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD8000 000763 (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD7000 000290 (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: SSDT 0x0000000078CD6000 00017A (v01 ACRSYS ACRPRDCT 00003000 1025 00040000)
[    0.000000] ACPI: FPDT 0x0000000078CD5000 000044 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: CSRT 0x0000000078CD3000 00014C (v00 ACRSYS ACRPRDCT 00000005 1025 00040000)
[    0.000000] ACPI: BGRT 0x0000000078CD2000 000038 (v01 ACRSYS ACRPRDCT 00000001 1025 00040000)
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] No NUMA configuration found
[    0.000000] Faking a node at [mem 0x0000000000000000-0x0000000079ffffff]
[    0.000000] NODE_DATA(0) allocated [mem 0x77fe7000-0x77febfff]
[    0.000000] Zone ranges:
[    0.000000]   DMA      [mem 0x0000000000001000-0x0000000000ffffff]
[    0.000000]   DMA32    [mem 0x0000000001000000-0x0000000079ffffff]
[    0.000000]   Normal   empty
[    0.000000]   Device   empty
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000000001000-0x000000000008efff]
[    0.000000]   node   0: [mem 0x0000000000090000-0x000000000009dfff]
[    0.000000]   node   0: [mem 0x0000000000100000-0x000000001fffffff]
[    0.000000]   node   0: [mem 0x0000000020100000-0x00000000782bafff]
[    0.000000]   node   0: [mem 0x0000000078cfb000-0x000000007951bfff]
[    0.000000]   node   0: [mem 0x000000007951d000-0x0000000079526fff]
[    0.000000]   node   0: [mem 0x0000000079e27000-0x0000000079ffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000000001000-0x0000000079ffffff]
[    0.000000] On node 0 totalpages: 494427
[    0.000000]   DMA zone: 64 pages used for memmap
[    0.000000]   DMA zone: 22 pages reserved
[    0.000000]   DMA zone: 3996 pages, LIFO batch:0
[    0.000000]   DMA32 zone: 7744 pages used for memmap
[    0.000000]   DMA32 zone: 490431 pages, LIFO batch:31
[    0.000000] x86/hpet: Will disable the HPET for this platform because it's not reliable
[    0.000000] Reserving Intel graphics memory at 0x000000007af00000-0x000000007eefffff
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] IOAPIC[0]: apic_id 2, version 32, address 0xfec00000, GSI 0-86
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.000000] Using ACPI (MADT) for SMP configuration information
[    0.000000] ACPI: HPET id: 0x8086a201 base: 0xfed00000
[    0.000000] smpboot: Allowing 4 CPUs, 0 hotplug CPUs
[    0.000000] PM: Registered nosave memory: [mem 0x00000000-0x00000fff]
[    0.000000] PM: Registered nosave memory: [mem 0x0008f000-0x0008ffff]
[    0.000000] PM: Registered nosave memory: [mem 0x0009e000-0x0009ffff]
[    0.000000] PM: Registered nosave memory: [mem 0x000a0000-0x000fffff]
[    0.000000] PM: Registered nosave memory: [mem 0x20000000-0x200fffff]
[    0.000000] PM: Registered nosave memory: [mem 0x782bb000-0x784bafff]
[    0.000000] PM: Registered nosave memory: [mem 0x784bb000-0x78bbafff]
[    0.000000] PM: Registered nosave memory: [mem 0x78bbb000-0x78cbafff]
[    0.000000] PM: Registered nosave memory: [mem 0x78cbb000-0x78cfafff]
[    0.000000] PM: Registered nosave memory: [mem 0x7951c000-0x7951cfff]
[    0.000000] PM: Registered nosave memory: [mem 0x79527000-0x79e26fff]
[    0.000000] e820: [mem 0x7ef00000-0xe00f7fff] available for PCI devices
[    0.000000] Booting paravirtualized kernel on bare hardware
[    0.000000] clocksource: refined-jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 6370452778343963 ns
[    0.000000] setup_percpu: NR_CPUS:128 nr_cpumask_bits:128 nr_cpu_ids:4 nr_node_ids:1
[    0.000000] percpu: Embedded 35 pages/cpu @ffff880076a00000 s105880 r8192 d29288 u524288
[    0.000000] pcpu-alloc: s105880 r8192 d29288 u524288 alloc=1*2097152
[    0.000000] pcpu-alloc: [0] 0 1 2 3 
[    0.000000] Built 1 zonelists in Node order, mobility grouping on.  Total pages: 486597
[    0.000000] Policy zone: DMA32
[    0.000000] Kernel command line: BOOT_IMAGE=/vmlinuz-next root=/dev/mmcblk1p2 rw intel_idle.max_cstate=1 fbcon=rotate:1 i915.modeset=1 i915.fastboot=1 enable_fbc=1 enable_psr=0 tsc=reliable clocksource=tsc force_tsc_stable=1 add_efi_memmap quiet
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] Calgary: detecting Calgary via BIOS EBDA area
[    0.000000] Calgary: Unable to locate Rio Grande table in EBDA - bailing!
[    0.000000] Memory: 1893144K/1977708K available (7322K kernel code, 1134K rwdata, 2280K rodata, 1356K init, 908K bss, 84564K reserved, 0K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 29780 entries in 117 pages
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000] 	RCU restricting CPUs from NR_CPUS=128 to nr_cpu_ids=4.
[    0.000000] RCU: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=4
[    0.000000] NR_IRQS:8448 nr_irqs:1024 0
[    0.000000] Console: colour dummy device 80x25
[    0.000000] console [tty0] enabled
[    0.000000] tsc: Detected 1333.000 MHz processor
[    0.000020] Calibrating delay loop (skipped), value calculated using timer frequency.. 2667.08 BogoMIPS (lpj=4443333)
[    0.000028] pid_max: default: 32768 minimum: 301
[    0.000060] ACPI: Core revision 20170303
[    0.003333] ACPI: 10 ACPI AML tables successfully acquired and loaded
[    0.003333] Security Framework initialized
[    0.003333] Yama: becoming mindful.
[    0.003333] Dentry cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.003333] Inode-cache hash table entries: 131072 (order: 8, 1048576 bytes)
[    0.003333] Mount-cache hash table entries: 4096 (order: 3, 32768 bytes)
[    0.003333] Mountpoint-cache hash table entries: 4096 (order: 3, 32768 bytes)
[    0.003333] CPU: Physical Processor ID: 0
[    0.003333] CPU: Processor Core ID: 0
[    0.003333] ENERGY_PERF_BIAS: Set to 'normal', was 'performance'
[    0.003333] ENERGY_PERF_BIAS: View and update with x86_energy_perf_policy(8)
[    0.003333] mce: CPU supports 6 MCE banks
[    0.003333] CPU0: Thermal monitoring enabled (TM1)
[    0.003333] process: using mwait in idle threads
[    0.003333] Last level iTLB entries: 4KB 48, 2MB 0, 4MB 0
[    0.003333] Last level dTLB entries: 4KB 128, 2MB 16, 4MB 16, 1GB 0
[    0.003333] Freeing SMP alternatives memory: 24K
[    0.003333] smpboot: Max logical packages: 1
[    0.003333] TSC deadline timer enabled
[    0.003333] smpboot: CPU0: Intel(R) Atom(TM) CPU  Z3740  @ 1.33GHz (family: 0x6, model: 0x37, stepping: 0x3)
[    0.013358] Performance Events: PEBS fmt2+, 8-deep LBR, Silvermont events, 8-deep LBR, full-width counters, Intel PMU driver.
[    0.013386] ... version:                3
[    0.013388] ... bit width:              40
[    0.013389] ... generic registers:      2
[    0.013391] ... value mask:             000000ffffffffff
[    0.013393] ... max period:             0000007fffffffff
[    0.013395] ... fixed-purpose events:   3
[    0.013397] ... event mask:             0000000700000003
[    0.033634] NMI watchdog: enabled on all CPUs, permanently consumes one hw-PMU counter.
[    0.040012] smp: Bringing up secondary CPUs ...
[    0.066712] x86: Booting SMP configuration:
[    0.066716] .... node  #0, CPUs:      #1 #2 #3
[    0.370151] smp: Brought up 1 node, 4 CPUs
[    0.370151] smpboot: Total of 4 processors activated (10677.65 BogoMIPS)
[    0.370826] sched_clock: Marking stable (369999963, 0)->(405379340, -35379377)
[    0.371546] devtmpfs: initialized
[    0.371690] x86/mm: Memory block size: 128MB
[    0.381679] PM: Registering ACPI NVS region [mem 0x0008f000-0x0008ffff] (4096 bytes)
[    0.381683] PM: Registering ACPI NVS region [mem 0x78bbb000-0x78cbafff] (1048576 bytes)
[    0.381729] PM: Registering ACPI NVS region [mem 0x79527000-0x79e26fff] (9437184 bytes)
[    0.382251] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 6370867519511994 ns
[    0.382273] futex hash table entries: 1024 (order: 4, 65536 bytes)
[    0.382431] pinctrl core: initialized pinctrl subsystem
[    0.382504] RTC time: 21:43:35, date: 07/13/17
[    0.382779] NET: Registered protocol family 16
[    0.386489] cpuidle: using governor ladder
[    0.386598] cpuidle: using governor menu
[    0.386603] PCCT header not found.
[    0.386727] ACPI: bus type PCI registered
[    0.386731] acpiphp: ACPI Hot Plug PCI Controller Driver version: 0.5
[    0.386892] PCI: MMCONFIG for domain 0000 [bus 00-3f] at [mem 0xe0000000-0xe3ffffff] (base 0xe0000000)
[    0.386929] PCI: not using MMCONFIG
[    0.386933] PCI: Using configuration type 1 for base access
[    0.389688] HugeTLB registered 2 MB page size, pre-allocated 0 pages
[    0.390435] ACPI: Added _OSI(Module Device)
[    0.390438] ACPI: Added _OSI(Processor Device)
[    0.390440] ACPI: Added _OSI(3.0 _SCP Extensions)
[    0.390443] ACPI: Added _OSI(Processor Aggregator Device)
[    0.410679] ACPI: Dynamic OEM Table Load:
[    0.410702] ACPI: SSDT 0xFFFF880073F73400 000353 (v01 PmRef  Cpu0Ist  00003000 INTL 20121114)
[    0.411323] ACPI: Dynamic OEM Table Load:
[    0.411342] ACPI: SSDT 0xFFFF880073F36800 000433 (v01 PmRef  Cpu0Cst  00003001 INTL 20121114)
[    0.412637] ACPI: Dynamic OEM Table Load:
[    0.412654] ACPI: SSDT 0xFFFF880073FE6E00 00015F (v01 PmRef  ApIst    00003000 INTL 20121114)
[    0.413226] ACPI: Dynamic OEM Table Load:
[    0.413243] ACPI: SSDT 0xFFFF880073FCC9C0 00008D (v01 PmRef  ApCst    00003000 INTL 20121114)
[    0.416722] ACPI: Interpreter enabled
[    0.416753] ACPI: (supports S0)
[    0.416757] ACPI: Using IOAPIC for interrupt routing
[    0.416843] PCI: MMCONFIG for domain 0000 [bus 00-3f] at [mem 0xe0000000-0xe3ffffff] (base 0xe0000000)
[    0.422380] [Firmware Info]: PCI: MMCONFIG at [mem 0xe0000000-0xe3ffffff] not reserved in ACPI motherboard resources
[    0.422384] PCI: not using MMCONFIG
[    0.422392] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    0.426914] ACPI: Power Resource [USBC] (on)
[    0.427791] ACPI: Power Resource [WWPR] (off)
[    0.436069] ACPI: Power Resource [PLPE] (on)
[    0.446230] ACPI: Power Resource [CLK0] (on)
[    0.446523] ACPI: Power Resource [P28X] (off)
[    0.446659] ACPI: Power Resource [P18X] (off)
[    0.447420] ACPI: Power Resource [CLK1] (on)
[    0.449867] ACPI: Power Resource [TCPR] (off)
[    0.459372] ACPI: PCI Root Bridge [PCI0] (domain 0000 [bus 00-ff])
[    0.459385] acpi PNP0A08:00: _OSC: OS supports [ASPM ClockPM Segments MSI]
[    0.459517] acpi PNP0A08:00: _OSC failed (AE_ERROR); disabling ASPM
[    0.459548] acpi PNP0A08:00: fail to add MMCONFIG information, can't access extended PCI configuration space under this bridge.
[    0.460294] PCI host bridge to bus 0000:00
[    0.460301] pci_bus 0000:00: root bus resource [io  0x0070-0x0077]
[    0.460306] pci_bus 0000:00: root bus resource [io  0x0000-0x006f window]
[    0.460310] pci_bus 0000:00: root bus resource [io  0x0078-0x0cf7 window]
[    0.460314] pci_bus 0000:00: root bus resource [io  0x0d00-0xffff window]
[    0.460318] pci_bus 0000:00: root bus resource [mem 0x000a0000-0x000bffff window]
[    0.460322] pci_bus 0000:00: root bus resource [mem 0x000c0000-0x000dffff window]
[    0.460326] pci_bus 0000:00: root bus resource [mem 0x000e0000-0x000fffff window]
[    0.460330] pci_bus 0000:00: root bus resource [mem 0x90c00000-0x90ffffff window]
[    0.460334] pci_bus 0000:00: root bus resource [mem 0x7af00001-0x7ef00000 window]
[    0.460338] pci_bus 0000:00: root bus resource [mem 0x80000000-0x908ffffe window]
[    0.460342] pci_bus 0000:00: root bus resource [mem 0xfed40000-0xfed40fff window]
[    0.460346] pci_bus 0000:00: root bus resource [bus 00-ff]
[    0.460364] pci 0000:00:00.0: [8086:0f00] type 00 class 0x060000
[    0.460572] pci 0000:00:02.0: [8086:0f31] type 00 class 0x030000
[    0.460593] pci 0000:00:02.0: reg 0x10: [mem 0x90000000-0x903fffff]
[    0.460610] pci 0000:00:02.0: reg 0x18: [mem 0x80000000-0x8fffffff pref]
[    0.460626] pci 0000:00:02.0: reg 0x20: [io  0x1000-0x1007]
[    0.460843] pci 0000:00:14.0: [8086:0f35] type 00 class 0x0c0330
[    0.460870] pci 0000:00:14.0: reg 0x10: [mem 0x90800000-0x9080ffff 64bit]
[    0.460954] pci 0000:00:14.0: PME# supported from D3hot D3cold
[    0.461133] pci 0000:00:1a.0: [8086:0f18] type 00 class 0x108000
[    0.461160] pci 0000:00:1a.0: reg 0x10: [mem 0x90700000-0x907fffff]
[    0.461175] pci 0000:00:1a.0: reg 0x14: [mem 0x90600000-0x906fffff]
[    0.461279] pci 0000:00:1a.0: PME# supported from D0 D3hot
[    0.461445] pci 0000:00:1f.0: [8086:0f1c] type 00 class 0x060100
[    0.462648] ACPI: PCI Interrupt Link [LNKA] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.462855] ACPI: PCI Interrupt Link [LNKB] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.463057] ACPI: PCI Interrupt Link [LNKC] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.463259] ACPI: PCI Interrupt Link [LNKD] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.463479] ACPI: PCI Interrupt Link [LNKE] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.463683] ACPI: PCI Interrupt Link [LNKF] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.463886] ACPI: PCI Interrupt Link [LNKG] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.464089] ACPI: PCI Interrupt Link [LNKH] (IRQs 3 4 5 6 10 11 12 14 15) *0, disabled.
[    0.475922] acpi 80860F09:00: Device [PWM1] is in always present list
[    0.514528] random: fast init done
[    0.533927] dw_dmac INTL9C60:00: DesignWare DMA Controller, 8 channels
[    0.567299] dw_dmac INTL9C60:01: DesignWare DMA Controller, 8 channels
[    0.567986] pci 0000:00:02.0: vgaarb: setting as boot VGA device
[    0.567992] pci 0000:00:02.0: vgaarb: VGA device added: decodes=io+mem,owns=io+mem,locks=none
[    0.567998] pci 0000:00:02.0: vgaarb: bridge control possible
[    0.568000] vgaarb: loaded
[    0.568216] pps_core: LinuxPPS API ver. 1 registered
[    0.568219] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.568227] PTP clock support registered
[    0.568244] EDAC MC: Ver: 3.0.0
[    0.568555] Registered efivars operations
[    0.582970] PCI: Using ACPI for IRQ routing
[    0.582978] PCI: pci_cache_line_size set to 64 bytes
[    0.583009] Expanded resource Reserved due to conflict with PCI Bus 0000:00
[    0.583016] e820: reserve RAM buffer [mem 0x0008f000-0x0008ffff]
[    0.583020] e820: reserve RAM buffer [mem 0x0009e000-0x0009ffff]
[    0.583023] e820: reserve RAM buffer [mem 0x782bb000-0x7bffffff]
[    0.583027] e820: reserve RAM buffer [mem 0x7951c000-0x7bffffff]
[    0.583043] e820: reserve RAM buffer [mem 0x79527000-0x7bffffff]
[    0.583045] e820: reserve RAM buffer [mem 0x7a000000-0x7bffffff]
[    0.583325] NetLabel: Initializing
[    0.583328] NetLabel:  domain hash size = 128
[    0.583330] NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
[    0.583388] NetLabel:  unlabeled traffic allowed by default
[    0.583670] clocksource: Switched to clocksource refined-jiffies
[    0.615197] VFS: Disk quotas dquot_6.6.0
[    0.615262] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.615508] pnp: PnP ACPI init
[    0.615967] pnp 00:00: Plug and Play ACPI device, IDs PNP0b00 (active)
[    0.616905] system 00:01: [io  0x0680-0x069f] has been reserved
[    0.616911] system 00:01: [io  0x0400-0x047f] has been reserved
[    0.616915] system 00:01: [io  0x0500-0x05fe] has been reserved
[    0.616919] system 00:01: [io  0x0600-0x061f] has been reserved
[    0.616924] system 00:01: [io  0x164e-0x164f] has been reserved
[    0.616947] system 00:01: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.630717] pnp: PnP ACPI: found 2 devices
[    0.636455] pci_bus 0000:00: resource 4 [io  0x0070-0x0077]
[    0.636461] pci_bus 0000:00: resource 5 [io  0x0000-0x006f window]
[    0.636466] pci_bus 0000:00: resource 6 [io  0x0078-0x0cf7 window]
[    0.636470] pci_bus 0000:00: resource 7 [io  0x0d00-0xffff window]
[    0.636474] pci_bus 0000:00: resource 8 [mem 0x000a0000-0x000bffff window]
[    0.636478] pci_bus 0000:00: resource 9 [mem 0x000c0000-0x000dffff window]
[    0.636482] pci_bus 0000:00: resource 10 [mem 0x000e0000-0x000fffff window]
[    0.636499] pci_bus 0000:00: resource 11 [mem 0x90c00000-0x90ffffff window]
[    0.636504] pci_bus 0000:00: resource 12 [mem 0x7af00001-0x7ef00000 window]
[    0.636508] pci_bus 0000:00: resource 13 [mem 0x80000000-0x908ffffe window]
[    0.636512] pci_bus 0000:00: resource 14 [mem 0xfed40000-0xfed40fff window]
[    0.638679] NET: Registered protocol family 2
[    0.639120] TCP established hash table entries: 16384 (order: 5, 131072 bytes)
[    0.639238] TCP bind hash table entries: 16384 (order: 6, 262144 bytes)
[    0.639370] TCP: Hash tables configured (established 16384 bind 16384)
[    0.639471] UDP hash table entries: 1024 (order: 3, 32768 bytes)
[    0.639502] UDP-Lite hash table entries: 1024 (order: 3, 32768 bytes)
[    0.639637] NET: Registered protocol family 1
[    0.639690] pci 0000:00:02.0: Video device with shadowed ROM at [mem 0x000c0000-0x000dffff]
[    0.640384] PCI: CLS 0 bytes, default 64
[    0.640526] Unpacking initramfs...
[    0.870387] Freeing initrd memory: 5492K
[    0.870546] clocksource: tsc: mask: 0xffffffffffffffff max_cycles: 0x1336e3dbd1a, max_idle_ns: 440795236868 ns
[    0.870608] clocksource: Switched to clocksource tsc
[    0.871444] Scanning for low memory corruption every 60 seconds
[    0.872962] Initialise system trusted keyrings
[    0.873077] workingset: timestamp_bits=40 max_order=19 bucket_order=0
[    0.876518] zbud: loaded
[    0.879506] Key type asymmetric registered
[    0.879554] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[    0.879648] io scheduler noop registered
[    0.879651] io scheduler deadline registered
[    0.879733] io scheduler cfq registered (default)
[    0.879737] io scheduler mq-deadline registered
[    0.879739] io scheduler kyber registered
[    0.880246] efifb: probing for efifb
[    0.880280] efifb: framebuffer at 0x80000000, using 4032k, total 4032k
[    0.880283] efifb: mode is 800x1280x32, linelength=3200, pages=1
[    0.880285] efifb: scrolling: redraw
[    0.880288] efifb: Truecolor: size=8:8:8:8, shift=24:16:8:0
[    0.892863] Console: switching to colour frame buffer device 160x50
[    0.904797] fb0: EFI VGA frame buffer device
[    0.904823] intel_idle: MWAIT substates: 0x33000020
[    0.904826] intel_idle: v0.4.1 model 0x37
[    0.904833] intel_idle: max_cstate 1 reached
[    0.905849] intel_idle: lapic_timer_reliable_states 0xffffffff
[    0.915861] GHES: HEST is not enabled!
[    0.916101] Serial: 8250/16550 driver, 4 ports, IRQ sharing enabled
[    0.917360] hpet: number irqs doesn't agree with number of timers
[    0.917424] Linux agpgart interface v0.103
[    0.921393] libphy: Fixed MDIO Bus: probed
[    0.921482] cnic: QLogic cnicDriver v2.5.22 (July 20, 2015)
[    0.921594] bnx2x: QLogic 5771x/578xx 10/20-Gigabit Ethernet Driver bnx2x 1.712.30-0 (2014/02/10)
[    0.921809] enic: Cisco VIC Ethernet NIC Driver, ver 2.3.0.31
[    0.921869] ACPI Warning: Could not enable fixed event - RealTimeClock (4) (20170303/evxface-654)
[    0.922041] rtc_cmos 00:00: rtc core: registered rtc_cmos as rtc0
[    0.922055] rtc_cmos 00:00: no alarms, 242 bytes nvram
[    0.922077] intel_pstate: Intel P-state driver initializing
[    0.922430] ledtrig-cpu: registered to indicate activity on CPUs
[    0.924186] NET: Registered protocol family 10
[    0.939286] Segment Routing with IPv6
[    0.939330] NET: Registered protocol family 17
[    0.940492] microcode: sig=0x30673, pf=0x2, revision=0x322
[    0.940611] microcode: Microcode Update Driver: v2.2.
[    0.940935] registered taskstats version 1
[    0.940950] Loading compiled-in X.509 certificates
[    0.940991] zswap: loaded using pool lzo/zbud
[    0.941572]   Magic number: 9:894:752
[    0.941590] tty ttyS3: hash matches
[    0.941739] rtc_cmos 00:00: setting system clock to 2017-07-13 21:43:36 UTC (1499982216)
[    0.941836] PM: Hibernation image not present or could not be loaded.
[    0.952294] Freeing unused kernel memory: 1356K
[    0.952299] Write protecting the kernel read-only data: 12288k
[    0.953002] Freeing unused kernel memory: 856K
[    0.962895] Freeing unused kernel memory: 1816K
[    1.149650] sdhci: Secure Digital Host Controller Interface driver
[    1.149653] sdhci: Copyright(c) Pierre Ossman
[    1.165057] i8042: PNP: No PS/2 controller found.
[    1.169729] ACPI: bus type USB registered
[    1.169796] usbcore: registered new interface driver usbfs
[    1.169822] usbcore: registered new interface driver hub
[    1.170412] usbcore: registered new device driver usb
[    1.173747] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.173774] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 1
[    1.174899] xhci_hcd 0000:00:14.0: hcc params 0x200077c1 hci version 0x100 quirks 0x00009810
[    1.174909] xhci_hcd 0000:00:14.0: cache line size of 64 is not supported
[    1.175533] hub 1-0:1.0: USB hub found
[    1.175555] hub 1-0:1.0: 6 ports detected
[    1.362239] mmc0: SDHCI controller on ACPI [INT33BB:00] using ADMA
[    1.378312] mmc1: SDHCI controller on ACPI [80860F14:00] using ADMA
[    1.395365] mmc2: SDHCI controller on ACPI [80860F14:01] using ADMA
[    1.437129] mmc0: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.447309] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.457684] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.462604] mmc1: new HS200 MMC card at address 0001
[    1.467962] mmcblk1: mmc1:0001 MCG8GC 58.2 GiB 
[    1.471522] mmcblk1boot0: mmc1:0001 MCG8GC partition 1 4.00 MiB
[    1.471976] mmcblk1boot1: mmc1:0001 MCG8GC partition 2 4.00 MiB
[    1.472152] mmcblk1rpmb: mmc1:0001 MCG8GC partition 3 4.00 MiB
[    1.475455]  mmcblk1: p1 p2
[    1.506249] mmc0: new ultra high speed DDR50 SDIO card at address 0001
[    1.580424] mmc0: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.590853] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.601035] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.697624] random: crng init done
[    1.708250] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.708271] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 2
[    1.709449] hub 2-0:1.0: USB hub found
[    1.709490] hub 2-0:1.0: 1 port detected
[    1.721573] mmc0: queuing unknown CIS tuple 0x80 (7 bytes)
[    1.731605] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[    1.741687] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[   51.672907] F2FS-fs (mmcblk1p2): Mounted with checkpoint version = 43208e15
[   51.814611] ip_tables: (C) 2000-2006 Netfilter Core Team
[   51.824238] systemd[1]: systemd 234 running in system mode. (+PAM -AUDIT -SELINUX -IMA -APPARMOR +SMACK -SYSVINIT +UTMP +LIBCRYPTSETUP +GCRYPT +GNUTLS +ACL +XZ +LZ4 +SECCOMP +BLKID +ELFUTILS +KMOD -IDN2 +IDN default-hierarchy=hybrid)
[   51.824634] systemd[1]: Detected architecture x86-64.
[   51.825712] systemd[1]: Set hostname to <erhoof_tablet>.
[   51.887813] systemd-gpt-auto-generator[166]: Failed to dissect: Input/output error
[   51.888841] systemd[160]: /usr/lib/systemd/system-generators/systemd-gpt-auto-generator failed with error code 1.
[   51.965211] systemd[1]: Listening on LVM2 metadata daemon socket.
[   51.965328] systemd[1]: Reached target Swap.
[   51.968920] systemd[1]: Listening on Process Core Dump Socket.
[   51.969012] systemd[1]: Listening on /dev/initctl Compatibility Named Pipe.
[   51.975466] systemd[1]: Listening on udev Kernel Socket.
[   51.975603] systemd[1]: Listening on udev Control Socket.
[   52.098624] systemd-journald[180]: Received request to flush runtime journal from PID 1
[   52.306341] ACPI: AC Adapter [ADP1] (on-line)
[   52.324226] 80860F0A:00: ttyS0 at MMIO 0x9094d000 (irq = 186, base_baud = 2764800) is a 16550A
[   52.406721] Bluetooth: Core ver 2.22
[   52.406766] NET: Registered protocol family 31
[   52.406768] Bluetooth: HCI device and connection manager initialized
[   52.406776] Bluetooth: HCI socket layer initialized
[   52.406781] Bluetooth: L2CAP socket layer initialized
[   52.406793] Bluetooth: SCO socket layer initialized
[   52.412171] wmi: Mapper loaded
[   52.424916] Bluetooth: HCI UART driver ver 2.3
[   52.424920] Bluetooth: HCI UART protocol H4 registered
[   52.424922] Bluetooth: HCI UART protocol BCSP registered
[   52.424961] Bluetooth: HCI UART protocol LL registered
[   52.424963] Bluetooth: HCI UART protocol ATH3K registered
[   52.424965] Bluetooth: HCI UART protocol Three-wire (H5) registered
[   52.425046] Bluetooth: HCI UART protocol Intel registered
[   52.431011] i8042: PNP: No PS/2 controller found.
[   52.440962] hci_bcm BCM2E3F:00: BCM irq: 187
[   52.441038] hci_bcm BCM2E3F:00: BCM2E3F:00 device registered.
[   52.441203] Bluetooth: HCI UART protocol Broadcom registered
[   52.441205] Bluetooth: HCI UART protocol QCA registered
[   52.441207] Bluetooth: HCI UART protocol AG6XX registered
[   52.441208] Bluetooth: HCI UART protocol Marvell registered
[   52.475535] [Firmware Bug]: No valid trip found
[   52.494191] intel_sst_acpi 80860F28:00: BYT-CR not detected
[   52.494374] intel_sst_acpi 80860F28:00: LPE base: 0x90a00000 size:0x200000
[   52.494378] intel_sst_acpi 80860F28:00: IRAM base: 0x90ac0000
[   52.494428] intel_sst_acpi 80860F28:00: DRAM base: 0x90b00000
[   52.494437] intel_sst_acpi 80860F28:00: SHIM base: 0x90b40000
[   52.494447] intel_sst_acpi 80860F28:00: Mailbox base: 0x90b44000
[   52.494458] intel_sst_acpi 80860F28:00: DDR base: 0x20000000
[   52.497349] intel_sst_acpi 80860F28:00: Got drv data max stream 25
[   52.511951] input: Lid Switch as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0C0D:00/input/input0
[   52.512462] ACPI: Lid Switch [LID]
[   52.579806] hidraw: raw HID events driver (C) Jiri Kosina
[   52.582590] input: PC Speaker as /devices/platform/pcspkr/input/input1
[   52.595379] ACPI: Battery Slot [BATC] (battery present)
[   52.630920] SSE version of gcm_enc/dec engaged.
[   52.640831] [drm] Memory usable by graphics device = 2048M
[   52.640837] checking generic (80000000 3f0000) vs hw (80000000 10000000)
[   52.640839] fb: switching to inteldrmfb from EFI VGA
[   52.640885] Console: switching to colour dummy device 80x25
[   52.641079] [drm] Replacing VGA console driver
[   52.641256] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[   52.641258] [drm] Driver supports precise vblank timestamp query.
[   52.642028] i915 0000:00:02.0: vgaarb: changed VGA decodes: olddecodes=io+mem,decodes=io+mem:owns=io+mem
[   52.682716] [drm] Initialized i915 1.6.0 20170703 for 0000:00:02.0 on minor 0
[   52.686348] ACPI: Video Device [GFX0] (multi-head: yes  rom: no  post: no)
[   52.690527] input: Video Bus as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0A08:00/LNXVIDEO:00/input/input2
[   52.692135] [drm] HDaudio controller not detected, using LPE audio instead

[   52.711861] i8042: PNP: No PS/2 controller found.
[   52.741553] input: gpio-keys as /devices/platform/gpio-keys.0.auto/input/input3
[   52.741931] input: gpio-keys as /devices/platform/gpio-keys.1.auto/input/input4
[   52.742394] iTCO_vendor_support: vendor-support=0
[   52.743845] bytcr_rt5640 bytcr_rt5640: quirk DMIC1_MAP enabled
[   52.743850] bytcr_rt5640 bytcr_rt5640: quirk DMIC enabled
[   52.743853] bytcr_rt5640 bytcr_rt5640: quirk MCLK_EN enabled
[   52.744562] iTCO_wdt: Intel TCO WatchDog Timer Driver v1.11
[   52.744765] iTCO_wdt: Found a Bay Trail SoC TCO device (Version=3, TCOBASE=0x0460)
[   52.757032] bytcr_rt5640 bytcr_rt5640: snd-soc-dummy-dai <-> media-cpu-dai mapping ok
[   52.758046] bytcr_rt5640 bytcr_rt5640: snd-soc-dummy-dai <-> deepbuffer-cpu-dai mapping ok
[   52.758105] compress asoc: snd-soc-dummy-dai <-> compress-cpu-dai mapping ok
[   52.761909] bytcr_rt5640 bytcr_rt5640: rt5640-aif1 <-> ssp2-port mapping ok
[   52.764864] iTCO_wdt: initialized. heartbeat=30 sec (nowayout=0)
[   52.766029] i915 0000:00:02.0: HDMI-A-2: EDID is invalid:
[   52.766036] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   52.766037] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   52.766039] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   52.766040] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   52.766042] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   52.766043] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   52.766044] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   52.766046] 	[00] ZERO 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
[   52.774445] fbcon: inteldrmfb (fb0) is primary device
[   52.780628] [drm:pipe_config_err [i915]] *ERROR* mismatch in dsi_pll.div (expected 0x00000157, found 0x000001ab)
[   52.780661] pipe state doesn't match!
[   52.780693] ------------[ cut here ]------------
[   52.780781] WARNING: CPU: 3 PID: 138 at drivers/gpu/drm/i915/intel_display.c:12295 intel_atomic_commit_tail+0xd71/0xf50 [i915]
[   52.780782] Modules linked in: evdev irqbypass iTCO_wdt snd_soc_sst_bytcr_rt5640(+) iTCO_vendor_support gpio_keys crct10dif_pclmul crc32c_intel ghash_clmulni_intel pcbc nls_iso8859_1 brcmfmac nls_cp437 aesni_intel brcmutil vfat aes_x86_64 fat crypto_simd cfg80211 glue_helper cryptd i915 intel_cstate snd_soc_rt5670 snd_soc_rt5645 i2c_hid(+) pcspkr hid battery drm_kms_helper snd_soc_rt5640 snd_soc_rl6231 drm mei_txe mei intel_gtt syscopyarea sysfillrect sysimgblt fb_sys_fops lpc_ich snd_intel_sst_acpi snd_intel_sst_core snd_soc_sst_atom_hifi2_platform thermal snd_soc_sst_match hci_uart snd_soc_core btbcm btqca wmi btintel button tpm_crb soc_button_array bluetooth dptf_power int3406_thermal video snd_compress snd_pcm_dmaengine snd_pcm snd_timer ecdh_generic rfkill snd crc16 processor_thermal_device
[   52.780841]  int3402_thermal int3403_thermal soundcore int3400_thermal ac97_bus int340x_thermal_zone intel_soc_dts_iosf acpi_thermal_rel acpi_pad ac i2c_designware_platform i2c_designware_core tpm_tis tpm_tis_core tpm 8250_dw spi_pxa2xx_platform sch_fq_codel ip_tables x_tables f2fs fscrypto mmc_block crc32_pclmul xhci_pci xhci_hcd usbcore usb_common serio sdhci_acpi sdhci led_class mmc_core
[   52.780872] CPU: 3 PID: 138 Comm: kworker/u8:3 Not tainted 4.12.0-W4+ #1
[   52.780873] Hardware name: Acer TP-W4-820-Z3742G06AII/Cheetah3, BIOS V1.16 03/13/2014
[   52.780882] Workqueue: events_unbound async_run_entry_fn
[   52.780884] task: ffff88007394ce00 task.stack: ffffc90000c3c000
[   52.780970] RIP: 0010:intel_atomic_commit_tail+0xd71/0xf50 [i915]
[   52.780971] RSP: 0018:ffffc90000c3f8a0 EFLAGS: 00010286
[   52.780974] RAX: 0000000000000019 RBX: ffff880011270310 RCX: 0000000000000019
[   52.780975] RDX: 0000000000000000 RSI: 0000000000000002 RDI: 0000000000000292
[   52.780976] RBP: ffffc90000c3f958 R08: 0000000000000000 R09: 0000000000000019
[   52.780978] R10: 00000000000614f0 R11: 0000000000000200 R12: ffff880071fc8800
[   52.780979] R13: ffff880073b3b000 R14: ffff88001122e000 R15: ffff880011270308
[   52.780982] FS:  0000000000000000(0000) GS:ffff880076b80000(0000) knlGS:0000000000000000
[   52.780983] CS:  0010 DS: 0000 ES: 0000 CR0: 0000000080050033
[   52.780985] CR2: 0000556a0df00000 CR3: 000000000e8b9000 CR4: 00000000001006e0
[   52.780986] Call Trace:
[   52.780996]  ? wake_bit_function+0x60/0x60
[   52.781074]  intel_atomic_commit+0x35c/0x4b0 [i915]
[   52.781090]  ? drm_atomic_check_only+0x37f/0x540 [drm]
[   52.781103]  drm_atomic_commit+0x4b/0x50 [drm]
[   52.781111]  restore_fbdev_mode_atomic+0x182/0x1f0 [drm_kms_helper]
[   52.781117]  restore_fbdev_mode+0x32/0x130 [drm_kms_helper]
[   52.781123]  drm_fb_helper_restore_fbdev_mode_unlocked+0x31/0x90 [drm_kms_helper]
[   52.781128]  drm_fb_helper_set_par+0x2d/0x60 [drm_kms_helper]
[   52.781205]  intel_fbdev_set_par+0x1a/0x70 [i915]
[   52.781209]  fbcon_init+0x484/0x650
[   52.781215]  visual_init+0xd6/0x130
[   52.781218]  do_bind_con_driver+0x1fc/0x410
[   52.781222]  do_take_over_console+0x82/0x1a0
[   52.781225]  do_fbcon_takeover+0x5c/0xb0
[   52.781227]  fbcon_event_notify+0x587/0x780
[   52.781232]  notifier_call_chain+0x4a/0x70
[   52.781235]  blocking_notifier_call_chain+0x43/0x60
[   52.781238]  fb_notifier_call_chain+0x1b/0x20
[   52.781241]  register_framebuffer+0x24d/0x360
[   52.781245]  ? vga_switcheroo_client_fb_set+0x5b/0x70
[   52.781252]  drm_fb_helper_initial_config+0x249/0x400 [drm_kms_helper]
[   52.781326]  intel_fbdev_initial_config+0x18/0x30 [i915]
[   52.781330]  async_run_entry_fn+0x37/0x150
[   52.781334]  process_one_work+0x1de/0x420
[   52.781338]  worker_thread+0x47/0x3f0
[   52.781341]  kthread+0x125/0x140
[   52.781344]  ? process_one_work+0x420/0x420
[   52.781347]  ? kthread_create_on_node+0x70/0x70
[   52.781351]  ret_from_fork+0x25/0x30
[   52.781353] Code: d0 a0 61 a0 e8 5e 9b c3 e0 0f ff 0f b6 8d 60 ff ff ff 44 0f b6 85 70 ff ff ff e9 3c fd ff ff 48 c7 c7 97 5c 60 a0 e8 3c 9b c3 e0 <0f> ff e9 aa f8 ff ff 48 8d 7d 80 31 f6 e8 9d 42 b7 e0 48 69 c3 
[   52.781398] ---[ end trace 1c93f81e6ccfe4df ]---
[   52.781693] Console: switching to colour frame buffer device 160x50
[   52.804974] i915 0000:00:02.0: fb0: inteldrmfb frame buffer device
[   52.849505] (NULL device *): hwmon_device_register() is deprecated. Please convert the driver to use hwmon_device_register_with_info().
[   52.849645] (NULL device *): hwmon_device_register() is deprecated. Please convert the driver to use hwmon_device_register_with_info().
[   52.856539] input: Intel HDMI/DP LPE Audio HDMI/DP,pcm=0 as /devices/pci0000:00/0000:00:02.0/hdmi-lpe-audio/sound/card1/input5
[   52.856706] input: Intel HDMI/DP LPE Audio HDMI/DP,pcm=1 as /devices/pci0000:00/0000:00:02.0/hdmi-lpe-audio/sound/card1/input6
[   52.858662] intel_rapl: Found RAPL domain package
[   52.858666] intel_rapl: Found RAPL domain core
[   52.936151] mmc0: queuing unknown CIS tuple 0x80 (7 bytes)
[   52.946439] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[   52.957000] mmc0: queuing unknown CIS tuple 0x80 (31 bytes)
[   53.005335] usbcore: registered new interface driver brcmfmac
[   53.122732] i2c_hid i2c-SMO91D0:00: failed to retrieve report from device.
[   53.147517] input: SYNA7300:00 06CB:0106 as /devices/platform/80860F41:05/i2c-5/i2c-SYNA7300:00/0018:06CB:0106.0002/input/input7
[   53.147734] hid-multitouch 0018:06CB:0106.0002: input,hidraw0: I2C HID v1.00 Device [SYNA7300:00 06CB:0106] on i2c-SYNA7300:00
[   53.154329] mousedev: PS/2 mouse device common for all mice
[   53.165366] brcmfmac: brcmf_c_preinit_dcmds: Firmware version = wl0: Jul 17 2013 07:36:07 version 6.10.197.71 (r412987) FWID 01-882d2634
[   53.534295] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[   53.567253] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[   54.087050] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[   54.209041] brcmfmac: brcmf_p2p_create_p2pdev: set p2p_disc error
[   54.209294] brcmfmac: brcmf_cfg80211_add_iface: add iface p2p-dev-wlan0 type 10 failed: err=-16
[   54.225231] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[   58.468832] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[   61.839681] intel_sst_acpi 80860F28:00: FW Version 01.0c.00.01
[   61.840125]  Baytrail Audio Port: ASoC: no backend DAIs enabled for Baytrail Audio Port
[   61.840541]  Baytrail Audio Port: ASoC: no backend DAIs enabled for Baytrail Audio Port
[   61.840900]  Baytrail Audio Port: ASoC: no backend DAIs enabled for Baytrail Audio Port