[    0.000000] Linux version 4.12.8-300.fc26.i686+PAE (mockbuild@bkernel01.phx2.fedoraproject.org) (gcc version 7.1.1 20170622 (Red Hat 7.1.1-3) (GCC) ) #1 SMP Thu Aug 17 15:49:25 UTC 2017
[    0.000000] x86/fpu: x87 FPU will use FXSAVE
[    0.000000] e820: BIOS-provided physical RAM map:
[    0.000000] BIOS-e820: [mem 0x0000000000000000-0x000000000009ffff] usable
[    0.000000] BIOS-e820: [mem 0x0000000000100000-0x00000000cffbffff] usable
[    0.000000] BIOS-e820: [mem 0x00000000cffc0000-0x00000000cffcfbff] ACPI data
[    0.000000] BIOS-e820: [mem 0x00000000cffcfc00-0x00000000cfffefff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000e0000000-0x00000000fec8ffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed00000-0x00000000fed003ff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fee00000-0x00000000fee0ffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000ffb00000-0x00000000ffffffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000100000000-0x00000002afffffff] usable
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] SMBIOS 2.3 present.
[    0.000000] DMI: Dell Computer Corporation PowerEdge 1850/0D8266, BIOS A01 09/02/2004
[    0.000000] tsc: Fast TSC calibration using PIT
[    0.000000] e820: update [mem 0x00000000-0x00000fff] usable ==> reserved
[    0.000000] e820: remove [mem 0x000a0000-0x000fffff] usable
[    0.000000] e820: last_pfn = 0x2b0000 max_arch_pfn = 0x1000000
[    0.000000] MTRR default type: uncachable
[    0.000000] MTRR fixed ranges enabled:
[    0.000000]   00000-9FFFF write-back
[    0.000000]   A0000-BFFFF uncachable
[    0.000000]   C0000-D3FFF write-protect
[    0.000000]   D4000-EBFFF uncachable
[    0.000000]   EC000-FFFFF write-protect
[    0.000000] MTRR variable ranges enabled:
[    0.000000]   0 base 000000000 mask E00000000 write-back
[    0.000000]   1 base 200000000 mask F80000000 write-back
[    0.000000]   2 base 280000000 mask FE0000000 write-back
[    0.000000]   3 base 2A0000000 mask FF0000000 write-back
[    0.000000]   4 base 0D0000000 mask FF0000000 uncachable
[    0.000000]   5 base 0E0000000 mask FE0000000 uncachable
[    0.000000]   6 disabled
[    0.000000]   7 disabled
[    0.000000] x86/PAT: Configuration [0-7]: WB  WC  UC- UC  WB  WC  UC- UC  
[    0.000000] e820: update [mem 0xd0000000-0xffffffff] usable ==> reserved
[    0.000000] found SMP MP-table at [mem 0x000fe710-0x000fe71f] mapped at [c00fe710]
[    0.000000] initial memory mapped: [mem 0x00000000-0x0b1fffff]
[    0.000000] Base memory trampoline at [c009b000] 9b000 size 16384
[    0.000000] BRK [0x0ad5c000, 0x0ad5cfff] PGTABLE
[    0.000000] BRK [0x0ad5d000, 0x0ad5ffff] PGTABLE
[    0.000000] BRK [0x0ad60000, 0x0ad60fff] PGTABLE
[    0.000000] BRK [0x0ad61000, 0x0ad61fff] PGTABLE
[    0.000000] RAMDISK: [mem 0x35377000-0x369b3fff]
[    0.000000] ACPI: Early table checksum verification disabled
[    0.000000] ACPI: RSDP 0x00000000000FD6C0 000014 (v00 DELL  )
[    0.000000] ACPI: RSDT 0x00000000000FD6D4 000034 (v01 DELL   PE BKC   00000001 MSFT 0100000A)
[    0.000000] ACPI: FACP 0x00000000000FD708 000074 (v01 DELL   PE BKC   00000001 MSFT 0100000A)
[    0.000000] ACPI: DSDT 0x00000000CFFC0000 003861 (v01 DELL   PE BKC   00000001 MSFT 0100000E)
[    0.000000] ACPI: FACS 0x00000000CFFCFC00 000040
[    0.000000] ACPI: APIC 0x00000000000FD77C 00009C (v01 DELL   PE BKC   00000001 MSFT 0100000A)
[    0.000000] ACPI: SPCR 0x00000000000FD824 000050 (v01 DELL   PE BKC   00000001 MSFT 0100000A)
[    0.000000] ACPI: HPET 0x00000000000FD874 000038 (v01 DELL   PE BKC   00000001 MSFT 0100000A)
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] 10120MB HIGHMEM available.
[    0.000000] 887MB LOWMEM available.
[    0.000000]   mapped low ram: 0 - 377fe000
[    0.000000]   low ram: 0 - 377fe000
[    0.000000] Zone ranges:
[    0.000000]   DMA      [mem 0x0000000000001000-0x0000000000ffffff]
[    0.000000]   Normal   [mem 0x0000000001000000-0x00000000377fdfff]
[    0.000000]   HighMem  [mem 0x00000000377fe000-0x00000002afffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000000001000-0x000000000009ffff]
[    0.000000]   node   0: [mem 0x0000000000100000-0x00000000cffbffff]
[    0.000000]   node   0: [mem 0x0000000100000000-0x00000002afffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000000001000-0x00000002afffffff]
[    0.000000] On node 0 totalpages: 2621279
[    0.000000] free_area_init_node: node 0, pgdat cab35240, node_mem_map ee7f7028
[    0.000000]   DMA zone: 40 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 3999 pages, LIFO batch:0
[    0.000000]   Normal zone: 2180 pages used for memmap
[    0.000000]   Normal zone: 223230 pages, LIFO batch:31
[    0.000000]   HighMem zone: 2394050 pages, LIFO batch:31
[    0.000000] Using APIC driver default
[    0.000000] ACPI: PM-Timer IO Port: 0x808
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] ACPI: LAPIC_NMI (acpi_id[0x01] high edge lint[0x1])
[    0.000000] ACPI: LAPIC_NMI (acpi_id[0x02] high edge lint[0x1])
[    0.000000] ACPI: LAPIC_NMI (acpi_id[0x03] high edge lint[0x1])
[    0.000000] ACPI: LAPIC_NMI (acpi_id[0x04] high edge lint[0x1])
[    0.000000] IOAPIC[0]: apic_id 8, version 32, address 0xfec00000, GSI 0-23
[    0.000000] IOAPIC[1]: apic_id 9, version 32, address 0xfec80000, GSI 32-55
[    0.000000] IOAPIC[2]: apic_id 10, version 32, address 0xfec83000, GSI 64-87
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.000000] ACPI: IRQ0 used by override.
[    0.000000] ACPI: IRQ9 used by override.
[    0.000000] Using ACPI (MADT) for SMP configuration information
[    0.000000] ACPI: HPET id: 0xffffffff base: 0xfed00000
[    0.000000] smpboot: Allowing 4 CPUs, 0 hotplug CPUs
[    0.000000] PM: Registered nosave memory: [mem 0x00000000-0x00000fff]
[    0.000000] PM: Registered nosave memory: [mem 0x000a0000-0x000fffff]
[    0.000000] e820: [mem 0xcffff000-0xdfffffff] available for PCI devices
[    0.000000] Booting paravirtualized kernel on bare hardware
[    0.000000] clocksource: refined-jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1910969940391419 ns
[    0.000000] setup_percpu: NR_CPUS:32 nr_cpumask_bits:4 nr_cpu_ids:4 nr_node_ids:1
[    0.000000] percpu: Embedded 21 pages/cpu @f77a5000 s57036 r0 d28980 u86016
[    0.000000] pcpu-alloc: s57036 r0 d28980 u86016 alloc=21*4096
[    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3 
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 2619059
[    0.000000] Kernel command line: BOOT_IMAGE=/vmlinuz-4.12.8-300.fc26.i686+PAE root=/dev/mapper/fedora-root ro rd.lvm.lv=fedora/root rd.lvm.lv=fedora/swap rhgb quiet audit=0 LANG=en_US.UTF-8
[    0.000000] audit: disabled (until reboot)
[    0.000000] PID hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes)
[    0.000000] microcode: microcode updated early to revision 0x17, date = 2005-04-22
[    0.000000] Initializing CPU#0
[    0.000000] Initializing HighMem for node 0 (000377fe:002b0000)
[    0.000000] Initializing Movable for node 0 (00000000:00000000)
[    0.000000] Memory: 10337344K/10485116K available (7761K kernel code, 797K rwdata, 3080K rodata, 912K init, 640K bss, 147772K reserved, 0K cma-reserved, 9576200K highmem)
[    0.000000] virtual kernel memory layout:
                   fixmap  : 0xffa76000 - 0xfffff000   (5668 kB)
                   pkmap   : 0xff800000 - 0xffa00000   (2048 kB)
                   vmalloc : 0xf7ffe000 - 0xff7fe000   ( 120 MB)
                   lowmem  : 0xc0000000 - 0xf77fe000   ( 887 MB)
                     .init : 0xcab76000 - 0xcac5a000   ( 912 kB)
                     .data : 0xca79468a - 0xcab606c0   (3888 kB)
                     .text : 0xca000000 - 0xca79468a   (7761 kB)
[    0.000000] Checking if this processor honours the WP bit even in supervisor mode...Ok.
[    0.000000] SLUB: HWalign=128, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 33291 entries in 66 pages
[    0.000000] Hierarchical RCU implementation.
[    0.000000] 	RCU restricting CPUs from NR_CPUS=32 to nr_cpu_ids=4.
[    0.000000] RCU: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=4
[    0.000000] NR_IRQS:2304 nr_irqs:1024 16
[    0.000000] CPU 0 irqstacks, hard=f70c2000 soft=f70c4000
[    0.000000] Console: colour VGA+ 80x25
[    0.000000] console [tty0] enabled
[    0.000000] clocksource: hpet: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 133484882848 ns
[    0.000000] hpet clockevent registered
[    0.000000] tsc: Fast TSC calibration using PIT
[    0.001000] tsc: Detected 2792.955 MHz processor
[    0.001000] Calibrating delay loop (skipped), value calculated using timer frequency.. 5585.91 BogoMIPS (lpj=2792955)
[    0.001000] pid_max: default: 32768 minimum: 301
[    0.001000] ACPI: Core revision 20170303
[    0.005241] ACPI: 1 ACPI AML tables successfully acquired and loaded
[    0.005322] Security Framework initialized
[    0.005326] Yama: becoming mindful.
[    0.005334] SELinux:  Initializing.
[    0.005369] SELinux:  Starting in permissive mode
[    0.005399] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.005403] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.005784] CPU: Physical Processor ID: 0
[    0.005786] CPU: Processor Core ID: 0
[    0.005799] mce: CPU supports 4 MCE banks
[    0.005813] CPU0: Thermal monitoring enabled (TM1)
[    0.005821] process: using mwait in idle threads
[    0.005832] Last level iTLB entries: 4KB 64, 2MB 64, 4MB 64
[    0.005834] Last level dTLB entries: 4KB 64, 2MB 0, 4MB 64, 1GB 0
[    0.006025] Freeing SMP alternatives memory: 32K
[    0.007374] smpboot: Max logical packages: 4
[    0.007385] Enabling APIC mode:  Flat.  Using 3 I/O APICs
[    0.007922] ..TIMER: vector=0x30 apic1=0 pin1=2 apic2=-1 pin2=-1
[    0.018000] smpboot: CPU0: Intel(R) Xeon(TM) CPU 2.80GHz (family: 0xf, model: 0x4, stepping: 0x1)
[    0.018000] Performance Events: Netburst events, Netburst P4/Xeon PMU driver.
[    0.018000] ... version:                0
[    0.018000] ... bit width:              40
[    0.018000] ... generic registers:      18
[    0.018000] ... value mask:             000000ffffffffff
[    0.018000] ... max period:             0000007fffffffff
[    0.018000] ... fixed-purpose events:   0
[    0.018000] ... event mask:             000000000003ffff
[    0.018429] NMI watchdog: enabled on all CPUs, permanently consumes one hw-PMU counter.
[    0.018468] smp: Bringing up secondary CPUs ...
[    0.018662] CPU 1 irqstacks, hard=f716e000 soft=f7170000
[    0.018665] x86: Booting SMP configuration:
[    0.018667] .... node  #0, CPUs:      #1
[    0.001000] Initializing CPU#1
[    0.001000] smpboot: CPU 1 Converting physical 3 to logical package 1
[    0.090207] CPU 2 irqstacks, hard=f719e000 soft=f71a0000
[    0.090209]  #2
[    0.001000] Initializing CPU#2
[    0.163245] CPU 3 irqstacks, hard=f71c2000 soft=f71c4000
[    0.163248]  #3
[    0.001000] Initializing CPU#3
[    0.235052] smp: Brought up 1 node, 4 CPUs
[    0.235052] smpboot: Total of 4 processors activated (22343.31 BogoMIPS)
[    0.236291] sched_clock: Marking stable (236000000, 0)->(358347355, -122347355)
[    0.237357] devtmpfs: initialized
[    0.238249] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1911260446275000 ns
[    0.238257] futex hash table entries: 1024 (order: 4, 65536 bytes)
[    0.238415] pinctrl core: initialized pinctrl subsystem
[    0.238471] RTC time: 16:15:16, date: 08/29/17
[    0.238656] NET: Registered protocol family 16
[    0.239233] cpuidle: using governor menu
[    0.239455] ACPI: bus type PCI registered
[    0.239459] acpiphp: ACPI Hot Plug PCI Controller Driver version: 0.5
[    0.239572] PCI: MMCONFIG for domain 0000 [bus 00-ff] at [mem 0xe0000000-0xefffffff] (base 0xe0000000)
[    0.239574] PCI: Intel Corporation E7520 Memory Controller Hub with MMCONFIG support
[    0.239581] PCI: MMCONFIG at [mem 0xe0000000-0xefffffff] reserved in E820
[    0.239582] PCI: Using MMCONFIG for extended config space
[    0.239584] PCI: Using configuration type 1 for base access
[    0.243095] HugeTLB registered 2 MB page size, pre-allocated 0 pages
[    0.243637] ACPI: Added _OSI(Module Device)
[    0.243639] ACPI: Added _OSI(Processor Device)
[    0.243641] ACPI: Added _OSI(3.0 _SCP Extensions)
[    0.243643] ACPI: Added _OSI(Processor Aggregator Device)
[    0.247771] ACPI: Interpreter enabled
[    0.247818] ACPI: (supports S0 S4 S5)
[    0.247820] ACPI: Using IOAPIC for interrupt routing
[    0.248429] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    0.262086] ACPI: PCI Root Bridge [PCI0] (domain 0000 [bus 00-ff])
[    0.262095] acpi PNP0A03:00: _OSC: OS supports [ExtendedConfig ASPM ClockPM Segments MSI]
[    0.262105] acpi PNP0A03:00: _OSC failed (AE_NOT_FOUND); disabling ASPM
[    0.263012] PCI host bridge to bus 0000:00
[    0.263017] pci_bus 0000:00: root bus resource [io  0x0000-0x0cf7 window]
[    0.263020] pci_bus 0000:00: root bus resource [io  0x0d00-0xffff window]
[    0.263023] pci_bus 0000:00: root bus resource [mem 0x000a0000-0x000bffff window]
[    0.263026] pci_bus 0000:00: root bus resource [mem 0xd0000000-0xfebfffff window]
[    0.263030] pci_bus 0000:00: root bus resource [bus 00-ff]
[    0.263048] pci 0000:00:00.0: [8086:3590] type 00 class 0x060000
[    0.263228] pci 0000:00:02.0: [8086:3595] type 01 class 0x060400
[    0.263305] pci 0000:00:02.0: PME# supported from D0 D3hot D3cold
[    0.263368] pci 0000:00:02.0: System wakeup disabled by ACPI
[    0.263445] pci 0000:00:04.0: [8086:3597] type 01 class 0x060400
[    0.263519] pci 0000:00:04.0: PME# supported from D0 D3hot D3cold
[    0.263577] pci 0000:00:04.0: System wakeup disabled by ACPI
[    0.263651] pci 0000:00:05.0: [8086:3598] type 01 class 0x060400
[    0.263725] pci 0000:00:05.0: PME# supported from D0 D3hot D3cold
[    0.263786] pci 0000:00:05.0: System wakeup disabled by ACPI
[    0.263856] pci 0000:00:06.0: [8086:3599] type 01 class 0x060400
[    0.263930] pci 0000:00:06.0: PME# supported from D0 D3hot D3cold
[    0.264002] pci 0000:00:06.0: System wakeup disabled by ACPI
[    0.264098] pci 0000:00:1d.0: [8086:24d2] type 00 class 0x0c0300
[    0.264148] pci 0000:00:1d.0: reg 0x20: [io  0xbce0-0xbcff]
[    0.264268] pci 0000:00:1d.1: [8086:24d4] type 00 class 0x0c0300
[    0.264318] pci 0000:00:1d.1: reg 0x20: [io  0xbcc0-0xbcdf]
[    0.264432] pci 0000:00:1d.2: [8086:24d7] type 00 class 0x0c0300
[    0.264481] pci 0000:00:1d.2: reg 0x20: [io  0xbca0-0xbcbf]
[    0.264610] pci 0000:00:1d.7: [8086:24dd] type 00 class 0x0c0320
[    0.264632] pci 0000:00:1d.7: reg 0x10: [mem 0xdff00000-0xdff003ff]
[    0.264736] pci 0000:00:1d.7: PME# supported from D0 D3hot D3cold
[    0.264838] pci 0000:00:1e.0: [8086:244e] type 01 class 0x060400
[    0.264983] pci 0000:00:1f.0: [8086:24d0] type 00 class 0x060100
[    0.265062] pci 0000:00:1f.0: quirk: [io  0x0800-0x087f] claimed by ICH4 ACPI/GPIO/TCO
[    0.265067] pci 0000:00:1f.0: quirk: [io  0x0880-0x08bf] claimed by ICH4 GPIO
[    0.265177] pci 0000:00:1f.1: [8086:24db] type 00 class 0x01018a
[    0.265193] pci 0000:00:1f.1: reg 0x10: [io  0x0000-0x0007]
[    0.265204] pci 0000:00:1f.1: reg 0x14: [io  0x0000-0x0003]
[    0.265214] pci 0000:00:1f.1: reg 0x18: [io  0x0000-0x0007]
[    0.265225] pci 0000:00:1f.1: reg 0x1c: [io  0x0000-0x0003]
[    0.265236] pci 0000:00:1f.1: reg 0x20: [io  0xfc00-0xfc0f]
[    0.265247] pci 0000:00:1f.1: reg 0x24: [mem 0x00000000-0x000003ff]
[    0.265262] pci 0000:00:1f.1: legacy IDE quirk: reg 0x10: [io  0x01f0-0x01f7]
[    0.265264] pci 0000:00:1f.1: legacy IDE quirk: reg 0x14: [io  0x03f6]
[    0.265266] pci 0000:00:1f.1: legacy IDE quirk: reg 0x18: [io  0x0170-0x0177]
[    0.265269] pci 0000:00:1f.1: legacy IDE quirk: reg 0x1c: [io  0x0376]
[    0.265483] pci 0000:01:00.0: [8086:0330] type 01 class 0x060400
[    0.265564] pci 0000:01:00.0: PME# supported from D0 D3hot D3cold
[    0.265673] pci 0000:01:00.2: [8086:0332] type 01 class 0x060400
[    0.265755] pci 0000:01:00.2: PME# supported from D0 D3hot D3cold
[    0.265860] pci 0000:01:00.0: disabling ASPM on pre-1.1 PCIe device.  You can enable it with 'pcie_aspm=force'
[    0.265872] pci 0000:00:02.0: PCI bridge to [bus 01-03]
[    0.265879] pci 0000:00:02.0:   bridge window [mem 0xdfc00000-0xdfefffff]
[    0.265886] pci 0000:00:02.0:   bridge window [mem 0xd8000000-0xd80fffff 64bit pref]
[    0.265982] pci 0000:02:0e.0: [1028:0013] type 00 class 0x010400
[    0.266010] pci 0000:02:0e.0: reg 0x10: [mem 0xd80f0000-0xd80fffff pref]
[    0.266032] pci 0000:02:0e.0: reg 0x18: [mem 0xdfde0000-0xdfdfffff]
[    0.266076] pci 0000:02:0e.0: reg 0x30: [mem 0xdfe00000-0xdfe1ffff pref]
[    0.266135] pci 0000:02:0e.0: supports D1
[    0.266217] pci 0000:01:00.0: PCI bridge to [bus 02]
[    0.266224] pci 0000:01:00.0:   bridge window [mem 0xdfd00000-0xdfefffff]
[    0.266231] pci 0000:01:00.0:   bridge window [mem 0xd8000000-0xd80fffff 64bit pref]
[    0.266324] pci 0000:01:00.2: PCI bridge to [bus 03]
[    0.266737] acpiphp: Slot [0] registered
[    0.266797] pci 0000:00:04.0: PCI bridge to [bus 04]
[    0.266942] pci 0000:05:00.0: [8086:0329] type 01 class 0x060400
[    0.266951] pci 0000:05:00.0: PXH quirk detected; SHPC device MSI disabled
[    0.267032] pci 0000:05:00.0: PME# supported from D0 D3hot D3cold
[    0.267151] pci 0000:05:00.2: [8086:032a] type 01 class 0x060400
[    0.267158] pci 0000:05:00.2: PXH quirk detected; SHPC device MSI disabled
[    0.267238] pci 0000:05:00.2: PME# supported from D0 D3hot D3cold
[    0.267344] pci 0000:05:00.0: disabling ASPM on pre-1.1 PCIe device.  You can enable it with 'pcie_aspm=force'
[    0.267355] pci 0000:00:05.0: PCI bridge to [bus 05-07]
[    0.267360] pci 0000:00:05.0:   bridge window [io  0xd000-0xefff]
[    0.267364] pci 0000:00:05.0:   bridge window [mem 0xdf700000-0xdfbfffff]
[    0.267449] pci 0000:06:07.0: [8086:1076] type 00 class 0x020000
[    0.267470] pci 0000:06:07.0: reg 0x10: [mem 0xdfae0000-0xdfafffff]
[    0.267489] pci 0000:06:07.0: reg 0x18: [io  0xecc0-0xecff]
[    0.267566] pci 0000:06:07.0: PME# supported from D0 D3hot D3cold
[    0.267662] pci 0000:05:00.0: PCI bridge to [bus 06]
[    0.267667] pci 0000:05:00.0:   bridge window [io  0xe000-0xefff]
[    0.267672] pci 0000:05:00.0:   bridge window [mem 0xdfa00000-0xdfbfffff]
[    0.267760] pci 0000:07:08.0: [8086:1076] type 00 class 0x020000
[    0.267781] pci 0000:07:08.0: reg 0x10: [mem 0xdf8e0000-0xdf8fffff]
[    0.267799] pci 0000:07:08.0: reg 0x18: [io  0xdcc0-0xdcff]
[    0.267876] pci 0000:07:08.0: PME# supported from D0 D3hot D3cold
[    0.267979] pci 0000:05:00.2: PCI bridge to [bus 07]
[    0.267984] pci 0000:05:00.2:   bridge window [io  0xd000-0xdfff]
[    0.267989] pci 0000:05:00.2:   bridge window [mem 0xdf800000-0xdf9fffff]
[    0.268397] acpiphp: Slot [0-2] registered
[    0.268459] pci 0000:00:06.0: PCI bridge to [bus 08]
[    0.268559] pci 0000:09:0d.0: [1002:5159] type 00 class 0x030000
[    0.268578] pci 0000:09:0d.0: reg 0x10: [mem 0xd0000000-0xd7ffffff pref]
[    0.268589] pci 0000:09:0d.0: reg 0x14: [io  0xcc00-0xccff]
[    0.268600] pci 0000:09:0d.0: reg 0x18: [mem 0xdf5f0000-0xdf5fffff]
[    0.268634] pci 0000:09:0d.0: reg 0x30: [mem 0x00000000-0x0001ffff pref]
[    0.268670] pci 0000:09:0d.0: supports D1 D2
[    0.268768] pci 0000:00:1e.0: PCI bridge to [bus 09] (subtractive decode)
[    0.268774] pci 0000:00:1e.0:   bridge window [io  0xc000-0xcfff]
[    0.268779] pci 0000:00:1e.0:   bridge window [mem 0xdf500000-0xdf6fffff]
[    0.268784] pci 0000:00:1e.0:   bridge window [mem 0xd0000000-0xd7ffffff pref]
[    0.268788] pci 0000:00:1e.0:   bridge window [io  0x0000-0x0cf7 window] (subtractive decode)
[    0.268790] pci 0000:00:1e.0:   bridge window [io  0x0d00-0xffff window] (subtractive decode)
[    0.268793] pci 0000:00:1e.0:   bridge window [mem 0x000a0000-0x000bffff window] (subtractive decode)
[    0.268796] pci 0000:00:1e.0:   bridge window [mem 0xd0000000-0xfebfffff window] (subtractive decode)
[    0.268826] pci_bus 0000:00: on NUMA node 0
[    0.271197] ACPI: PCI Interrupt Link [LNKA] (IRQs 3 4 5 6 7 10 *11 12)
[    0.271329] ACPI: PCI Interrupt Link [LNKB] (IRQs *3 4 5 6 7 10 11 12)
[    0.271460] ACPI: PCI Interrupt Link [LNKC] (IRQs 3 4 5 6 *7 10 11 12)
[    0.271591] ACPI: PCI Interrupt Link [LNKD] (IRQs 3 4 5 6 7 *10 11 12)
[    0.271725] ACPI: PCI Interrupt Link [LNKE] (IRQs 3 4 5 6 7 10 11 12) *0, disabled.
[    0.271860] ACPI: PCI Interrupt Link [LNKF] (IRQs 3 4 5 6 7 10 11 12) *0, disabled.
[    0.272010] ACPI: PCI Interrupt Link [LNKG] (IRQs 3 4 5 6 7 10 11 12) *0, disabled.
[    0.272146] ACPI: PCI Interrupt Link [LNKH] (IRQs 3 4 *5 6 7 10 11 12)
[    0.272243] ACPI: Enabled 1 GPEs in block 00 to 1F
[    0.272488] pci 0000:09:0d.0: vgaarb: setting as boot VGA device
[    0.272491] pci 0000:09:0d.0: vgaarb: VGA device added: decodes=io+mem,owns=io+mem,locks=none
[    0.272494] pci 0000:09:0d.0: vgaarb: bridge control possible
[    0.272495] vgaarb: loaded
[    0.272743] SCSI subsystem initialized
[    0.272848] libata version 3.00 loaded.
[    0.272909] ACPI: bus type USB registered
[    0.272952] usbcore: registered new interface driver usbfs
[    0.272972] usbcore: registered new interface driver hub
[    0.273032] usbcore: registered new device driver usb
[    0.273190] EDAC MC: Ver: 3.0.0
[    0.273469] PCI: Using ACPI for IRQ routing
[    0.281871] PCI: pci_cache_line_size set to 64 bytes
[    0.281941] Expanded resource Reserved due to conflict with PCI Bus 0000:00
[    0.281945] e820: reserve RAM buffer [mem 0xcffc0000-0xcfffffff]
[    0.282155] NetLabel: Initializing
[    0.282157] NetLabel:  domain hash size = 128
[    0.282158] NetLabel:  protocols = UNLABELED CIPSOv4 CALIPSO
[    0.282184] NetLabel:  unlabeled traffic allowed by default
[    0.282474] HPET: 3 timers in total, 0 timers will be used for per-cpu timer
[    0.282481] hpet0: at MMIO 0xfed00000, IRQs 2, 8, 0
[    0.282488] hpet0: 3 comparators, 64-bit 14.318180 MHz counter
[    0.284743] clocksource: Switched to clocksource hpet
[    0.311365] VFS: Disk quotas dquot_6.6.0
[    0.311404] VFS: Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
[    0.311578] pnp: PnP ACPI init
[    0.311781] pnp 00:00: Plug and Play ACPI device, IDs PNP0b00 (active)
[    0.312111] pnp 00:01: [dma 2]
[    0.312212] pnp 00:01: Plug and Play ACPI device, IDs PNP0700 (active)
[    0.312837] pnp 00:02: Plug and Play ACPI device, IDs PNP0303 (active)
[    0.313936] pnp 00:03: Plug and Play ACPI device, IDs PNP0f13 (active)
[    0.314225] pnp 00:04: Plug and Play ACPI device, IDs PNP0501 (active)
[    0.314428] system 00:05: [io  0x0800-0x087f] has been reserved
[    0.314432] system 00:05: [io  0x0880-0x08bf] has been reserved
[    0.314435] system 00:05: [io  0x08c0-0x08df] has been reserved
[    0.314439] system 00:05: [io  0x0c00-0x0c0f] has been reserved
[    0.314442] system 00:05: [io  0x0c10-0x0c1f] has been reserved
[    0.314445] system 00:05: [io  0x0ca0-0x0caf] has been reserved
[    0.314448] system 00:05: [io  0x0c20-0x0c3f] has been reserved
[    0.314455] system 00:05: Plug and Play ACPI device, IDs PNP0c01 (active)
[    0.315216] system 00:06: [mem 0xe0000000-0xefffffff] has been reserved
[    0.315223] system 00:06: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.315529] pnp: PnP ACPI: found 7 devices
[    0.354203] clocksource: acpi_pm: mask: 0xffffff max_cycles: 0xffffff, max_idle_ns: 2085701024 ns
[    0.354290] pci 0000:00:1f.1: BAR 5: assigned [mem 0xd8100000-0xd81003ff]
[    0.354299] pci 0000:01:00.0: PCI bridge to [bus 02]
[    0.354305] pci 0000:01:00.0:   bridge window [mem 0xdfd00000-0xdfefffff]
[    0.354310] pci 0000:01:00.0:   bridge window [mem 0xd8000000-0xd80fffff 64bit pref]
[    0.354316] pci 0000:01:00.2: PCI bridge to [bus 03]
[    0.354327] pci 0000:00:02.0: PCI bridge to [bus 01-03]
[    0.354333] pci 0000:00:02.0:   bridge window [mem 0xdfc00000-0xdfefffff]
[    0.354337] pci 0000:00:02.0:   bridge window [mem 0xd8000000-0xd80fffff 64bit pref]
[    0.354344] pci 0000:00:04.0: PCI bridge to [bus 04]
[    0.354356] pci 0000:05:00.0: PCI bridge to [bus 06]
[    0.354359] pci 0000:05:00.0:   bridge window [io  0xe000-0xefff]
[    0.354365] pci 0000:05:00.0:   bridge window [mem 0xdfa00000-0xdfbfffff]
[    0.354373] pci 0000:05:00.2: PCI bridge to [bus 07]
[    0.354377] pci 0000:05:00.2:   bridge window [io  0xd000-0xdfff]
[    0.354382] pci 0000:05:00.2:   bridge window [mem 0xdf800000-0xdf9fffff]
[    0.354390] pci 0000:00:05.0: PCI bridge to [bus 05-07]
[    0.354394] pci 0000:00:05.0:   bridge window [io  0xd000-0xefff]
[    0.354399] pci 0000:00:05.0:   bridge window [mem 0xdf700000-0xdfbfffff]
[    0.354408] pci 0000:00:06.0: PCI bridge to [bus 08]
[    0.354422] pci 0000:09:0d.0: BAR 6: assigned [mem 0xdf500000-0xdf51ffff pref]
[    0.354425] pci 0000:00:1e.0: PCI bridge to [bus 09]
[    0.354429] pci 0000:00:1e.0:   bridge window [io  0xc000-0xcfff]
[    0.354435] pci 0000:00:1e.0:   bridge window [mem 0xdf500000-0xdf6fffff]
[    0.354440] pci 0000:00:1e.0:   bridge window [mem 0xd0000000-0xd7ffffff pref]
[    0.354449] pci_bus 0000:00: resource 4 [io  0x0000-0x0cf7 window]
[    0.354451] pci_bus 0000:00: resource 5 [io  0x0d00-0xffff window]
[    0.354454] pci_bus 0000:00: resource 6 [mem 0x000a0000-0x000bffff window]
[    0.354457] pci_bus 0000:00: resource 7 [mem 0xd0000000-0xfebfffff window]
[    0.354460] pci_bus 0000:01: resource 1 [mem 0xdfc00000-0xdfefffff]
[    0.354462] pci_bus 0000:01: resource 2 [mem 0xd8000000-0xd80fffff 64bit pref]
[    0.354465] pci_bus 0000:02: resource 1 [mem 0xdfd00000-0xdfefffff]
[    0.354467] pci_bus 0000:02: resource 2 [mem 0xd8000000-0xd80fffff 64bit pref]
[    0.354470] pci_bus 0000:05: resource 0 [io  0xd000-0xefff]
[    0.354473] pci_bus 0000:05: resource 1 [mem 0xdf700000-0xdfbfffff]
[    0.354476] pci_bus 0000:06: resource 0 [io  0xe000-0xefff]
[    0.354478] pci_bus 0000:06: resource 1 [mem 0xdfa00000-0xdfbfffff]
[    0.354481] pci_bus 0000:07: resource 0 [io  0xd000-0xdfff]
[    0.354483] pci_bus 0000:07: resource 1 [mem 0xdf800000-0xdf9fffff]
[    0.354486] pci_bus 0000:09: resource 0 [io  0xc000-0xcfff]
[    0.354489] pci_bus 0000:09: resource 1 [mem 0xdf500000-0xdf6fffff]
[    0.354491] pci_bus 0000:09: resource 2 [mem 0xd0000000-0xd7ffffff pref]
[    0.354494] pci_bus 0000:09: resource 4 [io  0x0000-0x0cf7 window]
[    0.354496] pci_bus 0000:09: resource 5 [io  0x0d00-0xffff window]
[    0.354499] pci_bus 0000:09: resource 6 [mem 0x000a0000-0x000bffff window]
[    0.354501] pci_bus 0000:09: resource 7 [mem 0xd0000000-0xfebfffff window]
[    0.354648] NET: Registered protocol family 2
[    0.354985] TCP established hash table entries: 8192 (order: 3, 32768 bytes)
[    0.355007] TCP bind hash table entries: 8192 (order: 4, 65536 bytes)
[    0.355042] TCP: Hash tables configured (established 8192 bind 8192)
[    0.355097] UDP hash table entries: 512 (order: 2, 16384 bytes)
[    0.355106] UDP-Lite hash table entries: 512 (order: 2, 16384 bytes)
[    0.355192] NET: Registered protocol family 1
[    0.355221] pci_bus 0000:01: writes to ASPM control bits will be ignored
[    0.355230] pci_bus 0000:05: writes to ASPM control bits will be ignored
[    0.356502] pci 0000:01:00.0: rerouting interrupts for [8086:0330]
[    0.356511] pci 0000:01:00.2: rerouting interrupts for [8086:0332]
[    0.356521] pci 0000:05:00.0: rerouting interrupts for [8086:0329]
[    0.356527] pci 0000:05:00.2: rerouting interrupts for [8086:032a]
[    0.356547] pci 0000:09:0d.0: Video device with shadowed ROM at [mem 0x000c0000-0x000dffff]
[    0.356551] PCI: CLS 64 bytes, default 64
[    0.356647] Unpacking initramfs...
[    1.088433] Freeing initrd memory: 22772K
[    1.089651] apm: BIOS not found.
[    1.090737] Initialise system trusted keyrings
[    1.090779] Key type blacklist registered
[    1.090849] workingset: timestamp_bits=14 max_order=22 bucket_order=8
[    1.093649] zbud: loaded
[    1.094730] SELinux:  Registering netfilter hooks
[    2.144789] tsc: Refined TSC clocksource calibration: 2792.999 MHz
[    2.144798] clocksource: tsc: mask: 0xffffffffffffffff max_cycles: 0x28426b16f90, max_idle_ns: 440795205097 ns
[    2.693345] NET: Registered protocol family 38
[    2.693353] Key type asymmetric registered
[    2.693356] Asymmetric key parser 'x509' registered
[    2.693383] bounce: pool size: 64 pages
[    2.693425] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 248)
[    2.693507] io scheduler noop registered
[    2.693510] io scheduler deadline registered
[    2.693675] io scheduler cfq registered (default)
[    2.693677] io scheduler mq-deadline registered
[    2.693872] atomic64_test: passed for i586+ platform with CX8 and with SSE
[    2.695186] input: Power Button as /devices/LNXSYSTM:00/LNXPWRBN:00/input/input0
[    2.695192] ACPI: Power Button [PWRF]
[    2.695607] GHES: HEST is not enabled!
[    2.695837] Serial: 8250/16550 driver, 32 ports, IRQ sharing enabled
[    2.716358] 00:04: ttyS0 at I/O 0x3f8 (irq = 4, base_baud = 115200) is a 16550A
[    2.720848] Non-volatile memory driver v1.3
[    2.720910] Linux agpgart interface v0.103
[    2.721713] ata_piix 0000:00:1f.1: version 2.13
[    2.721728] ata_piix 0000:00:1f.1: enabling device (0005 -> 0007)
[    2.721944] ata_piix 0000:00:1f.1: can't derive routing for PCI INT A
[    2.722546] scsi host0: ata_piix
[    2.722747] scsi host1: ata_piix
[    2.722857] ata1: PATA max UDMA/100 cmd 0x1f0 ctl 0x3f6 bmdma 0xfc00 irq 14
[    2.722860] ata2: PATA max UDMA/100 cmd 0x170 ctl 0x376 bmdma 0xfc08 irq 15
[    2.723016] libphy: Fixed MDIO Bus: probed
[    2.723166] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    2.723172] ehci-pci: EHCI PCI platform driver
[    2.723436] ehci-pci 0000:00:1d.7: EHCI Host Controller
[    2.723519] ehci-pci 0000:00:1d.7: new USB bus registered, assigned bus number 1
[    2.723536] ehci-pci 0000:00:1d.7: debug port 1
[    2.727435] ehci-pci 0000:00:1d.7: cache line size of 64 is not supported
[    2.727462] ehci-pci 0000:00:1d.7: irq 23, io mem 0xdff00000
[    2.733802] ehci-pci 0000:00:1d.7: USB 2.0 started, EHCI 1.00
[    2.733894] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002
[    2.733898] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    2.733900] usb usb1: Product: EHCI Host Controller
[    2.733903] usb usb1: Manufacturer: Linux 4.12.8-300.fc26.i686+PAE ehci_hcd
[    2.733905] usb usb1: SerialNumber: 0000:00:1d.7
[    2.734121] hub 1-0:1.0: USB hub found
[    2.734133] hub 1-0:1.0: 6 ports detected
[    2.734401] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    2.734408] ohci-pci: OHCI PCI platform driver
[    2.734430] uhci_hcd: USB Universal Host Controller Interface driver
[    2.734636] uhci_hcd 0000:00:1d.0: UHCI Host Controller
[    2.734735] uhci_hcd 0000:00:1d.0: new USB bus registered, assigned bus number 2
[    2.734742] uhci_hcd 0000:00:1d.0: detected 2 ports
[    2.734792] uhci_hcd 0000:00:1d.0: irq 16, io base 0x0000bce0
[    2.734888] usb usb2: New USB device found, idVendor=1d6b, idProduct=0001
[    2.734891] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    2.734894] usb usb2: Product: UHCI Host Controller
[    2.734896] usb usb2: Manufacturer: Linux 4.12.8-300.fc26.i686+PAE uhci_hcd
[    2.734898] usb usb2: SerialNumber: 0000:00:1d.0
[    2.735095] hub 2-0:1.0: USB hub found
[    2.735107] hub 2-0:1.0: 2 ports detected
[    2.735457] uhci_hcd 0000:00:1d.1: UHCI Host Controller
[    2.735543] uhci_hcd 0000:00:1d.1: new USB bus registered, assigned bus number 3
[    2.735551] uhci_hcd 0000:00:1d.1: detected 2 ports
[    2.735579] uhci_hcd 0000:00:1d.1: irq 19, io base 0x0000bcc0
[    2.735664] usb usb3: New USB device found, idVendor=1d6b, idProduct=0001
[    2.735667] usb usb3: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    2.735669] usb usb3: Product: UHCI Host Controller
[    2.735671] usb usb3: Manufacturer: Linux 4.12.8-300.fc26.i686+PAE uhci_hcd
[    2.735673] usb usb3: SerialNumber: 0000:00:1d.1
[    2.735890] hub 3-0:1.0: USB hub found
[    2.735901] hub 3-0:1.0: 2 ports detected
[    2.736231] uhci_hcd 0000:00:1d.2: UHCI Host Controller
[    2.736323] uhci_hcd 0000:00:1d.2: new USB bus registered, assigned bus number 4
[    2.736333] uhci_hcd 0000:00:1d.2: detected 2 ports
[    2.736360] uhci_hcd 0000:00:1d.2: irq 18, io base 0x0000bca0
[    2.736446] usb usb4: New USB device found, idVendor=1d6b, idProduct=0001
[    2.736450] usb usb4: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    2.736452] usb usb4: Product: UHCI Host Controller
[    2.736454] usb usb4: Manufacturer: Linux 4.12.8-300.fc26.i686+PAE uhci_hcd
[    2.736456] usb usb4: SerialNumber: 0000:00:1d.2
[    2.736648] hub 4-0:1.0: USB hub found
[    2.736659] hub 4-0:1.0: 2 ports detected
[    2.736917] usbcore: registered new interface driver usbserial
[    2.736931] usbcore: registered new interface driver usbserial_generic
[    2.736943] usbserial: USB Serial support registered for generic
[    2.737014] i8042: PNP: PS/2 Controller [PNP0303:KBD,PNP0f13:MOU] at 0x60,0x64 irq 1,12
[    2.739986] serio: i8042 KBD port at 0x60,0x64 irq 1
[    2.739995] serio: i8042 AUX port at 0x60,0x64 irq 12
[    2.740193] mousedev: PS/2 mouse device common for all mice
[    2.740419] rtc_cmos 00:00: RTC can wake from S4
[    2.740592] rtc_cmos 00:00: rtc core: registered rtc_cmos as rtc0
[    2.740619] rtc_cmos 00:00: alarms up to one day, y3k, 242 bytes nvram, hpet irqs
[    2.740786] device-mapper: uevent: version 1.0.3
[    2.740946] device-mapper: ioctl: 4.35.0-ioctl (2016-06-23) initialised: dm-devel@redhat.com
[    2.741871] hidraw: raw HID events driver (C) Jiri Kosina
[    2.741972] usbcore: registered new interface driver usbhid
[    2.741973] usbhid: USB HID core driver
[    2.742151] drop_monitor: Initializing network drop monitor service
[    2.742276] ip_tables: (C) 2000-2006 Netfilter Core Team
[    2.742363] Initializing XFRM netlink socket
[    2.742626] NET: Registered protocol family 10
[    2.747505] Segment Routing with IPv6
[    2.747537] mip6: Mobile IPv6
[    2.747540] NET: Registered protocol family 17
[    2.748166] RAS: Correctable Errors collector initialized.
[    2.748223] microcode: sig=0xf41, pf=0x1, revision=0x17
[    2.748308] microcode: Microcode Update Driver: v2.2.
[    2.748316] Using IPI No-Shortcut mode
[    2.748568] registered taskstats version 1
[    2.748582] Loading compiled-in X.509 certificates
[    2.752572] alg: No test for pkcs1pad(rsa,sha256) (pkcs1pad(rsa-generic,sha256))
[    2.760133] Loaded X.509 cert 'Fedora kernel signing key: a374a2c5c548ec1d8b0ab2037efcca9800eaa639'
[    2.760186] zswap: loaded using pool lzo/zbud
[    2.777329] input: AT Translated Set 2 keyboard as /devices/platform/i8042/serio0/input/input1
[    2.788565] Key type big_key registered
[    2.792933] Key type encrypted registered
[    2.793318]   Magic number: 13:608:288
[    2.793372] tty tty21: hash matches
[    2.793454] rtc_cmos 00:00: setting system clock to 2017-08-29 16:15:19 UTC (1504023319)
[    2.793516] PM: Hibernation image not present or could not be loaded.
[    2.883403] ata1.00: ATAPI: TEAC CD-ROM CD-224E, K.9A, max UDMA/33
[    2.888018] ata1.00: configured for UDMA/33
[    2.890562] scsi 0:0:0:0: CD-ROM            TEAC     CD-224E          K.9A PQ: 0 ANSI: 5
[    2.904339] sr 0:0:0:0: [sr0] scsi3-mmc drive: 24x/24x cd/rw xa/form2 cdda tray
[    2.904343] cdrom: Uniform CD-ROM driver Revision: 3.20
[    2.904593] sr 0:0:0:0: Attached scsi CD-ROM sr0
[    2.904754] sr 0:0:0:0: Attached scsi generic sg0 type 5
[    2.907096] Freeing unused kernel memory: 912K
[    2.907212] Write protecting the kernel text: 7764k
[    2.907270] Write protecting the kernel read-only data: 3088k
[    2.907272] NX-protecting the kernel data: 6572k
[    2.907530] x86/mm: Checked W+X mappings: passed, no W+X pages found.
[    2.907537] rodata_test: all tests were successful
[    2.918565] random: systemd: uninitialized urandom read (16 bytes read)
[    2.919177] random: systemd: uninitialized urandom read (16 bytes read)
[    2.922956] systemd[1]: systemd 233 running in system mode. (+PAM +AUDIT +SELINUX +IMA -APPARMOR +SMACK +SYSVINIT +UTMP +LIBCRYPTSETUP +GCRYPT +GNUTLS +ACL +XZ +LZ4 +SECCOMP +BLKID +ELFUTILS +KMOD +IDN default-hierarchy=hybrid)
[    2.923288] systemd[1]: Detected architecture x86.
[    2.923296] systemd[1]: Running in initial RAM disk.
[    2.923337] systemd[1]: Set hostname to <>.
[    3.016343] random: systemd: uninitialized urandom read (16 bytes read)
[    3.016436] random: systemd: uninitialized urandom read (16 bytes read)
[    3.016606] random: systemd: uninitialized urandom read (16 bytes read)
[    3.019122] random: systemd: uninitialized urandom read (16 bytes read)
[    3.019972] random: systemd: uninitialized urandom read (16 bytes read)
[    3.021382] random: systemd: uninitialized urandom read (16 bytes read)
[    3.021479] random: systemd: uninitialized urandom read (16 bytes read)
[    3.022347] random: systemd: uninitialized urandom read (16 bytes read)
[    3.036563] systemd[1]: Reached target Timers.
[    3.036813] systemd[1]: Listening on udev Control Socket.
[    3.036902] systemd[1]: Listening on udev Kernel Socket.
[    3.037026] systemd[1]: Listening on Journal Socket (/dev/log).
[    3.037074] systemd[1]: Reached target Local File Systems.
[    3.038147] systemd[1]: Created slice System Slice.
[    3.048838] usb 1-3: new high-speed USB device number 2 using ehci-pci
[    3.153024] clocksource: Switched to clocksource tsc
[    3.168209] usb 1-3: New USB device found, idVendor=413c, idProduct=a001
[    3.168216] usb 1-3: New USB device strings: Mfr=0, Product=0, SerialNumber=0
[    3.168671] hub 1-3:1.0: USB hub found
[    3.168830] hub 1-3:1.0: 2 ports detected
[    3.653788] megaraid cmm: 2.20.2.7 (Release Date: Sun Jul 16 00:01:03 EST 2006)
[    3.673165] megaraid: 2.20.5.1 (Release Date: Thu Nov 16 15:32:35 EST 2006)
[    3.673234] megaraid: probe new device 0x1028:0x0013:0x1028:0x016c: 
[    3.673238] bus 2:slot 14:func 0
[    3.673528] megaraid 0000:02:0e.0: PCI IRQ 46 -> rerouted to legacy IRQ 18
[    3.685662] e1000: Intel(R) PRO/1000 Network Driver - version 7.3.21-k8-NAPI
[    3.685666] e1000: Copyright (c) 1999-2006 Intel Corporation.
[    3.685708] megaraid: fw version:[5B2D] bios version:[H435]
[    3.685902] e1000 0000:06:07.0: PCI IRQ 64 -> rerouted to legacy IRQ 16
[    3.693491] scsi host2: LSI Logic MegaRAID driver
[    3.693996] scsi[2]: scanning scsi channel 0 [Phy 0]
[    3.693999]  for non-raid devices
[    3.837881] input: ImExPS/2 Generic Explorer Mouse as /devices/platform/i8042/serio1/input/input3
[    3.896244] e1000 0000:06:07.0 eth0: (PCI:66MHz:32-bit) 00:11:43:31:c4:86
[    3.896258] e1000 0000:06:07.0 eth0: Intel(R) PRO/1000 Network Connection
[    3.898515] e1000 0000:07:08.0: PCI IRQ 65 -> rerouted to legacy IRQ 17
[    4.003618] [drm] radeon kernel modesetting enabled.
[    4.004479] [drm] initializing kernel modesetting (RV100 0x1002:0x5159 0x1028:0x016C 0x00).
[    4.004666] radeon 0000:09:0d.0: VRAM: 128M 0x00000000D0000000 - 0x00000000D7FFFFFF (16M used)
[    4.004672] radeon 0000:09:0d.0: GTT: 512M 0x00000000B0000000 - 0x00000000CFFFFFFF
[    4.004690] [drm] Detected VRAM RAM=128M, BAR=128M
[    4.004692] [drm] RAM width 32bits DDR
[    4.004876] [TTM] Zone  kernel: Available graphics memory: 392430 kiB
[    4.004878] [TTM] Zone highmem: Available graphics memory: 5180530 kiB
[    4.004879] [TTM] Initializing pool allocator
[    4.004888] [TTM] Initializing DMA pool allocator
[    4.004946] [drm] radeon: 16M of VRAM memory ready
[    4.004948] [drm] radeon: 512M of GTT memory ready.
[    4.004977] [drm] GART: num cpu pages 131072, num gpu pages 131072
[    4.026710] [drm] PCI GART of 512M enabled (table at 0x0000000036680000).
[    4.026770] radeon 0000:09:0d.0: WB disabled
[    4.026776] radeon 0000:09:0d.0: fence driver on ring 0 use gpu addr 0x00000000b0000000 and cpu addr 0xf65aa000
[    4.026779] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[    4.026780] [drm] Driver supports precise vblank timestamp query.
[    4.026825] [drm] radeon: irq initialized.
[    4.026844] [drm] Loading R100 Microcode
[    4.027127] [drm] radeon: ring at 0x00000000B0001000
[    4.027155] [drm] ring test succeeded in 1 usecs
[    4.027379] [drm] ib test succeeded in 0 usecs
[    4.027977] [drm] No TV DAC info found in BIOS
[    4.028150] [drm] Radeon Display Connectors
[    4.028152] [drm] Connector 0:
[    4.028154] [drm]   VGA-1
[    4.028158] [drm]   DDC: 0x60 0x60 0x60 0x60 0x60 0x60 0x60 0x60
[    4.028159] [drm]   Encoders:
[    4.028161] [drm]     CRT1: INTERNAL_DAC1
[    4.028164] [drm] Connector 1:
[    4.028165] [drm]   VGA-2
[    4.028169] [drm]   DDC: 0x6c 0x6c 0x6c 0x6c 0x6c 0x6c 0x6c 0x6c
[    4.028172] [drm]   Encoders:
[    4.028174] [drm]     CRT2: INTERNAL_DAC2
[    4.028176] [drm] Connector 2:
[    4.028177] [drm]   DVI-I-1
[    4.028179] [drm]   HPD1
[    4.028182] [drm]   DDC: 0x64 0x64 0x64 0x64 0x64 0x64 0x64 0x64
[    4.028183] [drm]   Encoders:
[    4.028185] [drm]     CRT2: INTERNAL_DAC2
[    4.028187] [drm]     DFP1: INTERNAL_TMDS1
[    4.106399] e1000 0000:07:08.0 eth1: (PCI:66MHz:32-bit) 00:11:43:31:c4:87
[    4.106413] e1000 0000:07:08.0 eth1: Intel(R) PRO/1000 Network Connection
[    4.106896] [drm] fb mappable at 0xD0040000
[    4.106904] [drm] vram apper at 0xD0000000
[    4.106905] [drm] size 786432
[    4.106907] [drm] fb depth is 8
[    4.106908] [drm]    pitch is 1024
[    4.107049] fbcon: radeondrmfb (fb0) is primary device
[    4.111247] e1000 0000:07:08.0 enp7s8: renamed from eth1
[    4.268256] Console: switching to colour frame buffer device 128x48
[    4.275542] radeon 0000:09:0d.0: fb0: radeondrmfb frame buffer device
[    4.280136] [drm] Initialized radeon 2.50.0 20080528 for 0000:09:0d.0 on minor 0
[    4.280377] e1000 0000:06:07.0 enp6s7: renamed from eth0
[    4.712273] scsi 2:0:6:0: Processor         PE/PV    1x2 SCSI BP      1.0  PQ: 0 ANSI: 2
[    6.725187] scsi[2]: scanning scsi channel 1
[    6.725191]  [virtual] for logical drives
[    6.725379] scsi 2:1:0:0: Direct-Access     MegaRAID LD 0 RAID1   69G 5B2D PQ: 0 ANSI: 2
[    6.737626] scsi 2:0:6:0: Attached scsi generic sg1 type 3
[    6.738015] sd 2:1:0:0: [sda] 143114240 512-byte logical blocks: (73.3 GB/68.2 GiB)
[    6.738048] sd 2:1:0:0: [sda] Write Protect is off
[    6.738053] sd 2:1:0:0: [sda] Mode Sense: 00 00 00 00
[    6.738080] sd 2:1:0:0: [sda] Asking for cache data failed
[    6.738191] sd 2:1:0:0: [sda] Assuming drive cache: write through
[    6.741137] sd 2:1:0:0: Attached scsi generic sg2 type 0
[    6.741516]  sda: sda1 sda2
[    6.742097] sd 2:1:0:0: [sda] Attached SCSI disk
[    6.782386] random: fast init done
[    7.361908] EXT4-fs (dm-0): mounted filesystem with ordered data mode. Opts: (null)
[    8.043687] systemd-journald[164]: Received SIGTERM from PID 1 (systemd).
[    8.063796] random: crng init done
[    8.237740] systemd: 16 output lines suppressed due to ratelimiting
[    9.085388] SELinux:  Disabled at runtime.
[    9.085451] SELinux:  Unregistering netfilter hooks
[   11.550720] EXT4-fs (dm-0): re-mounted. Opts: (null)
[   11.808995] RPC: Registered named UNIX socket transport module.
[   11.808999] RPC: Registered udp transport module.
[   11.809000] RPC: Registered tcp transport module.
[   11.809001] RPC: Registered tcp NFSv4.1 backchannel transport module.
[   11.860827] systemd-journald[611]: Received request to flush runtime journal from PID 1
[   12.258492] Installing knfsd (copyright (C) 1996 okir@monad.swb.de).
[   13.535977] intel_rng: FWH not detected
[   13.537212] pci 0000:00:00.1: [8086:3591] type 00 class 0xff0000
[   13.537492] EDAC e752x: tolm = d0000, remapbase = 280000, remaplimit = 2ac000
[   13.538181] EDAC MC0: Giving out device to module e752x_edac controller E7520: DEV 0000:00:00.0 (POLLED)
[   13.538247] EDAC PCI0: Giving out device to module e752x_edac controller EDAC PCI controller: DEV 0000:00:00.0 (POLLED)
[   13.629582] ACPI: Video Device [EVGA] (multi-head: no  rom: yes  post: no)
[   13.629856] input: Video Bus as /devices/LNXSYSTM:00/LNXSYBUS:00/PNP0A03:00/device:20/LNXVIDEO:00/input/input4
[   13.860422] dcdbas dcdbas: Dell Systems Management Base Driver (version 5.6.0-3.2)
[   14.069258] ppdev: user-space parallel port driver
[   14.146570] iTCO_vendor_support: vendor-support=0
[   14.166208] iTCO_wdt: Intel TCO WatchDog Timer Driver v1.11
[   14.166286] iTCO_wdt: Found a ICH5 or ICH5R TCO device (Version=1, TCOBASE=0x0860)
[   14.166524] iTCO_wdt: initialized. heartbeat=30 sec (nowayout=0)
[   14.376185] Adding 2195452k swap on /dev/mapper/fedora-swap.  Priority:-1 extents:1 across:2195452k FS
[   14.821131] EXT4-fs (sda1): mounted filesystem with ordered data mode. Opts: (null)
[   15.909637] EXT4-fs (dm-2): mounted filesystem with ordered data mode. Opts: (null)
[   22.995830] ip6_tables: (C) 2000-2006 Netfilter Core Team
[   23.009812] ipmi message handler version 39.2
[   23.102479] ipmi device interface
[   23.180809] IPMI System Interface driver.
[   23.180875] ipmi_si: probing via SMBIOS
[   23.180880] ipmi_si: SMBIOS: io 0xca8 regsize 1 spacing 4 irq 0
[   23.180883] ipmi_si: Adding SMBIOS-specified kcs state machine
[   23.180891] ipmi_si: Trying SMBIOS-specified kcs state machine at i/o address 0xca8, slave address 0x20, irq 0
[   23.212204] Ebtables v2.0 registered
[   23.301439] ipmi_si ipmi_si.0: Found new BMC (man_id: 0x0002a2, prod_id: 0x0000, dev_id: 0x20)
[   23.301588] ipmi_si ipmi_si.0: IPMI kcs interface initialized
[   23.458303] nf_conntrack version 0.5.0 (65536 buckets, 262144 max)
[   23.971237] bridge: filtering via arp/ip/ip6tables is no longer available by default. Update your scripts to load br_netfilter if you need this.
[   24.172429] Netfilter messages via NETLINK v0.30.
[   24.195193] ip_set: protocol 6
[   24.363616] IPv6: ADDRCONF(NETDEV_UP): enp6s7: link is not ready
[   24.364558] e1000: enp6s7 NIC Link is Up 100 Mbps Full Duplex, Flow Control: RX
[   24.364628] IPv6: ADDRCONF(NETDEV_CHANGE): enp6s7: link becomes ready
[   32.791752] IPv6: ADDRCONF(NETDEV_UP): enp7s8: link is not ready
[   32.815086] e1000: enp7s8 NIC Link is Up 1000 Mbps Full Duplex, Flow Control: RX/TX
[   32.815230] IPv6: ADDRCONF(NETDEV_CHANGE): enp7s8: link becomes ready
[   40.420989] Loading iSCSI transport class v2.0-870.
[   40.796425] NFSD: starting 90-second grace period (net cab29400)
[   41.051739] iscsi: registered transport (tcp)
[   41.057879] scsi host3: iSCSI Initiator over TCP/IP
[   41.075107] scsi 3:0:0:0: Direct-Access     Promise  VessRAID 1840i   0306 PQ: 0 ANSI: 5
[   41.085837] sd 3:0:0:0: Attached scsi generic sg3 type 0
[   41.089932] sd 3:0:0:0: [sdb] 23437498368 512-byte logical blocks: (12.0 TB/10.9 TiB)
[   41.090344] sd 3:0:0:0: [sdb] Write Protect is off
[   41.090348] sd 3:0:0:0: [sdb] Mode Sense: a3 00 10 08
[   41.090929] sd 3:0:0:0: [sdb] Write cache: enabled, read cache: enabled, supports DPO and FUA
[   41.099707] sd 3:0:0:0: [sdb] Attached SCSI disk
[   43.465609] tun: Universal TUN/TAP device driver, 1.6
[   43.468947] virbr0: port 1(virbr0-nic) entered blocking state
[   43.468952] virbr0: port 1(virbr0-nic) entered disabled state
[   43.469046] device virbr0-nic entered promiscuous mode
[   43.826466] virbr0: port 1(virbr0-nic) entered blocking state
[   43.826475] virbr0: port 1(virbr0-nic) entered listening state
[   43.933771] virbr0: port 1(virbr0-nic) entered disabled state
[   46.913875] FS-Cache: Loaded
[   46.960225] FS-Cache: Netfs 'nfs' registered for caching
[   46.986025] Key type dns_resolver registered
[   47.050333] NFS: Registering the id_resolver key type
[   47.050351] Key type id_resolver registered
[   47.050352] Key type id_legacy registered
[  491.329611] usbcore: registered new interface driver usb-storage
[ 6593.843608] perf: interrupt took too long (2504 > 2500), lowering kernel.perf_event_max_sample_rate to 79000
[ 9696.048748] perf: interrupt took too long (3145 > 3130), lowering kernel.perf_event_max_sample_rate to 63000
[14523.778184] perf: interrupt took too long (3951 > 3931), lowering kernel.perf_event_max_sample_rate to 50000
[23190.625412] perf: interrupt took too long (4943 > 4938), lowering kernel.perf_event_max_sample_rate to 40000