[    0.000000] Linux version 3.14.4 (stephan@buildserver.fritz.box) (gcc version 4.9.0 (GCC) ) #1 SMP Mon May 19 10:03:40 CEST 2014
[    0.000000] Command line: BOOT_IMAGE=/KERNEL boot=LABEL=System disk=LABEL=Storage  ssh quiet
[    0.000000] e820: BIOS-provided physical RAM map:
[    0.000000] BIOS-e820: [mem 0x0000000000000000-0x000000000002ffff] usable
[    0.000000] BIOS-e820: [mem 0x0000000000030000-0x000000000003ffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000040000-0x000000000009fbff] usable
[    0.000000] BIOS-e820: [mem 0x000000000009fc00-0x000000000009ffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000000f0000-0x00000000000fffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000000100000-0x0000000000efffff] usable
[    0.000000] BIOS-e820: [mem 0x0000000000f00000-0x0000000000ffffff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000001000000-0x000000007bf70fff] usable
[    0.000000] BIOS-e820: [mem 0x000000007bf71000-0x000000007e9fffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000f0000000-0x00000000f3ffffff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed10000-0x00000000fed19fff] reserved
[    0.000000] BIOS-e820: [mem 0x00000000fed84000-0x00000000fed84fff] reserved
[    0.000000] BIOS-e820: [mem 0x0000000100000000-0x00000001005fffff] usable
[    0.000000] NX (Execute Disable) protection: active
[    0.000000] SMBIOS 2.7 present.
[    0.000000] DMI: GOOGLE Panther, BIOS          02/14/2014
[    0.000000] e820: update [mem 0x00000000-0x00000fff] usable ==> reserved
[    0.000000] e820: remove [mem 0x000a0000-0x000fffff] usable
[    0.000000] No AGP bridge found
[    0.000000] e820: last_pfn = 0x100600 max_arch_pfn = 0x400000000
[    0.000000] MTRR default type: uncachable
[    0.000000] MTRR fixed ranges enabled:
[    0.000000]   00000-9FFFF write-back
[    0.000000]   A0000-BFFFF uncachable
[    0.000000]   C0000-FFFFF write-back
[    0.000000] MTRR variable ranges enabled:
[    0.000000]   0 base 0000000000 mask 7F80000000 write-back
[    0.000000]   1 base 007C800000 mask 7FFF800000 uncachable
[    0.000000]   2 base 007D000000 mask 7FFF000000 uncachable
[    0.000000]   3 base 007E000000 mask 7FFE000000 uncachable
[    0.000000]   4 base 00D0000000 mask 7FF0000000 write-combining
[    0.000000]   5 base 00FF800000 mask 7FFF800000 uncachable
[    0.000000]   6 base 0100000000 mask 7F00000000 write-back
[    0.000000]   7 disabled
[    0.000000]   8 disabled
[    0.000000]   9 disabled
[    0.000000] x86 PAT enabled: cpu 0, old 0x7040600070406, new 0x7010600070106
[    0.000000] e820: last_pfn = 0x7bf71 max_arch_pfn = 0x400000000
[    0.000000] Base memory trampoline at [ffff880000099000] 99000 size 24576
[    0.000000] Using GB pages for direct mapping
[    0.000000] init_memory_mapping: [mem 0x00000000-0x000fffff]
[    0.000000]  [mem 0x00000000-0x000fffff] page 4k
[    0.000000] BRK [0x02200000, 0x02200fff] PGTABLE
[    0.000000] BRK [0x02201000, 0x02201fff] PGTABLE
[    0.000000] BRK [0x02202000, 0x02202fff] PGTABLE
[    0.000000] init_memory_mapping: [mem 0x100400000-0x1005fffff]
[    0.000000]  [mem 0x100400000-0x1005fffff] page 2M
[    0.000000] BRK [0x02203000, 0x02203fff] PGTABLE
[    0.000000] init_memory_mapping: [mem 0x100000000-0x1003fffff]
[    0.000000]  [mem 0x100000000-0x1003fffff] page 2M
[    0.000000] init_memory_mapping: [mem 0x00100000-0x00efffff]
[    0.000000]  [mem 0x00100000-0x001fffff] page 4k
[    0.000000]  [mem 0x00200000-0x00dfffff] page 2M
[    0.000000]  [mem 0x00e00000-0x00efffff] page 4k
[    0.000000] BRK [0x02204000, 0x02204fff] PGTABLE
[    0.000000] init_memory_mapping: [mem 0x01000000-0x7bf70fff]
[    0.000000]  [mem 0x01000000-0x7bdfffff] page 2M
[    0.000000]  [mem 0x7be00000-0x7bf70fff] page 4k
[    0.000000] ACPI: RSDP 00000000000f67b0 000024 (v02 CORE  )
[    0.000000] ACPI: XSDT 000000007bf8c0e0 000054 (v01 CORE   COREBOOT 00000000 CORE 00000000)
[    0.000000] ACPI: FACP 000000007bf902a0 0000F4 (v03 CORE   COREBOOT 00000000 CORE 00000001)
[    0.000000] ACPI Error: Gpe0Block - 32-bit FADT register is too long (32 bytes, 256 bits) to convert to GAS struct - 255 bits max, truncating (20131218/tbfadt-204)
[    0.000000] ACPI: DSDT 000000007bf8c250 004042 (v02 COREv4 COREBOOT 20110725 INTL 20090123)
[    0.000000] ACPI: FACS 000000007bf8c210 000040
[    0.000000] ACPI: HPET 000000007bf903a0 000038 (v01 CORE   COREBOOT 00000000 CORE 00000000)
[    0.000000] ACPI: APIC 000000007bf903e0 00005C (v01 CORE   COREBOOT 00000000 CORE 00000000)
[    0.000000] ACPI: MCFG 000000007bf90440 00003C (v01 CORE   COREBOOT 00000000 CORE 00000000)
[    0.000000] ACPI: SSDT 000000007bf91340 0008A0 (v02 CORE   COREBOOT 0000002A CORE 0000002A)
[    0.000000] ACPI: SSDT 000000007bf91be0 00005C (v02 CORE   COREBOOT 0000002A CORE 0000002A)
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] No NUMA configuration found
[    0.000000] Faking a node at [mem 0x0000000000000000-0x00000001005fffff]
[    0.000000] Initmem setup node 0 [mem 0x00000000-0x1005fffff]
[    0.000000]   NODE_DATA [mem 0x1005fa000-0x1005fdfff]
[    0.000000]  [ffffea0000000000-ffffea00041fffff] PMD -> [ffff880079800000-ffff88007b9fffff] on node 0
[    0.000000] Zone ranges:
[    0.000000]   DMA      [mem 0x00001000-0x00ffffff]
[    0.000000]   DMA32    [mem 0x01000000-0xffffffff]
[    0.000000]   Normal   [mem 0x100000000-0x1005fffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x00001000-0x0002ffff]
[    0.000000]   node   0: [mem 0x00040000-0x0009efff]
[    0.000000]   node   0: [mem 0x00100000-0x00efffff]
[    0.000000]   node   0: [mem 0x01000000-0x7bf70fff]
[    0.000000]   node   0: [mem 0x100000000-0x1005fffff]
[    0.000000] On node 0 totalpages: 508927
[    0.000000]   DMA zone: 59 pages used for memmap
[    0.000000]   DMA zone: 21 pages reserved
[    0.000000]   DMA zone: 3726 pages, LIFO batch:0
[    0.000000]   DMA32 zone: 7870 pages used for memmap
[    0.000000]   DMA32 zone: 503665 pages, LIFO batch:31
[    0.000000]   Normal zone: 24 pages used for memmap
[    0.000000]   Normal zone: 1536 pages, LIFO batch:0
[    0.000000] ACPI: PM-Timer IO Port: 0x1008
[    0.000000] ACPI: Local APIC address 0xfee00000
[    0.000000] ACPI: LAPIC (acpi_id[0x00] lapic_id[0x00] enabled)
[    0.000000] ACPI: LAPIC (acpi_id[0x01] lapic_id[0x02] enabled)
[    0.000000] ACPI: IOAPIC (id[0x02] address[0xfec00000] gsi_base[0])
[    0.000000] IOAPIC[0]: apic_id 2, version 32, address 0xfec00000, GSI 0-39
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
[    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
[    0.000000] ACPI: IRQ0 used by override.
[    0.000000] ACPI: IRQ2 used by override.
[    0.000000] ACPI: IRQ9 used by override.
[    0.000000] Using ACPI (MADT) for SMP configuration information
[    0.000000] ACPI: HPET id: 0x8086a201 base: 0xfed00000
[    0.000000] smpboot: Allowing 2 CPUs, 0 hotplug CPUs
[    0.000000] nr_irqs_gsi: 56
[    0.000000] e820: [mem 0x7ea00000-0xefffffff] available for PCI devices
[    0.000000] setup_percpu: NR_CPUS:8 nr_cpumask_bits:8 nr_cpu_ids:2 nr_node_ids:1
[    0.000000] PERCPU: Embedded 26 pages/cpu @ffff880100200000 s75584 r8192 d22720 u1048576
[    0.000000] pcpu-alloc: s75584 r8192 d22720 u1048576 alloc=1*2097152
[    0.000000] pcpu-alloc: [0] 0 1 
[    0.000000] Built 1 zonelists in Node order, mobility grouping on.  Total pages: 500953
[    0.000000] Policy zone: Normal
[    0.000000] Kernel command line: root=/dev/ram0 rdinit=/init radeon.audio=1 radeon.dpm=1 BOOT_IMAGE=/KERNEL boot=LABEL=System disk=LABEL=Storage  ssh quiet
[    0.000000] PID hash table entries: 4096 (order: 3, 32768 bytes)
[    0.000000] xsave: enabled xstate_bv 0x3, cntxt size 0x240
[    0.000000] Checking aperture...
[    0.000000] No AGP bridge found
[    0.000000] Memory: 1916008K/2035708K available (7604K kernel code, 726K rwdata, 5720K rodata, 2848K init, 492K bss, 119700K reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=2, Nodes=1
[    0.000000] Hierarchical RCU implementation.
[    0.000000] 	CONFIG_RCU_FANOUT set to non-default value of 32
[    0.000000] 	RCU dyntick-idle grace-period acceleration is enabled.
[    0.000000] 	RCU restricting CPUs from NR_CPUS=8 to nr_cpu_ids=2.
[    0.000000] 	Offload RCU callbacks from all CPUs
[    0.000000] 	Offload RCU callbacks from CPUs: 0-1.
[    0.000000] RCU: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=2
[    0.000000] NR_IRQS:4352 nr_irqs:512 16
[    0.000000] Console: colour VGA+ 80x25
[    0.000000] console [tty0] enabled
[    0.000000] hpet clockevent registered
[    0.000000] tsc: Fast TSC calibration using PIT
[    0.000000] tsc: Detected 1396.828 MHz processor
[    0.000012] Calibrating delay loop (skipped), value calculated using timer frequency.. 2794.05 BogoMIPS (lpj=4656093)
[    0.000016] pid_max: default: 32768 minimum: 301
[    0.000024] ACPI: Core revision 20131218
[    0.002617] ACPI: All ACPI Tables successfully acquired
[    0.002874] Dentry cache hash table entries: 262144 (order: 9, 2097152 bytes)
[    0.003505] Inode-cache hash table entries: 131072 (order: 8, 1048576 bytes)
[    0.003808] Mount-cache hash table entries: 4096 (order: 3, 32768 bytes)
[    0.003814] Mountpoint-cache hash table entries: 4096 (order: 3, 32768 bytes)
[    0.004053] CPU: Physical Processor ID: 0
[    0.004055] CPU: Processor Core ID: 0
[    0.005397] Last level iTLB entries: 4KB 1024, 2MB 1024, 4MB 1024
[    0.005397] Last level dTLB entries: 4KB 1024, 2MB 1024, 4MB 1024, 1GB 4
[    0.005397] tlb_flushall_shift: 6
[    0.005540] Freeing SMP alternatives memory: 20K (ffffffff8217f000 - ffffffff82184000)
[    0.006190] ..TIMER: vector=0x30 apic1=0 pin1=2 apic2=-1 pin2=-1
[    0.039192] smpboot: CPU0: Intel(R) Celeron(R) 2955U @ 1.40GHz (fam: 06, model: 45, stepping: 01)
[    0.039200] TSC deadline timer enabled
[    0.039208] Performance Events: PEBS fmt2+, 16-deep LBR, Haswell events, full-width counters, Intel PMU driver.
[    0.039218] ... version:                3
[    0.039220] ... bit width:              48
[    0.039221] ... generic registers:      8
[    0.039223] ... value mask:             0000ffffffffffff
[    0.039225] ... max period:             0000ffffffffffff
[    0.039226] ... fixed-purpose events:   3
[    0.039228] ... event mask:             00000007000000ff
[    0.039524] x86: Booting SMP configuration:
[    0.039527] .... node  #0, CPUs:      #1
[    0.054090] x86: Booted up 1 node, 2 CPUs
[    0.054093] smpboot: Total of 2 processors activated (5589.11 BogoMIPS)
[    0.054174] NMI watchdog: enabled on all CPUs, permanently consumes one hw-PMU counter.
[    0.055953] devtmpfs: initialized
[    0.056541] xor: measuring software checksum speed
[    0.087401]    prefetch64-sse:  9598.800 MB/sec
[    0.120744]    generic_sse:  8594.400 MB/sec
[    0.120746] xor: using function: prefetch64-sse (9598.800 MB/sec)
[    0.120749] pinctrl core: initialized pinctrl subsystem
[    0.120813] NET: Registered protocol family 16
[    0.121082] cpuidle: using governor ladder
[    0.121084] cpuidle: using governor menu
[    0.121266] ACPI: bus type PCI registered
[    0.121312] PCI: MMCONFIG for domain 0000 [bus 00-3f] at [mem 0xf0000000-0xf3ffffff] (base 0xf0000000)
[    0.121315] PCI: MMCONFIG at [mem 0xf0000000-0xf3ffffff] reserved in E820
[    0.123968] PCI: Using configuration type 1 for base access
[    0.126686] bio: create slab <bio-0> at 0
[    0.180775] raid6: sse2x1    4344 MB/s
[    0.237448] raid6: sse2x2    5562 MB/s
[    0.294131] raid6: sse2x4    6610 MB/s
[    0.294133] raid6: using algorithm sse2x4 (6610 MB/s)
[    0.294136] raid6: using ssse3x2 recovery algorithm
[    0.294168] ACPI: Added _OSI(Module Device)
[    0.294170] ACPI: Added _OSI(Processor Device)
[    0.294172] ACPI: Added _OSI(3.0 _SCP Extensions)
[    0.294174] ACPI: Added _OSI(Processor Aggregator Device)
[    0.297290] ACPI: Interpreter enabled
[    0.297298] ACPI Exception: AE_NOT_FOUND, While evaluating Sleep State [\_S1_] (20131218/hwxface-580)
[    0.297304] ACPI Exception: AE_NOT_FOUND, While evaluating Sleep State [\_S2_] (20131218/hwxface-580)
[    0.297316] ACPI: (supports S0 S3 S5)
[    0.297318] ACPI: Using IOAPIC for interrupt routing
[    0.297346] PCI: Using host bridge windows from ACPI; if necessary, use "pci=nocrs" and report a bug
[    0.306643] ACPI: Power Resource [FNP0] (off)
[    0.306682] ACPI: Power Resource [FNP1] (off)
[    0.306719] ACPI: Power Resource [FNP2] (off)
[    0.306756] ACPI: Power Resource [FNP3] (off)
[    0.306790] ACPI: Power Resource [FNP4] (on)
[    0.307425] ACPI: PCI Root Bridge [PCI0] (domain 0000 [bus 00-ff])
[    0.307432] acpi PNP0A08:00: _OSC: OS supports [ExtendedConfig ASPM ClockPM Segments MSI]
[    0.307480] acpi PNP0A08:00: _OSC: OS now controls [PCIeHotplug PME AER PCIeCapability]
[    0.307587] acpi PNP0A08:00: ignoring host bridge window [mem 0x000cc000-0x000cffff] (conflicts with Video ROM [mem 0x000c0000-0x000cebff])
[    0.307593] acpi PNP0A08:00: [Firmware Info]: MMCONFIG for domain 0000 [bus 00-3f] only partially covers this bridge
[    0.307625] PCI host bridge to bus 0000:00
[    0.307629] pci_bus 0000:00: root bus resource [bus 00-ff]
[    0.307632] pci_bus 0000:00: root bus resource [io  0x0000-0x0cf7]
[    0.307635] pci_bus 0000:00: root bus resource [io  0x0d00-0xffff]
[    0.307637] pci_bus 0000:00: root bus resource [mem 0x000a0000-0x000bffff]
[    0.307639] pci_bus 0000:00: root bus resource [mem 0x000c0000-0x000c3fff]
[    0.307642] pci_bus 0000:00: root bus resource [mem 0x000c4000-0x000c7fff]
[    0.307644] pci_bus 0000:00: root bus resource [mem 0x000c8000-0x000cbfff]
[    0.307647] pci_bus 0000:00: root bus resource [mem 0x000d0000-0x000d3fff]
[    0.307649] pci_bus 0000:00: root bus resource [mem 0x000d4000-0x000d7fff]
[    0.307652] pci_bus 0000:00: root bus resource [mem 0x000d8000-0x000dbfff]
[    0.307654] pci_bus 0000:00: root bus resource [mem 0x000dc000-0x000dffff]
[    0.307656] pci_bus 0000:00: root bus resource [mem 0x000e0000-0x000e3fff]
[    0.307659] pci_bus 0000:00: root bus resource [mem 0x000e4000-0x000e7fff]
[    0.307661] pci_bus 0000:00: root bus resource [mem 0x000e8000-0x000ebfff]
[    0.307663] pci_bus 0000:00: root bus resource [mem 0x000ec000-0x000effff]
[    0.307666] pci_bus 0000:00: root bus resource [mem 0x000f0000-0x000fffff]
[    0.307668] pci_bus 0000:00: root bus resource [mem 0x7ea00001-0xfebfffff]
[    0.307671] pci_bus 0000:00: root bus resource [mem 0xfed40000-0xfed44fff]
[    0.307682] pci 0000:00:00.0: [8086:0a04] type 00 class 0x060000
[    0.307802] pci 0000:00:02.0: [8086:0a06] type 00 class 0x030000
[    0.307819] pci 0000:00:02.0: reg 0x10: [mem 0xe0000000-0xe03fffff 64bit]
[    0.307829] pci 0000:00:02.0: reg 0x18: [mem 0xd0000000-0xdfffffff 64bit pref]
[    0.307837] pci 0000:00:02.0: reg 0x20: [io  0x3000-0x303f]
[    0.307945] pci 0000:00:03.0: [8086:0a0c] type 00 class 0x040300
[    0.307957] pci 0000:00:03.0: reg 0x10: [mem 0xe0710000-0xe0713fff 64bit]
[    0.308092] pci 0000:00:14.0: [8086:9c31] type 00 class 0x0c0330
[    0.308113] pci 0000:00:14.0: reg 0x10: [mem 0xe0700000-0xe070ffff 64bit]
[    0.308182] pci 0000:00:14.0: PME# supported from D3hot D3cold
[    0.308229] pci 0000:00:14.0: System wakeup disabled by ACPI
[    0.308286] pci 0000:00:1b.0: [8086:9c20] type 00 class 0x040300
[    0.308303] pci 0000:00:1b.0: reg 0x10: [mem 0xe0714000-0xe0717fff 64bit]
[    0.308381] pci 0000:00:1b.0: PME# supported from D0 D3hot D3cold
[    0.308429] pci 0000:00:1b.0: System wakeup disabled by ACPI
[    0.308473] pci 0000:00:1c.0: [8086:9c14] type 01 class 0x060400
[    0.308547] pci 0000:00:1c.0: PME# supported from D0 D3hot D3cold
[    0.308639] pci 0000:00:1c.1: [8086:9c16] type 01 class 0x060400
[    0.308712] pci 0000:00:1c.1: PME# supported from D0 D3hot D3cold
[    0.308801] pci 0000:00:1c.2: [8086:9c18] type 01 class 0x060400
[    0.308873] pci 0000:00:1c.2: PME# supported from D0 D3hot D3cold
[    0.308973] pci 0000:00:1f.0: [8086:9c45] type 00 class 0x060100
[    0.309173] pci 0000:00:1f.2: [8086:9c03] type 00 class 0x010601
[    0.309191] pci 0000:00:1f.2: reg 0x10: [io  0x3060-0x3067]
[    0.309201] pci 0000:00:1f.2: reg 0x14: [io  0x3070-0x3073]
[    0.309210] pci 0000:00:1f.2: reg 0x18: [io  0x3068-0x306f]
[    0.309218] pci 0000:00:1f.2: reg 0x1c: [io  0x3074-0x3077]
[    0.309227] pci 0000:00:1f.2: reg 0x20: [io  0x3040-0x305f]
[    0.309237] pci 0000:00:1f.2: reg 0x24: [mem 0xe0719000-0xe07197ff]
[    0.309278] pci 0000:00:1f.2: PME# supported from D3hot
[    0.309361] pci 0000:00:1f.3: [8086:9c22] type 00 class 0x0c0500
[    0.309378] pci 0000:00:1f.3: reg 0x10: [mem 0xe0719c00-0xe0719cff 64bit]
[    0.309401] pci 0000:00:1f.3: reg 0x20: [io  0x0400-0x041f]
[    0.309507] pci 0000:00:1f.6: [8086:9c24] type 00 class 0x118000
[    0.309542] pci 0000:00:1f.6: reg 0x10: [mem 0xe0718000-0xe0718fff 64bit]
[    0.309793] pci 0000:01:00.0: [10ec:8168] type 00 class 0x020000
[    0.309812] pci 0000:01:00.0: reg 0x10: [io  0x2000-0x20ff]
[    0.309844] pci 0000:01:00.0: reg 0x18: [mem 0xe0500000-0xe0500fff 64bit]
[    0.309865] pci 0000:01:00.0: reg 0x20: [mem 0xe0400000-0xe0403fff 64bit pref]
[    0.309964] pci 0000:01:00.0: supports D1 D2
[    0.309967] pci 0000:01:00.0: PME# supported from D0 D1 D2 D3hot D3cold
[    0.310011] pci 0000:01:00.0: System wakeup disabled by ACPI
[    0.314182] pci 0000:00:1c.0: PCI bridge to [bus 01]
[    0.314186] pci 0000:00:1c.0:   bridge window [io  0x2000-0x2fff]
[    0.314191] pci 0000:00:1c.0:   bridge window [mem 0xe0500000-0xe05fffff]
[    0.314197] pci 0000:00:1c.0:   bridge window [mem 0xe0400000-0xe04fffff 64bit pref]
[    0.314282] pci 0000:02:00.0: [168c:0034] type 00 class 0x028000
[    0.314316] pci 0000:02:00.0: reg 0x10: [mem 0xe0600000-0xe067ffff 64bit]
[    0.314396] pci 0000:02:00.0: reg 0x30: [mem 0xe0680000-0xe068ffff pref]
[    0.314505] pci 0000:02:00.0: supports D1
[    0.314507] pci 0000:02:00.0: PME# supported from D0 D1 D3hot
[    0.314553] pci 0000:02:00.0: System wakeup disabled by ACPI
[    0.320855] pci 0000:00:1c.1: PCI bridge to [bus 02]
[    0.320861] pci 0000:00:1c.1:   bridge window [mem 0xe0600000-0xe06fffff]
[    0.320922] pci 0000:00:1c.2: PCI bridge to [bus 03]
[    0.321036] ACPI: PCI Interrupt Link [LNKA] (IRQs 1 3 4 5 6 7 10 12 14 15) *11, disabled.
[    0.321088] ACPI: PCI Interrupt Link [LNKB] (IRQs 1 3 4 5 6 7 11 12 14 15) *10, disabled.
[    0.321136] ACPI: PCI Interrupt Link [LNKC] (IRQs 1 3 4 5 6 7 10 12 14 15) *11, disabled.
[    0.321183] ACPI: PCI Interrupt Link [LNKD] (IRQs 1 3 4 5 6 7 *11 12 14 15), disabled.
[    0.321230] ACPI: PCI Interrupt Link [LNKE] (IRQs 1 3 4 5 6 7 10 12 14 15) *0, disabled.
[    0.321277] ACPI: PCI Interrupt Link [LNKF] (IRQs 1 3 4 5 6 7 11 12 14 15) *0, disabled.
[    0.321325] ACPI: PCI Interrupt Link [LNKG] (IRQs 1 3 4 5 6 7 10 12 14 15) *0, disabled.
[    0.321374] ACPI: PCI Interrupt Link [LNKH] (IRQs 1 3 4 5 6 7 11 12 14 15) *0, disabled.
[    0.321992] vgaarb: device added: PCI:0000:00:02.0,decodes=io+mem,owns=io+mem,locks=none
[    0.321997] vgaarb: loaded
[    0.321998] vgaarb: bridge control possible 0000:00:02.0
[    0.322083] SCSI subsystem initialized
[    0.322131] libata version 3.00 loaded.
[    0.322163] ACPI: bus type USB registered
[    0.322191] usbcore: registered new interface driver usbfs
[    0.322204] usbcore: registered new interface driver hub
[    0.322240] usbcore: registered new device driver usb
[    0.322264] pps_core: LinuxPPS API ver. 1 registered
[    0.322265] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.322270] PTP clock support registered
[    0.322317] Advanced Linux Sound Architecture Driver Initialized.
[    0.322319] PCI: Using ACPI for IRQ routing
[    0.323870] PCI: pci_cache_line_size set to 64 bytes
[    0.323920] e820: reserve RAM buffer [mem 0x0009fc00-0x0009ffff]
[    0.323922] e820: reserve RAM buffer [mem 0x7bf71000-0x7bffffff]
[    0.323925] e820: reserve RAM buffer [mem 0x100600000-0x103ffffff]
[    0.324249] Switched to clocksource hpet
[    0.324311] pnp: PnP ACPI init
[    0.324323] ACPI: bus type PNP registered
[    0.324395] system 00:00: [mem 0xfed1c000-0xfed1ffff] has been reserved
[    0.324399] system 00:00: [mem 0xfed10000-0xfed13fff] has been reserved
[    0.324402] system 00:00: [mem 0xfed18000-0xfed18fff] has been reserved
[    0.324405] system 00:00: [mem 0xfed19000-0xfed19fff] has been reserved
[    0.324407] system 00:00: [mem 0xf0000000-0xf3ffffff] has been reserved
[    0.324410] system 00:00: [mem 0xfed20000-0xfed3ffff] has been reserved
[    0.324413] system 00:00: [mem 0xfed40000-0xfed44fff] has been reserved
[    0.324416] system 00:00: [mem 0xfed45000-0xfed8ffff] could not be reserved
[    0.324419] system 00:00: [mem 0x00f00000-0x00ffffff] has been reserved
[    0.324423] system 00:00: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.324571] pnp 00:01: [dma 4]
[    0.324600] pnp 00:01: Plug and Play ACPI device, IDs PNP0200 (active)
[    0.324629] pnp 00:02: Plug and Play ACPI device, IDs INT0800 (active)
[    0.324726] system 00:03: [mem 0xfed00000-0xfed003ff] has been reserved
[    0.324730] system 00:03: Plug and Play ACPI device, IDs PNP0103 PNP0c01 (active)
[    0.324769] pnp 00:04: Plug and Play ACPI device, IDs PNP0c04 (active)
[    0.324842] system 00:05: [io  0x1000-0x10fe] could not be reserved
[    0.324846] system 00:05: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.324876] pnp 00:06: Plug and Play ACPI device, IDs PNP0b00 (active)
[    0.324979] system 00:07: [io  0x0700-0x0707] has been reserved
[    0.324982] system 00:07: [io  0x0710-0x0713] has been reserved
[    0.324985] system 00:07: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.325032] system 00:08: [io  0x0720] has been reserved
[    0.325035] system 00:08: [io  0x0730-0x0737] has been reserved
[    0.325038] system 00:08: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.325126] pnp 00:09: Plug and Play ACPI device, IDs PNP0501 (active)
[    0.325214] pnp 00:0a: Plug and Play ACPI device, IDs PNP0303 PNP030b (active)
[    0.325299] pnp 00:0b: Plug and Play ACPI device, IDs PNP0f13 (active)
[    0.325350] pnp 00:0c: Plug and Play ACPI device, IDs IFX0102 PNP0c31 (active)
[    0.325451] system 00:0d: Plug and Play ACPI device, IDs PNP0c02 (active)
[    0.325565] pnp: PnP ACPI: found 14 devices
[    0.325566] ACPI: bus type PNP unregistered
[    0.332024] pci 0000:00:1c.0: PCI bridge to [bus 01]
[    0.332028] pci 0000:00:1c.0:   bridge window [io  0x2000-0x2fff]
[    0.332035] pci 0000:00:1c.0:   bridge window [mem 0xe0500000-0xe05fffff]
[    0.332040] pci 0000:00:1c.0:   bridge window [mem 0xe0400000-0xe04fffff 64bit pref]
[    0.332046] pci 0000:00:1c.1: PCI bridge to [bus 02]
[    0.332052] pci 0000:00:1c.1:   bridge window [mem 0xe0600000-0xe06fffff]
[    0.332061] pci 0000:00:1c.2: PCI bridge to [bus 03]
[    0.332075] pci_bus 0000:00: resource 4 [io  0x0000-0x0cf7]
[    0.332078] pci_bus 0000:00: resource 5 [io  0x0d00-0xffff]
[    0.332081] pci_bus 0000:00: resource 6 [mem 0x000a0000-0x000bffff]
[    0.332083] pci_bus 0000:00: resource 7 [mem 0x000c0000-0x000c3fff]
[    0.332086] pci_bus 0000:00: resource 8 [mem 0x000c4000-0x000c7fff]
[    0.332088] pci_bus 0000:00: resource 9 [mem 0x000c8000-0x000cbfff]
[    0.332091] pci_bus 0000:00: resource 10 [mem 0x000d0000-0x000d3fff]
[    0.332093] pci_bus 0000:00: resource 11 [mem 0x000d4000-0x000d7fff]
[    0.332096] pci_bus 0000:00: resource 12 [mem 0x000d8000-0x000dbfff]
[    0.332098] pci_bus 0000:00: resource 13 [mem 0x000dc000-0x000dffff]
[    0.332100] pci_bus 0000:00: resource 14 [mem 0x000e0000-0x000e3fff]
[    0.332103] pci_bus 0000:00: resource 15 [mem 0x000e4000-0x000e7fff]
[    0.332105] pci_bus 0000:00: resource 16 [mem 0x000e8000-0x000ebfff]
[    0.332108] pci_bus 0000:00: resource 17 [mem 0x000ec000-0x000effff]
[    0.332110] pci_bus 0000:00: resource 18 [mem 0x000f0000-0x000fffff]
[    0.332113] pci_bus 0000:00: resource 19 [mem 0x7ea00001-0xfebfffff]
[    0.332115] pci_bus 0000:00: resource 20 [mem 0xfed40000-0xfed44fff]
[    0.332118] pci_bus 0000:01: resource 0 [io  0x2000-0x2fff]
[    0.332120] pci_bus 0000:01: resource 1 [mem 0xe0500000-0xe05fffff]
[    0.332123] pci_bus 0000:01: resource 2 [mem 0xe0400000-0xe04fffff 64bit pref]
[    0.332126] pci_bus 0000:02: resource 1 [mem 0xe0600000-0xe06fffff]
[    0.332161] NET: Registered protocol family 2
[    0.332333] TCP established hash table entries: 16384 (order: 5, 131072 bytes)
[    0.332387] TCP bind hash table entries: 16384 (order: 6, 262144 bytes)
[    0.332432] TCP: Hash tables configured (established 16384 bind 16384)
[    0.332457] TCP: reno registered
[    0.332464] UDP hash table entries: 1024 (order: 3, 32768 bytes)
[    0.332476] UDP-Lite hash table entries: 1024 (order: 3, 32768 bytes)
[    0.332538] NET: Registered protocol family 1
[    0.332628] RPC: Registered named UNIX socket transport module.
[    0.332630] RPC: Registered udp transport module.
[    0.332632] RPC: Registered tcp transport module.
[    0.332633] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.332643] pci 0000:00:02.0: Boot video device
[    0.332896] PCI: CLS 64 bytes, default 64
[    0.376164] PCI-DMA: Using software bounce buffering for IO (SWIOTLB)
[    0.376171] software IO TLB [mem 0x75800000-0x79800000] (64MB) mapped at [ffff880075800000-ffff8800797fffff]
[    0.376481] RAPL PMU detected, hw unit 2^-14 Joules, API unit is 2^-32 Joules, 3 fixed counters 655360 ms ovfl timer
[    0.376516] microcode: CPU0 sig=0x40651, pf=0x40, revision=0x15
[    0.376525] microcode: CPU1 sig=0x40651, pf=0x40, revision=0x15
[    0.376581] microcode: Microcode Update Driver: v2.00 <tigran@aivazian.fsnet.co.uk>, Peter Oruba
[    0.376879] futex hash table entries: 512 (order: 3, 32768 bytes)
[    0.379469] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.379762] NFS: Registering the id_resolver key type
[    0.379774] Key type id_resolver registered
[    0.379776] Key type id_legacy registered
[    0.379781] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.380020] JFS: nTxBlock = 8192, nTxLock = 65536
[    0.381671] SGI XFS with security attributes, large block/inode numbers, no debug enabled
[    0.382194] msgmni has been set to 3742
[    0.383008] alg: No test for stdrng (krng)
[    0.383061] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 251)
[    0.383064] io scheduler noop registered
[    0.383072] io scheduler cfq registered (default)
[    0.383280] pcieport 0000:00:1c.0: irq 56 for MSI/MSI-X
[    0.383468] pcieport 0000:00:1c.1: irq 57 for MSI/MSI-X
[    0.383563] pcieport 0000:00:1c.2: irq 58 for MSI/MSI-X
[    0.383676] aer 0000:00:1c.0:pcie02: service driver aer loaded
[    0.383703] aer 0000:00:1c.1:pcie02: service driver aer loaded
[    0.383733] aer 0000:00:1c.2:pcie02: service driver aer loaded
[    0.383750] pcieport 0000:00:1c.0: Signaling PME through PCIe PME interrupt
[    0.383753] pci 0000:01:00.0: Signaling PME through PCIe PME interrupt
[    0.383757] pcie_pme 0000:00:1c.0:pcie01: service driver pcie_pme loaded
[    0.383767] pcieport 0000:00:1c.1: Signaling PME through PCIe PME interrupt
[    0.383769] pci 0000:02:00.0: Signaling PME through PCIe PME interrupt
[    0.383774] pcie_pme 0000:00:1c.1:pcie01: service driver pcie_pme loaded
[    0.383786] pcieport 0000:00:1c.2: Signaling PME through PCIe PME interrupt
[    0.383790] pcie_pme 0000:00:1c.2:pcie01: service driver pcie_pme loaded
[    0.383838] intel_idle: MWAIT substates: 0x11142120
[    0.383840] intel_idle: v0.4 model 0x45
[    0.383841] intel_idle: lapic_timer_reliable_states 0xffffffff
[    0.384065] input: Power Button as /devices/LNXSYSTM:00/device:00/PNP0C0C:00/input/input0
[    0.384070] ACPI: Power Button [PWRB]
[    0.384124] input: Power Button as /devices/LNXSYSTM:00/LNXPWRBN:00/input/input1
[    0.384127] ACPI: Power Button [PWRF]
[    0.384201] ACPI: Fan [FAN0] (off)
[    0.384236] ACPI: Fan [FAN1] (off)
[    0.384289] ACPI: Fan [FAN2] (off)
[    0.384321] ACPI: Fan [FAN3] (off)
[    0.384359] ACPI: Fan [FAN4] (on)
[    0.384533] ACPI: Video Device [GFX0] (multi-head: yes  rom: no  post: no)
[    0.384662] input: Video Bus as /devices/LNXSYSTM:00/device:00/PNP0A08:00/LNXVIDEO:00/input/input2
[    0.385605] thermal LNXTHERM:00: registered as thermal_zone0
[    0.385608] ACPI: Thermal Zone [THRM] (37 C)
[    0.385686] Serial: 8250/16550 driver, 4 ports, IRQ sharing disabled
[    0.406427] 00:09: ttyS0 at I/O 0x3f8 (irq = 4, base_baud = 115200) is a 16550A
[    0.406859] Linux agpgart interface v0.103
[    0.406905] [drm] Initialized drm 1.1.0 20060810
[    0.406920] [drm] radeon kernel modesetting enabled.
[    0.407723] [drm] Memory usable by graphics device = 2048M
[    0.423093] i915 0000:00:02.0: irq 59 for MSI/MSI-X
[    0.423101] [drm] Supports vblank timestamp caching Rev 2 (21.10.2013).
[    0.423103] [drm] Driver supports precise vblank timestamp query.
[    0.423179] vgaarb: device changed decodes: PCI:0000:00:02.0,olddecodes=io+mem,decodes=io+mem:owns=io+mem
[    0.506919] fbcon: inteldrmfb (fb0) is primary device
[    0.708551] Console: switching to colour frame buffer device 240x67
[    0.717088] i915 0000:00:02.0: fb0: inteldrmfb frame buffer device
[    0.717091] i915 0000:00:02.0: registered panic notifier
[    0.717118] [drm] Initialized i915 1.6.0 20080730 for 0000:00:02.0 on minor 0
[    0.719863] brd: module loaded
[    0.719907] loop: module loaded
[    0.720228] nbd: registered device at major 43
[    0.721649] Loading iSCSI transport class v2.0-870.
[    0.721773] iscsi: registered transport (tcp)
[    0.721858] ahci 0000:00:1f.2: version 3.0
[    0.722032] ahci 0000:00:1f.2: irq 60 for MSI/MSI-X
[    0.722051] ahci 0000:00:1f.2: SSS flag set, parallel bus scan disabled
[    0.722070] ahci 0000:00:1f.2: AHCI 0001.0300 32 slots 2 ports 6 Gbps 0x1 impl SATA mode
[    0.722074] ahci 0000:00:1f.2: flags: 64bit ncq ilck stag pm led clo only pio slum part deso sadm apst 
[    0.722410] scsi0 : ahci
[    0.722537] scsi1 : ahci
[    0.722609] ata1: SATA max UDMA/133 abar m2048@0xe0719000 port 0xe0719100 irq 60
[    0.722612] ata2: DUMMY
[    0.723061] tun: Universal TUN/TAP device driver, 1.6
[    0.723063] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
[    0.723131] pcnet32: pcnet32.c:v1.35 21.Apr.2008 tsbogend@alpha.franken.de
[    0.723158] Atheros(R) L2 Ethernet Driver - version 2.2.3
[    0.723160] Copyright (c) 2007 Atheros Corporation.
[    0.723240] cnic: Broadcom NetXtreme II CNIC Driver cnic v2.5.20 (March 14, 2014)
[    0.723291] uli526x: ULi M5261/M5263 net driver, version 0.9.3 (2005-7-29)
[    0.723307] e100: Intel(R) PRO/100 Network Driver, 3.5.24-k2-NAPI
[    0.723308] e100: Copyright(c) 1999-2006 Intel Corporation
[    0.723326] e1000: Intel(R) PRO/1000 Network Driver - version 7.3.21-k8-NAPI
[    0.723328] e1000: Copyright (c) 1999-2006 Intel Corporation.
[    0.723344] e1000e: Intel(R) PRO/1000 Network Driver - 2.3.2-k
[    0.723346] e1000e: Copyright(c) 1999 - 2013 Intel Corporation.
[    0.723365] igb: Intel(R) Gigabit Ethernet Network Driver - version 5.0.5-k
[    0.723367] igb: Copyright (c) 2007-2013 Intel Corporation.
[    0.723395] jme: JMicron JMC2XX ethernet driver version 1.0.8
[    0.723426] sky2: driver version 1.30
[    0.723493] r8169 Gigabit Ethernet driver 2.3LK-NAPI loaded
[    0.727930] r8169 0000:01:00.0: irq 61 for MSI/MSI-X
[    0.728107] r8169 0000:01:00.0 eth0: RTL8168g/8111g at 0xffffc90000360000, c4:54:44:38:e6:9c, XID 0c000800 IRQ 61
[    0.728111] r8169 0000:01:00.0 eth0: jumbo features [frames: 9200 bytes, tx checksumming: ko]
[    0.728202] PPP generic driver version 2.4.2
[    0.728262] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    0.728264] ehci-pci: EHCI PCI platform driver
[    0.728279] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    0.728285] ohci-pci: OHCI PCI platform driver
[    0.728297] uhci_hcd: USB Universal Host Controller Interface driver
[    0.728332] usbcore: registered new interface driver usb-storage
[    0.728393] i8042: PNP: PS/2 Controller [PNP0303:PS2K,PNP0f13:PS2M] at 0x60,0x64 irq 1,12
[    0.728805] serio: i8042 KBD port at 0x60,0x64 irq 1
[    0.728812] serio: i8042 AUX port at 0x60,0x64 irq 12
[    0.728936] mousedev: PS/2 mouse device common for all mice
[    0.729550] rtc_cmos 00:06: RTC can wake from S4
[    0.729757] rtc_cmos 00:06: rtc core: registered rtc_cmos as rtc0
[    0.729788] rtc_cmos 00:06: alarms up to one month, 242 bytes nvram, hpet irqs
[    0.729798] i2c /dev entries driver
[    0.730429] i801_smbus 0000:00:1f.3: SMBus using PCI Interrupt
[    0.730684] sdhci: Secure Digital Host Controller Interface driver
[    0.730686] sdhci: Copyright(c) Pierre Ossman
[    0.730710] No iBFT detected.
[    0.730726] hidraw: raw HID events driver (C) Jiri Kosina
[    0.730974] usbcore: registered new interface driver usbhid
[    0.730976] usbhid: USB HID core driver
[    0.730999] usbcore: registered new interface driver rts5139
[    0.731001] rts5208: Initializing Realtek PCIE storage driver...
[    0.731172] TCP: cubic registered
[    0.731329] NET: Registered protocol family 10
[    0.731654] NET: Registered protocol family 17
[    0.731678] Key type dns_resolver registered
[    0.732312] bio: create slab <bio-1> at 1
[    0.732533] Btrfs loaded
[    0.732866] rtc_cmos 00:06: setting system clock to 2014-05-21 14:53:10 UTC (1400683990)
[    0.733089] ALSA device list:
[    0.733091]   No soundcards found.
[    1.040944] ata1: SATA link up 6.0 Gbps (SStatus 133 SControl 300)
[    1.041845] ata1.00: ATA-9: SanDisk SSD U110 16GB, U221000, max UDMA/133
[    1.041855] ata1.00: 31277232 sectors, multi 1: LBA48 NCQ (depth 31/32)
[    1.042982] ata1.00: configured for UDMA/133
[    1.043314] scsi 0:0:0:0: Direct-Access     ATA      SanDisk SSD U110 U221 PQ: 0 ANSI: 5
[    1.043653] sd 0:0:0:0: Attached scsi generic sg0 type 0
[    1.043672] sd 0:0:0:0: [sda] 31277232 512-byte logical blocks: (16.0 GB/14.9 GiB)
[    1.043813] sd 0:0:0:0: [sda] Write Protect is off
[    1.043819] sd 0:0:0:0: [sda] Mode Sense: 00 3a 00 00
[    1.043844] sd 0:0:0:0: [sda] Write cache: enabled, read cache: enabled, doesn't support DPO or FUA
[    1.044590]  sda: sda1 sda2
[    1.045218] sd 0:0:0:0: [sda] Attached SCSI disk
[    1.052485] Freeing unused kernel memory: 2848K (ffffffff81eb7000 - ffffffff8217f000)
[    1.052492] Write protecting the kernel read-only data: 14336k
[    1.057008] Freeing unused kernel memory: 576K (ffff880001770000 - ffff880001800000)
[    1.059964] Freeing unused kernel memory: 424K (ffff880001d96000 - ffff880001e00000)
[    1.082049] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.082063] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 1
[    1.082163] xhci_hcd 0000:00:14.0: cache line size of 64 is not supported
[    1.082192] xhci_hcd 0000:00:14.0: irq 62 for MSI/MSI-X
[    1.082558] hub 1-0:1.0: USB hub found
[    1.082576] hub 1-0:1.0: 8 ports detected
[    1.082949] xhci_hcd 0000:00:14.0: xHCI Host Controller
[    1.082956] xhci_hcd 0000:00:14.0: new USB bus registered, assigned bus number 2
[    1.083340] hub 2-0:1.0: USB hub found
[    1.083355] hub 2-0:1.0: 4 ports detected
[    1.114216] EXT4-fs (sda1): couldn't mount as ext3 due to feature incompatibilities
[    1.114583] EXT4-fs (sda1): couldn't mount as ext2 due to feature incompatibilities
[    1.116553] EXT4-fs (sda1): mounted filesystem with ordered data mode. Opts: (null)
[    1.236436] EXT4-fs (sda2): couldn't mount as ext3 due to feature incompatibilities
[    1.236760] EXT4-fs (sda2): couldn't mount as ext2 due to feature incompatibilities
[    1.239033] EXT4-fs (sda2): mounted filesystem with ordered data mode. Opts: (null)
[    1.377458] tsc: Refined TSC clocksource calibration: 1396.766 MHz
[    1.440788] usb 1-4: new full-speed USB device number 2 using xhci_hcd
[    1.615562] usb 1-4: string descriptor 0 malformed (err = -61), defaulting to 0x0409
[    1.886339] random: systemd urandom read with 40 bits of entropy available
[    1.886532] systemd[1]: systemd 212 running in system mode. (-PAM -AUDIT -SELINUX -IMA -SYSVINIT -LIBCRYPTSETUP -GCRYPT -ACL -XZ -SECCOMP -APPARMOR)
[    1.886699] systemd[1]: Detected architecture 'x86-64'.
[    1.886800] systemd[1]: Set hostname to <openelec>.
[    1.886857] systemd[1]: Initializing machine ID from random generator.
[    1.914636] systemd[1]: Cannot add dependency job for unit display-manager.service, ignoring: Unit display-manager.service failed to load: No such file or directory.
[    1.915032] systemd[1]: Starting Paths.
[    1.915051] systemd[1]: Reached target Paths.
[    1.915067] systemd[1]: Starting Swap.
[    1.915079] systemd[1]: Reached target Swap.
[    1.915091] systemd[1]: Starting Root Slice.
[    1.915121] systemd[1]: Created slice Root Slice.
[    1.915133] systemd[1]: Starting User and Session Slice.
[    1.915172] systemd[1]: Created slice User and Session Slice.
[    1.915184] systemd[1]: Starting /dev/initctl Compatibility Named Pipe.
[    1.915222] systemd[1]: Listening on /dev/initctl Compatibility Named Pipe.
[    1.915233] systemd[1]: Starting Delayed Shutdown Socket.
[    1.915264] systemd[1]: Listening on Delayed Shutdown Socket.
[    1.915282] systemd[1]: Starting udev Control Socket.
[    1.915315] systemd[1]: Listening on udev Control Socket.
[    1.915330] systemd[1]: Starting udev Kernel Socket.
[    1.915358] systemd[1]: Listening on udev Kernel Socket.
[    1.915371] systemd[1]: Starting Journal Socket.
[    1.915440] systemd[1]: Listening on Journal Socket.
[    1.915460] systemd[1]: Starting System Slice.
[    1.915497] systemd[1]: Created slice System Slice.
[    1.915612] systemd[1]: Starting Remount Root and Kernel File Systems...
[    1.915920] systemd[1]: Mounting Temporary Directory...
[    1.916427] systemd[1]: Starting Setup User config dir...
[    1.916718] systemd[1]: Mounted Huge Pages File System.
[    1.916753] systemd[1]: Mounting POSIX Message Queue File System...
[    1.917541] systemd[1]: Starting Create list of required static device nodes for the current kernel...
[    1.917832] systemd[1]: Starting Setup Loopback interface...
[    1.918112] systemd[1]: Mounting Debug File System...
[    1.918361] systemd[1]: Starting Set ondemand threshold...
[    1.918620] systemd[1]: Starting Show Version...
[    1.923040] systemd[1]: Starting Load Kernel Modules...
[    1.924731] systemd[1]: Starting Apply Kernel Variables...
[    1.925046] systemd[1]: Starting udev Coldplug all Devices...
[    1.925317] systemd[1]: Starting Slices.
[    1.925333] systemd[1]: Reached target Slices.
[    1.925364] systemd[1]: Mounting Variable Directory...
[    1.934300] systemd[1]: Started Setup debug config.
[    1.934714] systemd[1]: Started Remount Root and Kernel File Systems.
[    1.939597] systemd[1]: Mounted Temporary Directory.
[    1.941952] systemd[1]: Mounted Debug File System.
[    1.941995] systemd[1]: Mounted POSIX Message Queue File System.
[    1.942372] systemd[1]: Started Set ondemand threshold.
[    1.942861] systemd[1]: Mounted Variable Directory.
[    1.957552] systemd[1]: Started Create list of required static device nodes for the current kernel.
[    1.957789] systemd[1]: Started Setup Loopback interface.
[    1.958003] systemd[1]: Started Show Version.
[    1.965243] systemd[1]: Started Load Kernel Modules.
[    1.965477] systemd[1]: Started Apply Kernel Variables.
[    1.983678] systemd[1]: Mounted FUSE Control File System.
[    1.983706] systemd[1]: Mounted Configuration File System.
[    1.983720] systemd[1]: Starting Restoring Backup...
[    1.984243] systemd[1]: Started Factory reset.
[    1.984277] systemd[1]: Started FS Resize.
[    1.984357] systemd[1]: Starting Create Static Device Nodes in /dev...
[    1.985162] systemd[1]: Started udev Coldplug all Devices.
[    1.992013] systemd[1]: Started Create Static Device Nodes in /dev.
[    1.994710] systemd[1]: Started Restoring Backup.
[    1.996060] systemd[1]: Starting Local File Systems (Pre).
[    1.996081] systemd[1]: Reached target Local File Systems (Pre).
[    2.047170] systemd[1]: Started Setup User config dir.
[    2.047267] systemd[1]: Starting Local File Systems.
[    2.047284] systemd[1]: Reached target Local File Systems.
[    2.047343] systemd[1]: Starting Setup Hostname...
[    2.047662] systemd[1]: Starting Setup machine-id...
[    2.048190] systemd[1]: Starting Create Volatile Files and Directories...
[    2.056398] systemd[1]: Started Create Volatile Files and Directories.
[    2.056493] systemd[1]: Starting Update hwdb.bin...
[    2.056894] systemd[1]: Started Debug /var/log relink.
[    2.057383] systemd[1]: Started Setup Hostname.
[    2.064416] systemd[1]: Started Update hwdb.bin.
[    2.064500] systemd[1]: Starting udev Kernel Device Manager...
[    2.065060] systemd[1]: Started Setup machine-id.
[    2.065145] systemd[1]: Starting Journal Service...
[    2.065477] systemd[1]: Started Journal Service.
[    2.071181] systemd-udevd[199]: starting version 212
[    2.206159] systemd-journald[200]: Received request to flush runtime journal from PID 1
[    2.239666] cfg80211: Calling CRDA to update world regulatory domain
[    2.239678] cfg80211: World regulatory domain updated:
[    2.239681] cfg80211:  DFS Master region: unset
[    2.239682] cfg80211:   (start_freq - end_freq @ bandwidth), (max_antenna_gain, max_eirp)
[    2.239685] cfg80211:   (2402000 KHz - 2472000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[    2.239688] cfg80211:   (2457000 KHz - 2482000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[    2.239690] cfg80211:   (2474000 KHz - 2494000 KHz @ 20000 KHz), (2000 mBi, 0 mBm)
[    2.239692] cfg80211:   (5170000 KHz - 5250000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[    2.239694] cfg80211:   (5735000 KHz - 5835000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[    2.239696] cfg80211:   (57240000 KHz - 63720000 KHz @ 2160000 KHz), (N/A, 0 mBm)
[    2.243467] snd_hda_intel 0000:00:03.0: irq 63 for MSI/MSI-X
[    2.245740] snd_hda_intel 0000:00:1b.0: irq 64 for MSI/MSI-X
[    2.283448] Bluetooth: Core ver 2.18
[    2.283473] NET: Registered protocol family 31
[    2.283476] Bluetooth: HCI device and connection manager initialized
[    2.283484] Bluetooth: HCI socket layer initialized
[    2.283487] Bluetooth: L2CAP socket layer initialized
[    2.283498] Bluetooth: SCO socket layer initialized
[    2.301086] input: HDA Intel HDMI HDMI/DP,pcm=8 as /devices/pci0000:00/0000:00:03.0/sound/card0/input10
[    2.301233] input: HDA Intel HDMI HDMI/DP,pcm=7 as /devices/pci0000:00/0000:00:03.0/sound/card0/input9
[    2.301313] input: HDA Intel HDMI HDMI/DP,pcm=3 as /devices/pci0000:00/0000:00:03.0/sound/card0/input8
[    2.321999] ath: phy0: ASPM enabled: 0x43
[    2.322005] ath: EEPROM regdomain: 0x60
[    2.322007] ath: EEPROM indicates we should expect a direct regpair map
[    2.322010] ath: Country alpha2 being used: 00
[    2.322012] ath: Regpair used: 0x60
[    2.322592] ieee80211 phy0: Selected rate control algorithm 'minstrel_ht'
[    2.322873] ieee80211 phy0: Atheros AR9462 Rev:2 mem=0xffffc90015980000, irq=19
[    2.336919] input: HDA Digital PCBeep as /devices/pci0000:00/0000:00:1b.0/input/input11
[    2.341452] input: HDA Intel PCH Headphone as /devices/pci0000:00/0000:00:1b.0/sound/card1/input13
[    2.342350] input: HDA Intel PCH Mic as /devices/pci0000:00/0000:00:1b.0/sound/card1/input12
[    2.342811] [drm] Enabling RC6 states: RC6 on, RC6p off, RC6pp off
[    2.345554] usbcore: registered new interface driver ath3k
[    2.345965] usb 1-4: USB disconnect, device number 2
[    2.347896] usbcore: registered new interface driver btusb
[    2.385495] Switched to clocksource tsc
[    2.447748] r8169 0000:01:00.0 eth0: link down
[    2.461602] IPv6: ADDRCONF(NETDEV_UP): eth0: link is not ready
[    2.650876] IPv6: ADDRCONF(NETDEV_UP): wlan0: link is not ready
[    2.655132] usb 1-4: new full-speed USB device number 3 using xhci_hcd
[    2.831627] usb 1-4: string descriptor 0 malformed (err = -61), defaulting to 0x0409
[    3.039381] wlan0: authenticate with 7c:d1:c3:cc:02:ed
[    3.055943] wlan0: direct probe to 7c:d1:c3:cc:02:ed (try 1/3)
[    3.257138] wlan0: send auth to 7c:d1:c3:cc:02:ed (try 2/3)
[    3.271596] wlan0: authenticated
[    3.273803] wlan0: associate with 7c:d1:c3:cc:02:ed (try 1/3)
[    3.388646] wlan0: RX AssocResp from 7c:d1:c3:cc:02:ed (capab=0x1511 status=0 aid=2)
[    3.388704] wlan0: associated
[    3.388734] IPv6: ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
[    3.388783] cfg80211: Calling CRDA for country: NO
[    3.388816] ath: EEPROM regdomain: 0x8242
[    3.388818] ath: EEPROM indicates we should expect a country code
[    3.388820] ath: doing EEPROM country->regdmn map search
[    3.388822] ath: country maps to regdmn code: 0x37
[    3.388824] ath: Country alpha2 being used: NO
[    3.388825] ath: Regpair used: 0x37
[    3.388827] ath: regdomain 0x8242 dynamically updated by country IE
[    3.388856] cfg80211: Regulatory domain changed to country: NO
[    3.388858] cfg80211:  DFS Master region: ETSI
[    3.388860] cfg80211:   (start_freq - end_freq @ bandwidth), (max_antenna_gain, max_eirp)
[    3.388863] cfg80211:   (2402000 KHz - 2482000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[    3.388865] cfg80211:   (5170000 KHz - 5250000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[    3.388867] cfg80211:   (5250000 KHz - 5330000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[    3.388869] cfg80211:   (5490000 KHz - 5710000 KHz @ 80000 KHz), (2700 mBi, 0 mBm)
[    3.388871] cfg80211:   (57240000 KHz - 65880000 KHz @ 2160000 KHz), (4000 mBi, 0 mBm)
[    3.465969] wlan0: Limiting TX power to 30 (30 - 0) dBm as advertised by 7c:d1:c3:cc:02:ed
[    3.498337] random: nonblocking pool is initialized
[  466.058769] wlan0: authenticate with 7c:d1:c3:cc:02:ec
[  466.064843] wlan0: send auth to 7c:d1:c3:cc:02:ec (try 1/3)
[  466.065589] cfg80211: Calling CRDA to update world regulatory domain
[  466.065636] cfg80211: World regulatory domain updated:
[  466.065639] cfg80211:  DFS Master region: unset
[  466.065641] cfg80211:   (start_freq - end_freq @ bandwidth), (max_antenna_gain, max_eirp)
[  466.065644] cfg80211:   (2402000 KHz - 2472000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[  466.065647] cfg80211:   (2457000 KHz - 2482000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[  466.065686] cfg80211:   (2474000 KHz - 2494000 KHz @ 20000 KHz), (2000 mBi, 0 mBm)
[  466.065688] cfg80211:   (5170000 KHz - 5250000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[  466.065691] cfg80211:   (5735000 KHz - 5835000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[  466.065693] cfg80211:   (57240000 KHz - 63720000 KHz @ 2160000 KHz), (N/A, 0 mBm)
[  466.066828] wlan0: authenticated
[  466.069944] wlan0: associate with 7c:d1:c3:cc:02:ec (try 1/3)
[  466.073731] wlan0: RX AssocResp from 7c:d1:c3:cc:02:ec (capab=0x1431 status=0 aid=3)
[  466.073791] wlan0: associated
[  466.073820] IPv6: ADDRCONF(NETDEV_CHANGE): wlan0: link becomes ready
[  466.073855] cfg80211: Calling CRDA for country: NO
[  466.073883] ath: EEPROM regdomain: 0x8242
[  466.073885] ath: EEPROM indicates we should expect a country code
[  466.073887] ath: doing EEPROM country->regdmn map search
[  466.073889] ath: country maps to regdmn code: 0x37
[  466.073890] ath: Country alpha2 being used: NO
[  466.073892] ath: Regpair used: 0x37
[  466.073894] ath: regdomain 0x8242 dynamically updated by country IE
[  466.073923] cfg80211: Regulatory domain changed to country: NO
[  466.073924] cfg80211:  DFS Master region: ETSI
[  466.073926] cfg80211:   (start_freq - end_freq @ bandwidth), (max_antenna_gain, max_eirp)
[  466.073929] cfg80211:   (2402000 KHz - 2482000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[  466.073931] cfg80211:   (5170000 KHz - 5250000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[  466.073933] cfg80211:   (5250000 KHz - 5330000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[  466.073936] cfg80211:   (5490000 KHz - 5710000 KHz @ 80000 KHz), (2700 mBi, 0 mBm)
[  466.073938] cfg80211:   (57240000 KHz - 65880000 KHz @ 2160000 KHz), (4000 mBi, 0 mBm)
[  532.403981] wlan0: authenticate with 7c:d1:c3:cc:02:ed
[  532.410386] wlan0: send auth to 7c:d1:c3:cc:02:ed (try 1/3)
[  532.411188] cfg80211: Calling CRDA to update world regulatory domain
[  532.411481] wlan0: authenticated
[  532.411523] cfg80211: World regulatory domain updated:
[  532.411525] cfg80211:  DFS Master region: unset
[  532.411528] cfg80211:   (start_freq - end_freq @ bandwidth), (max_antenna_gain, max_eirp)
[  532.411531] cfg80211:   (2402000 KHz - 2472000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[  532.411533] cfg80211:   (2457000 KHz - 2482000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[  532.411535] cfg80211:   (2474000 KHz - 2494000 KHz @ 20000 KHz), (2000 mBi, 0 mBm)
[  532.411537] cfg80211:   (5170000 KHz - 5250000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[  532.411539] cfg80211:   (5735000 KHz - 5835000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[  532.411542] cfg80211:   (57240000 KHz - 63720000 KHz @ 2160000 KHz), (N/A, 0 mBm)
[  532.416001] wlan0: associate with 7c:d1:c3:cc:02:ed (try 1/3)
[  532.417769] wlan0: RX AssocResp from 7c:d1:c3:cc:02:ed (capab=0x1511 status=0 aid=2)
[  532.417824] wlan0: associated
[  532.417876] cfg80211: Calling CRDA for country: NO
[  532.417904] ath: EEPROM regdomain: 0x8242
[  532.417905] ath: EEPROM indicates we should expect a country code
[  532.417907] ath: doing EEPROM country->regdmn map search
[  532.417909] ath: country maps to regdmn code: 0x37
[  532.417911] ath: Country alpha2 being used: NO
[  532.417913] ath: Regpair used: 0x37
[  532.417914] ath: regdomain 0x8242 dynamically updated by country IE
[  532.417943] cfg80211: Regulatory domain changed to country: NO
[  532.417945] cfg80211:  DFS Master region: ETSI
[  532.417947] cfg80211:   (start_freq - end_freq @ bandwidth), (max_antenna_gain, max_eirp)
[  532.417949] cfg80211:   (2402000 KHz - 2482000 KHz @ 40000 KHz), (2000 mBi, 0 mBm)
[  532.417952] cfg80211:   (5170000 KHz - 5250000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[  532.417954] cfg80211:   (5250000 KHz - 5330000 KHz @ 80000 KHz), (2000 mBi, 0 mBm)
[  532.417956] cfg80211:   (5490000 KHz - 5710000 KHz @ 80000 KHz), (2700 mBi, 0 mBm)
[  532.417961] cfg80211:   (57240000 KHz - 65880000 KHz @ 2160000 KHz), (4000 mBi, 0 mBm)
[  532.479069] wlan0: Limiting TX power to 30 (30 - 0) dBm as advertised by 7c:d1:c3:cc:02:ed
[ 8878.895449] INFO: task Xorg:383 blocked for more than 120 seconds.
[ 8878.895451]       Not tainted 3.14.4 #1
[ 8878.895452] "echo 0 > /proc/sys/kernel/hung_task_timeout_secs" disables this message.
[ 8878.895456] Xorg            D ffff880100311b40     0   383    375 0x00000000
[ 8878.895460]  ffff880060d860b0 0000000000000002 0000000000011b40 ffff880060d860b0
[ 8878.895462]  ffff8800614fdfd8 ffff88010053f000 ffff88007449e988 ffff880074478000
[ 8878.895463]  ffff8800744782b8 ffff880074512900 ffff8800744782f8 ffffffff8144e42d
[ 8878.895464] Call Trace:
[ 8878.895474]  [<ffffffff8144e42d>] ? intel_crtc_wait_for_pending_flips+0x8c/0xe7
[ 8878.895478]  [<ffffffff81058cc6>] ? finish_wait+0x5d/0x5d
[ 8878.895481]  [<ffffffff8145ae00>] ? intel_crtc_set_config+0x716/0x7ac
[ 8878.895487]  [<ffffffff81380e15>] ? drm_mode_set_config_internal+0x46/0xb1
[ 8878.895490]  [<ffffffff8137411f>] ? drm_fb_helper_set_par+0x5a/0x9a
[ 8878.895495]  [<ffffffff8130b7da>] ? fb_set_var+0x264/0x345
[ 8878.895498]  [<ffffffff81372af2>] ? drm_fb_helper_setcmap+0x55/0x336
[ 8878.895502]  [<ffffffff813141d9>] ? fbcon_blank+0x75/0x1cb
[ 8878.895506]  [<ffffffff81050934>] ? local_clock+0x5/0x1b
[ 8878.895510]  [<ffffffff8135f321>] ? do_unblank_screen+0xd7/0x143
[ 8878.895514]  [<ffffffff81357359>] ? complete_change_console+0x4c/0xb7
[ 8878.895517]  [<ffffffff81358257>] ? vt_ioctl+0xe93/0x1108
[ 8878.895521]  [<ffffffff81027f61>] ? __do_page_fault+0x280/0x2e8
[ 8878.895524]  [<ffffffff8135031c>] ? tty_ioctl+0x952/0x9b3
[ 8878.895528]  [<ffffffff81086ff8>] ? generic_file_aio_write+0x53/0xb2
[ 8878.895532]  [<ffffffff810e3e4e>] ? fsnotify+0x244/0x269
[ 8878.895535]  [<ffffffff810c727e>] ? do_vfs_ioctl+0x34b/0x3fd
[ 8878.895538]  [<ffffffff81050c1f>] ? account_user_time+0x1b/0x33
[ 8878.895541]  [<ffffffff81050f31>] ? vtime_account_user+0x34/0x3e
[ 8878.895543]  [<ffffffff810c7369>] ? SyS_ioctl+0x39/0x58
[ 8878.895547]  [<ffffffff81769699>] ? tracesys+0xd0/0xd5